# Enterprise Switches - Options

The Cisco Enterprise Switch family of devices is a set of switching hubs consisting of the Catalyst 1200, 1600, 2900, 4000, 5000, 5002, 5500, 6000, and CPW 2200 products.

This online help system describes all of the features in enterprise switches. Most of this information applies to all models. However, for some features, information categories available in the help system might not apply to your switch model. For example, if your switch does not support brouting, the brouting information in the main help system does not apply to your device. Context-sensitive help that you invoke from a particular device display applies only to that device.

Navigating a Catalyst 5000 Series Device Interface Using CiscoView

IP Addresses and CiscoView Catalyst 5500 Invocation Options

## Virtual Switch Support

In this device package release, certain Cisco Catalyst 6500 Series hardware provides support for Virtual Switch functionality, which allows you to manage two switches as if they are only one. For more information, click here.

## Catalyst QoS Device Manager (CatQDM)

CatQDM is a graphical user interface (GUI) application developed as an addlet using the CiscoView development environment. CatQDM, which is supported by Catalyst 6000 devices, provides a user interface for configuring and monitoring QoS features.

For more information, click here to access the CatQDM online help system.

Click on one of the following links for more information.

## Managing Catalyst 1200, 2900, 4000, 5000, 5500, 5509, 6000, and CPW 2200 Switches

Managing Device Configuration

Managing Card Configuration

Managing Port Configuration

Managing a Catalyst 5500 with an LS1010 PAM

Displaying Power Supply Information

Monitoring Device Performance

Monitoring Port Performance

## Managing Catalyst 1600 Series Switches

Managing 1600 Device Configuration

Managing 1600 Port Configuration

Monitoring 1600 Device Performance

Monitoring 1600 Port Performance