# Add/Edit IPX ACL

Configuration > Classification > IPX ACL > Add/Edit ACL

This dialog box displays a list of IPX Access Control Entries (ACEs). From here, you can launch dialog boxes to add, edit, or delete IPX ACEs.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- ACL Name (caqIpxAclName)

- Protocol Type (caqIpxAceProtocolType)

- Source Net (caqIpxAceSrcNet)

- Destination Net (caqIpxAceDestNet)

- Destination Node (caqIpxAceDestNode)

- Destination Net Mask (caqIpxAceDestNetMask)

- Destination Node Mask (caqIpxAceDestNodeMask)

The following list specifies buttons in this dialog box, as well as their function:

- Click Add ACE to open the Add/Edit Access Control Element dialog box and add a new IPX ACE.

- Click Edit ACE to open the Add/Edit Access Control Element dialog box and edit an existing IPX ACE.

- Click Delete ACE to remove an existing IPX ACE.

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

ACL Name (caqIpxAclName)

The name of an Access Control List (ACL). This name is unique throughout all of the ACL tables that refer to the list which the entry belongs to in the device.

Protocol Type (caqIpxAceProtocolType)

The protocol number field in the IPX header used to indicate the higher layer protocol. The value can range from 0 to 255.

Source Net (caqIpxAceSrcNet)

Indicates the source network from which the packet is being sent. This is a 32-bit value that uniquely identifies the IPX network cable segment in IPX protocol.

Destination Net (caqIpxAceDestNet)

Number of the destination network to which the packet is being sent. This is a 32-bit value that uniquely identifies the IPX network cable segment in IPX protocol. A network number of 0xFFFFFFFF matches all networks.

Destination Node (caqIpxAceDestNode)

Node on the destination network to which the packet is being sent. This is a 48-bit value.

Destination Net Mask (caqIpxAceDestNetMask)

Mask to be applied to the destination net. This is a 32-bit value that has the same format as the destination net.

Destination Node Mask (caqIpxAceDestNodeMask)

Mask to be applied to the destination node. This is a 48-bit value.

The following table outlines which policy types are supported by the IP, IPX, and MAC interfaces on Sup1 and Sup2 supervisor cards.

Table 1: Policy Types Supported

Policy Type | Sup1 Card | Sup2 Card
IP | IPX | MAC | IP | IPX | MAC
Micro Flow | Yes | No | No | Yes | No | No
Aggregate Flow | Yes | Yes | Yes | Yes | Yes | Yes
No Trust | Yes | Yes | Yes | Yes | No | No
Trust CoS | Yes | Yes | Yes | Yes | Yes | Yes
DSCP | Yes | No | No | Yes | No | No
IP Prec | Yes | No | No | Yes | No | No