# Home Agent Mobile Network Group Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Home Agent Mobile Network Group Configs.

The following information appears:

> MR Address Type (cmiHaMrAddrType)

> Inet Address (cmiHaMrAddr)

> MR Dynamic Registration (cmiHaMrDynamic)

> Create/Delete Row (cmiHaMrStatus)

### MR Address Type (cmiHaMrAddrType)

Type of IP address stored in cmiHaMrAddr. Only IPv4 address type is supported.

### Inet Address (cmiHaMrAddr)

IP address of a mobile router providing mobility to one or more networks. Only IPv4 addresses are supported.

### MR Dynamic Registration (cmiHaMrDynamic)

Specifies whether the mobile router is capable of registering networks dynamically or not.

### Create/Delete Row (cmiHaMrStatus)

The row status for the mobile router entry.