# Firewall Service Blade: Configure HTTP Service on Firewall Interface(s)

You can configure the HTTP service on firewall interface(s), using this fourth option of the firewall service blade setup wizard, or the Configure HTTP Service on Firewall Interface(s) option in the Firewall menu.

## Navigation

1. Right-click the blade, then select Firewall Service Blade Setup Wizard.

2. Click Next till the Configure HTTP Service on Firewall Interface(s) option, in the left pane, is selected.

The following information appears:

Interface Name

HTTP Interface IP Address

HTTP Interface Mask

In the Firewall Service Blade Setup Wizard:

To configure the HTTP server status, click Configure HTTP.

To remove HTTP service from the interface, select a row, then click Remove HTTP.

To go to the previous wizard option, click Back .

To go to the next wizard option, click Next .

### Interface Name

Name of the firewall interface.

### HTTP Interface IP Address

IP address assigned to the interface.

### HTTP Interface Mask

Subnet mask of the VLAN IP address.