# Add/Edit MAC ACE

Configuration > Classification > MAC ACL > Add/Edit ACL > Add/Edit ACE

In this dialog box, you can specify the settings for a particular MAC ACE.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Protocol Type (caqMacAceEthertype)

- Source Mac (caqMacAceSrcMac)

- Source Mac Mask (caqMacAceSrcMacMask)

- Destination Mac (caqMacAceDestMac)

- Destination Mac Mask (caqMacAceDestMacMask)

- Policy Selection to be Applied

The following list specifies buttons in this dialog box, as well as their function:

- Click Change to apply a different policy selection to the MAC ACE.

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

Protocol Type (caqMacAceEthertype)

A 16-bit hexadecimal number which indicates the matched Ethernet type. A value of "0x0000" means that any Ethernet type will be matched.

Source Mac (caqMacAceSrcMac)

Indicates the 48-bit source MAC address.

Source Mac Mask (caqMacAceSrcMacMask)

Indicates the 48-bit source MAC address mask.

Destination Mac (caqMacAceDestMac)

Indicates the 48-bit destination MAC address.

Destination Mac Mask (caqMacAceDestMacMask)

Indicates the 48-bit destination MAC address mask.

Policy Selection to be Applied

An entry in the caqQosActionSelectTable object.

The following table outlines which policy types are supported by the IP, IPX, and MAC interfaces on Sup1 and Sup2 supervisor cards.

Table 1: Policy Types Supported

Policy Type | Sup1 Card | Sup2 Card
IP | IPX | MAC | IP | IPX | MAC
Micro Flow | Yes | No | No | Yes | No | No
Aggregate Flow | Yes | Yes | Yes | Yes | Yes | Yes
No Trust | Yes | Yes | Yes | Yes | No | No
Trust CoS | Yes | Yes | Yes | Yes | Yes | Yes
DSCP | Yes | No | No | Yes | No | No
IP Prec | Yes | No | No | Yes | No | No