# Status

## Navigation

Right-click the device and then select Configure > Redundant Framework > Status.

The Status dialog box indicates the status of the Redundant Framework (RF) subsystem on the device.

The following information is displayed:

> Redundancy Status:

- Active Supervisor Slot Number (cRFStatusUnitId)

- Active Supervisor State (cRFStatusUnitState)

- Standby Supervisor Slot Number (cRFStatusPeerUnitId)

- Standby Supervisor State (cRFStatusPeerUnitState)

- Primary Mode (cRFStatusPrimaryMode)

- Duplex State (cRFStatusDuplexMode)

- Manual Swact Inhibit (cRFStatusManualSwactInhibit)

- Swact Reason Code (cRFStatusLastSwactReasonCode)

- Fail over Time (cRFStatusFailoverTime)

- StandBy Entry Time (cRFStatusPeerStandByEntryTime)

> Redundancy Mode Capabilities:

- Redundancy Mode (cRFStatusRFModeCapsMode)

- Redundancy Mode Description (cRFStatusRFModeCapsModeDescr)

### Redundancy Status:

### Active Supervisor Slot Number (cRFStatusUnitId)

A unique identifier for this redundant unit. This identifier is implementation-specific but the method for selecting the ID must remain consistent throughout the redundant system. Some example identifiers include: slot id, physical or logical entity id, or a unique ID assigned internally by the RF subsystem.

### Active Supervisor State (cRFStatusUnitState)

Current state of RF on this unit.

### Standby Supervisor Slot Number (cRFStatusPeerUnitId)

Unique identifier for the redundant peer unit. This identifier is implementation-specific but the method for selecting the ID must remain consistent throughout the redundant system. Some example identifiers include: slot id, physical or logical mentity id, or a unique ID assigned internally by the RF subsystem.

### Standby Supervisor State (cRFStatusPeerUnitState)

Current state of RF on the peer unit.

### Primary Mode (cRFStatusPrimaryMode)

When the value of this object is "true", it indicates that this unit is the primary unit. The primary unit is given a higher priority or precedence over the secondary unit. Only one redundant unit can be the primary unit at any given time.

Note that the terms primary/secondary are not synonymous with the terms active/standby. At any given time, the primary unit may be the active unit or the standby unit; likewise for the secondary unit.

### Duplex State (cRFStatusDuplexMode)

Indicates whether the redundant peer unit has been detected or not. True means that it has been detected.

### Manual Swact Inhibit (cRFStatusManualSwactInhibit)

Indicates whether a manual switch of activity is permitted. False means that manual switch of activity is allowed. The valuet is the inverse of the status of manual SWACTs. A switch of activity happens when the standby redundant unit becomes active and the previously active unit is in standby mode.

### Swact Reason Code (cRFStatusLastSwactReasonCode)

Reason for the last switch of activity.

### Fail over Time (cRFStatusFailoverTime)

Value of sysUpTime when the primary redundant unit took over as the active unit. The value of this object is zero until the first switchover.

### StandBy Entry Time (cRFStatusPeerStandByEntryTime)

Value of sysUpTime when the peer redundant unit entered the standbyHot state. The value of this object is zero after system initialization.

### Redundancy Mode Capabilities:

### Redundancy Mode (cRFStatusRFModeCapsMode)

The redundancy mode that can be supported on the device

### Redundancy Mode Description (cRFStatusRFModeCapsModeDescr)

The description of the device implementation specific terminology associated with its supported redundancy mode.