# GGSN Access Point Traffic Statistics

## Procedure

1. Right-click the device and then select Monitor.

2. Select GGSN Access Point Statistics from the Category list.

3. Select a row and click on Monitor.

4. Select category GGSN Access Point Traffic Statistics.

The following information appears:

> Upstream Bytes (cgprsAccPtRevUpstreamTrafficVol)

> Downstream Bytes (cgprsAccPtRevDownstrTrafficVol)

> Upstream Packets (cgprsAccPtUpstreamPacketCount)

> Downstream Packets (cgprsAccPtDownstreamPacketCount)

> DHCP Address Requests (cgprsAccPtDhcpAddrRequests)

> Succesful DHCP Address Requests (cgprsAccPtSuccDhcpAddrRequests)

> DHCP Address Release Requests (cgprsAccPtDhcpAddrReleases)

### Upstream Bytes (cgprsAccPtRevUpstreamTrafficVol)

This object indicates the total payload volume in upstream traffic. Data flow from MS to PDN is considered to be upstream traffic.

### Downstream Bytes (cgprsAccPtRevDownstrTrafficVol)

This object indicates the total payload volume in downstream traffic. Data flow from PDN to MS is considered as downstream traffic.

### Upstream Packets (cgprsAccPtUpstreamPacketCount)

This object represents the total number of upstream packets sent on this APN. Data flow from MS to PDN is considered to be upstream traffic. This counter is triggered when upstream traffic is being routed to PDN.

### Downstream Packets (cgprsAccPtDownstreamPacketCount)

This object represents the total number of downstream packets sent on this APN. Data flow from PDN to MS is considered to be downstream traffic. This counter is triggered when downstream traffic is being routed to PDN.

### DHCP Address Requests (cgprsAccPtDhcpAddrRequests)

This object represents the total number of DHCP address request sent by the GGSN on this APN. Trigger Condition: This counter is triggered by create pdp request message.

### Succesful DHCP Address Requests (cgprsAccPtSuccDhcpAddrRequests)

This object represents the total number of successful DHCP address request sent by the GGSN on this APN. This counter is triggered by create pdp request message.

### DHCP Address Release Requests (cgprsAccPtDhcpAddrReleases)

This object represents the total number of DHCP address release request sent by the GGSN on this APN.

This counter is triggered by delete pdp request message.