# RP Registration Accepted Statistics

This dialog box displays Packet Control Function (PCF) and Service Option (SO)-based Radio Packet (RP) Registration Accepted Statistics.

## Navigation

1. Right-click the device, and select Monitor.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category list.

3. Select a row and click the RP Registration Statistics button.

The following information appears:

> Registration Requests Received (cCdmaPcfSoRpRegRcvdReqs)

> Registration Requests Accepted (cCdmaPcfSoRpRegAcptdReqs)

> New Connection Requests Accepted (cCdmaPcfSoRpInitRegAcptdReqs)

> Re-registration Requests Accepted (cCdmaPcfSoRpReRegAcptdReqs)

> De-registration Requests Accepted (cCdmaPcfSoRpDeRegAcptdReqs)

> Accepted Handoff A11 Registrations (cCdmaPcfSoRpHandoffRegAcptdReqs)

### Registration Requests Received (cCdmaPcfSoRpRegRcvdReqs)

The number of A11 registration requests received since system startup.

### Registration Requests Accepted (cCdmaPcfSoRpRegAcptdReqs)

The number of A11 registration requests accepted since system startup.

### New Connection Requests Accepted (cCdmaPcfSoRpInitRegAcptdReqs)

Since system startup, the number of accepted A11 registration requests meant for establishing new R-P connections.

### Re-registration Requests Accepted (cCdmaPcfSoRpReRegAcptdReqs)

The number of accepted A11 registration requests meant for refreshing the established R-P connections since system startup.

### De-registration Requests Accepted (cCdmaPcfSoRpDeRegAcptdReqs)

The number of accepted A11 registration requests meant for de-establishing the established R-P connections since system startup.

### Accepted Handoff A11 Registrations (cCdmaPcfSoRpHandoffRegAcptdReqs)

The total number of accepted handoff A11 registration requests meant for already existing session, since system startup.