# GGSN Traffic Class BW Allocation Table

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN CAC Virtual BW Pool from the Category drop-down box.

3. With an entry selected in the GGSN CAC Virtual BW Pool dialog box, click Traffic Class Details.

The following information appears:

> Traffic Class (cggsnQosBWPoolTrafClass)

> % of BW Allocated (cggsnQosBWPoolTrafClassPerVal)

> Absolute Value of BW Allocated (cggsnQosBWPoolTrafClassAbsVal)

> Available Unused BW (cggsnQosBWPoolTrafClassAvailBw)

### Traffic Class (cggsnQosBWPoolTrafClass)

Indicates the traffic class for which bandwidth allocation is needed. There are four possible values:

> conversational

> streaming

> interactive

> background

### % of BW Allocated (cggsnQosBWPoolTrafClassPerVal)

Percentage of bandwidth allocated to the traffic class set in cggsnQosBWPoolTrafClass. This object is valid and can be set only when cggsnQosBWPoolTrafClassPercent is set to true.

### Absolute Value of BW Allocated (cggsnQosBWPoolTrafClassAbsVal)

Indicates the absolute value of bandwidth allocated to the traffic class set in cggsnQosBWPoolTrafClass. This object is valid and can be set only when cggsnQosBWPoolTrafClassPercent is set to false.

### Available Unused BW (cggsnQosBWPoolTrafClassAvailBw)

Indicates the absolute available bandwidth left unused for the traffic class set in cggsnQosBWPoolTrafClass.