PIB Attribute

# PIB Attribute

Device>Configure>PIB>Attribute

This table provides specific attributes of the device. These include configuration values such as the configured PDP addresses, the maximum message size, and specific device capabilities. The latter include input port-based and output port-based classification and or policing, support for flow based policing, aggregate based policing, traffic shaping capabilities, and more.

QoS Domain (qosDevicePepDomain)

This table field provides the QoS domain that this device belongs to. This is configured locally on the device (perhaps by some protocol such as SNMP). By default, it is the zero-length string.

Primary PDP (qosDevicePrimaryPdp)

This table field provides the address of the PDP configured to be the primary PDP for the device.

Secondary PDP (qosDeviceSecondaryPdp)

This table field provides the address of the PDP configured to be the secondary PDP for the device. An address of zero indicates no secondary is configured.

Max. Message Size (bytes) (qosDeviceMaxMessageSize)

This table field provides the maximum size message that this PEP is capable of receiving in bytes. A value of zero means that the maximum message size is unspecified (but does not mean it is unlimited). A message greater than this maximum results in a 'Message Too Big' error on a 'no commit' REP.

Capabilities (qosDeviceCapabilities)

This table field provides an enumeration of device capabilities. Used by the PDP to select policies and configuration to push to the PEP.