# RP Registration Request Errors of Invalid Reasons

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select RP Registration Request Errors of Invalid Reasons from the Category list.

The following information appears:

> Invalid Packet Length (cCdmaRegReqInvPakLenErrs)

> Invalid Protocol Value (cCdmaRegReqInvProtocolErrs)

> Invalid Flags Value (cCdmaRegReqInvFlagsErrs)

> Invalid Authentication Key (cCdmaRegReqInvMHAEKeyErrs)

> Invalid SPI (cCdmaRegReqInvSPIErrs)

> Invalid Connection ID (cCdmaRegReqInvConnectionIDErrs)

> Invalid MN ID (cCdmaRegReqInvMNIDErrs)

> Invalid MN ID Type (cCdmaRegReqInvMNIDTypeErrs)

### Invalid Packet Length (cCdmaRegReqInvPakLenErrs)

The number of invalid registration requests due to packet length while parsing since the system was last restarted.

### Invalid Protocol Value (cCdmaRegReqInvProtocolErrs)

The number of invalid protocol value in the Registration Request Session Specific Extension since the system was last restarted.

### Invalid Flags Value (cCdmaRegReqInvFlagsErrs)

The number of invalid flags value in the Registration Request since the system was last restarted.

### Invalid Authentication Key (cCdmaRegReqInvMHAEKeyErrs)

The number of invalid authentication key in the Registration Request Mobile-Home Authentication Extension since the system was last restarted.

### Invalid SPI (cCdmaRegReqInvSPIErrs)

The number of invalid SPI in the Registration Request Mobile-Home Authentication Extension since the system was last restarted.

### Invalid Connection ID (cCdmaRegReqInvConnectionIDErrs)

The number of invalid connection ID in the Registration Request since the system was last restarted.

### Invalid MN ID (cCdmaRegReqInvMNIDErrs)

The number of invalid mobile node ID in the Registration Request since the system was last restarted.

### Invalid MN ID Type (cCdmaRegReqInvMNIDTypeErrs)

The number of invalid MN ID type in the Registration Request since the system was last restarted.