# Monitoring DS1 Current Statistics

The CiscoView Monitor Port window displays the following current statistical information for a DS1 port:

Erred Secs (dsx1CurrentESs)

Severe Erred Secs (dsx1CurrentSESs)

Severe Erred Framing Secs (dsx1CurrentSEFSs)

Unavail Erred Secs (dsx1CurrentUASs)

Ctroled Slip Secs (dsx1CurrentCSSs)

Path Coding Violates (dsx1CurrentPCVs)

Line Erred Secs (dsx1CurrentLESs)

Bursty Erred Secs (dsx1CurrentBESs)

Degraded Mins (dsx1CurrentDMs)

Line Code Violates (dsx1CurrentLCVs)

# Erred Secs (dsx1CurrentESs)

Shows the number of seconds during which errors were recorded for a DS1 interface during the current 15-minute interval.

# Severe Erred Secs (dsx1CurrentSESs)

Shows the number of seconds during which severe errors were recorded for a DS1 interface during the current 15-minute interval.

# Severe Erred Framing Secs (dsx1CurrentSEFSs)

Shows the number of seconds during which severe framing errors were recorded for a DS1 interface during the current 15-minute interval.

# Unavail Erred Secs (dsx1CurrentUASs)

Shows the number of seconds during which for the specified DS1 interface was unavailable during the current 15-minute interval.

# Ctroled Slip Secs (dsx1CurrentCSSs)

Shows the number of seconds during which controlled slips were recorded for a DS1 interface during the current 15-minute interval.

# Path Coding Violates (dsx1CurrentPCVs)

Shows the number of path coding violations recorded for a DS1 interface during the current 15-minute interval.

# Line Erred Secs (dsx1CurrentLESs)

Shows the number of seconds during which line errors were recorded for a DS1 interface during the current 15-minute interval.

# Bursty Erred Secs (dsx1CurrentBESs)

Shows the number of seconds during which bursty errors were recorded for a DS1 interface during the current 15-minute interval.

# Degraded Mins (dsx1CurrentDMs)

Shows the number of degraded minutes recorded for a DS1 interface during the current 15-minute interval.

# Line Code Violates (dsx1CurrentLCVs)

Shows the number of line code violations recorded for a DS1 interface during the current 15-minute interval.