# CDMA PDSN Registration Failures

This dialog box is applicable to Controller, Member, and Peer to Peer clusters. From here, you can view rejected registration statistics.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Registration Failures.

The following data is displayed:

> Registration Request Failed Unspecified (cCdmaRPRegReasonUnSpecFailures)

> Registration Request Failed Administrative (cCdmaRPRegAdminProhibFailures)

> Registration Request Failed Insuff Resource (cCdmaRPRegInsuffResFailures)

> Registration Request Failed MN Authentication (cCdmaRPRegMNAuthenFailures)

> Registration Request Failed Identity Mismatch (cCdmaRPRegIdentMismatchFailures)

> Registration Request Failed Poor Request (cCdmaRPRegBadRequestFailures)

### Registration Request Failed Unspecified (cCdmaRPRegReasonUnSpecFailures)

Number of registration requests that failed because the packet control function (PCF) address was not found in the configured PCF packet data serving node (PDSN) list, for an unspecified reason, since system startup.

### Registration Request Failed Administrative (cCdmaRPRegAdminProhibFailures)

Number of registration requests that failed because the PCF address was not found in the configured PCF PDSN list, due to administrative prohibition, since system startup.

### Registration Request Failed Insuff Resource (cCdmaRPRegInsuffResFailures)

Number of registration requests that failed because the PCF number or session number has reached the maximum value since system startup.

### Registration Request Failed MN Authentication (cCdmaRPRegMNAuthenFailures)

Number of registration requests that failed due to a mobile node (MN) authentication failure since system startup.

### Registration Request Failed Identity Mismatch (cCdmaRPRegIdentMismatchFailures)

Number of registration requests that failed due to a registration identity mismatch since system startup.

### Registration Request Failed Poor Request (cCdmaRPRegBadRequestFailures)

Number of registration requests that failed due to a poorly formed request since system startup.