# Configure Outside Access Port

The Configure Outside Access Port option of the VPN Service Blade Access Port Mode Setup Wizard dialog box enables you to use the name and ID of the outside VLAN interface to configure the VLAN configuration port in the access mode.

## Procedure

1. Right-click on the IPSec VPN Service Blade, then select VPN Service Blade Setup Wizard.

2. Click Create. The IPSec VLAN Configuration dialog box appears.

3. Select the radio button Access Port Mode, then click Configure.... The VPN Service Blade Access Port Mode Setup Wizard dialog box appears.

4. Select a VLAN from the table or create a new VLAN.

5. Click Next.

The following information appears:

Access Port

Outside VLAN ID

Click Next to view the commands to be sent to the device.

### Access Port

Name of the access port.

### Outside VLAN ID

Identifier of the outside VLAN interface.