# CDMA PDSN System Information

Use this option to view PDSN system information.

## Procedure

To access CDMA PDSN system information:

1. Right-click the device and select Configure from the popup menu.

> > The Configure Device dialog box appears.

2. Select CDMA PDSN System Information from the Category list.

The following information appears:

Max Number of Sessions (cCdmaSessionMaxAllowed)

Max Number of PCF (cCdmaPcfMaxAllowed)

Host Name (cCdmaServingPdsnHostname)

PDSN System Version (cCdmaSystemVersion)

PDSN Authentication Timer (cCdmaSessionPdsnAuthenTimer)

Max Session Notification Enable (cCdmaSessionMaxNotifEnabled)

Max PCF Notification Enable (cCdmaPcfMaxAllowedNotifEnabled)

Invalid Registration Notification Enable (cCdmaRegReqFailedNotifEnabled)

PDSN Status (cCdmaSystemStatus)

High Threshold Allowed (cCdmaSessionHighThreshold)

Low Threshold Allowed (cCdmaSessionLowThreshold)

Session Redundancy Enabled (cCdmaSrEnabled)

### Max Number of Sessions (cCdmaSessionMaxAllowed)

Maximum number of sessions allowed by system. Max number of sessions is applicable to member and peer-peer.

Displays zero if no limitation on the number of PDSN sessions.

### Max Number of PCF (cCdmaPcfMaxAllowed)

Maximum number of packet control functions (PCF) allowed by system. Max number of PCF is applicable to member and peer-peer.

Displays zero if no limitation on the number of PCF sessions.

### Host Name (cCdmaServingPdsnHostname)

Host name of serving Packet Data Serving Node (PDSN). The host name is applicable to controller, member and peer-peer.

### PDSN System Version (cCdmaSystemVersion)

CISCO packet data switching node release version, example output: 1.1. The system version is applicable to controller, member and peer-peer.

### PDSN Authentication Timer (cCdmaSessionPdsnAuthenTimer)

Timer for Mobile IP (MoIP) users not using PPP authentication. Authentication timer is applicable to member and peer-peer.

### Max Session Notification Enable (cCdmaSessionMaxNotifEnabled)

Indicates whether to send notification when maximum number of sessions is reached. Enable max sessions notification is applicable to member and peer-peer.

Values are:

true | Send failure notification.
false | Do not send failure notification.

Default is false.

### Max PCF Notification Enable (cCdmaPcfMaxAllowedNotifEnabled)

Indicates whether to send notification when maximum number of interconnected packet control function (PCF) is reached. Max PCF notification is applicable to member and peer-peer.

Values are:

true | Send failure notification.
false | Do not send failure notification.

Default is false.

### Invalid Registration Notification Enable (cCdmaRegReqFailedNotifEnabled)

When true, a failure notification is sent out to the manager when a session terminates because of a registration request failure. Default is false. Enabling the notification is applicable to controller, member and peer-peer.

### PDSN Status (cCdmaSystemStatus)

Operational status of the PDSN subsystem. The PDSN status is applicable to controller, member and peer-peer.

### High Threshold Allowed (cCdmaSessionHighThreshold)

Maximum number of allowed sessions. The agent generates a notification when this threshold is reached during call setup. High threshold allowed is applicable for member and peer-peer.

### Low Threshold Allowed (cCdmaSessionLowThreshold)

Minimum number of allowed sessions. The agent generates a notification when this threshold is reached during call release. Low threshold allowed is applicable for member and peer-peer.

### Session Redundancy Enabled (cCdmaSrEnabled)

Indicates whether the session redundancy feature is enabled.