# Physical

Network Analysis Module > Configure > Physical

The following information is displayed in the Physical dialog box:

Name of the Module (moduleName)

Name assigned to the module or card by the network administrator, such as “London.”

Module Model (moduleModel)

Manufacturer’s model number for the card or module.

Serial Number (moduleSerialNumber)

Serial number of the card or module (for example, 900000023).

Hardware Version (moduleHwVersion)

Version number of the card being managed (for example, 3.1).

Firmware Version (moduleFwVersion)

Firmware version of the card being managed (for example, 2.0).

Software Version (moduleSwVersion)

Software version of the card being managed (for example, 3.2).

Status (moduleStatus)

Current status of the module or card. Possible values are ok, minorFault, majorFault, or other. If the status is not ok, the value of the Diagnostic Errors field gives more information about the cause of the problem.

IP Address (moduleIPAddress)

IP address of the module or card.

Note: This field is only displayed on NAM and IDS modules.

Feature Card (moduleSubType)

Type of daughterboard attached to this module, if any.

Note: This MIB is supported by the following modules: WS-X5505, WS-X5506, WS-X5509, WS-X5302, WS-X5530, WS-X5540, WS-X6K-SUP-2GE (Catalyst 6000 only), and WS-X6348-RJ45.

Sub modules supported by WS-X5505, WS-X5506 and WS-X5509:

- wsf5510(3), -- EARL 1

- wsf5511(4), -- EARL 1+

Sub modules supported by WS-X5302:

- wsx5304(6), -- VIP II carrier

Sub modules supported by WS-X5530 and WS-X5540:

- wsf5520(7), -- EARL 1+

- wsf5521(8), -- NFFC

- wsf5531(9), -- NFFC II

Sub modules supported by WS-X6K-SUP-2GE and WS-X6K-S2U-MSFC2 (Catalyst 6000 only):

- wsf6020(100), -- L2 switching card

- wsf6020a(101),-- L2 switching card II

- wsf6kpfc(102), -- L3 switching engine

- wsf6kpfc2(103), -- L3 switching engine II

Sub modules supported by WS-X6348-RJ45:

- wsf6kvpwr(104) -- inline power card

Uplink Card (moduleSubType2)

Type of additional daughterboard attached to this module, if any.

Note: This MIB is supported by the Supervisor III module only.

Diagnostic Errors (moduleTestResult)

Result of the module’s self-test. None indicates that the module passed all tests.

Intake Temperature (entSensorValue)

Temperature recorded by the device's intake sensor.

Exhaust Temperature (entSensorValue)

Temperature recorded by the device's exhaust sensor.

Device1 Temperature (entSensorValue)

Temperature recorded by the device1 sensor.

Device2 Temperature (entSensorValue)

Temperature recorded by the device2 sensor.

Click OK to continue. Click Apply to save the changes in the dialog box. Click Cancel to close the dialog box. Click Refresh to update the contents of the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.