# Receive Side Low Priority Traffic

Use this option to monitor statistics of low priority traffic reception from higher layer for current interval for a particular side of a particular SRP interface.

## Procedure

To access low priority traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Current Interval Statistics of Higher Layer dialog box appears.

2. Select Rx Higher Layer Statistics from the Category menu to display Receive Higher Layer Statistics dialog box.

3. Select Low Priority Traffic from the Category menu to display low priority traffic information.

Low Priority Traffic dialog box displays:

Unicast Low Priority Packets (srpHostCurUcastLowPriPktsIn)

Unicast Low Priority Octets (srpHostCurUcastLowPriOctetsIn)

Multicast Low Priority Packets (srpHostCurMcastLowPriPktsIn)

Multicast Low Priority Octets (srpHostCurMcastLowPriOctetsIn)

### Unicast Low Priority Packets (srpHostCurUcastLowPriPktsIn)

Number of unicast packets received from the higher layer during a 15-minute interval.

### Unicast Low Priority Octets (srpHostCurUcastLowPriOctetsIn)

Number of unicast octets received from the higher layer during a 15-minute interval.

### Multicast Low Priority Packets (srpHostCurMcastLowPriPktsIn)

Number of multicast packets received from the higher layer during a 15-minute interval.

### Multicast Low Priority Octets (srpHostCurMcastLowPriOctetsIn)

Number of multicast octets received from the higher layer during a 15-minute interval.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components