# Foreign Agent Visitors Table

The table displays the following information:

Visitor IP Address (faVisitorIPAddress)

Visitor Home Address (faVisitorHomeAddress )

Visitor HA Address (faVisitorHomeAgentAddress)

Total LifeTime of Registration (faVisitorTimeGranted)

Remaining LifeTime of Registration (faVisitorTimeRemaining)

Registration Flags (faVisitorRegFlags)

4 LSBs of Registration ID(faVisitorRegIDLow)

4 MSBs of Registration ID (faVisitorRegIDHigh)

Registration Accepted (faVisitorRegIsAccepted)

### Visitor IP Address (faVisitorIPAddress)

Source IP address of Visitor's registration request.

### Visitor Home Address (faVisitorHomeAddress )

Home IP address of the visiting mobile node.

### Visitor HA Address (faVisitorHomeAgentAddress)

Home agent IP address of the visiting mobile node.

### Total LifeTime of Registration (faVisitorTimeGranted)

The lifetime, in seconds, granted to the mobile node for the registration.

Note: Valid only if faVisitorRegIsAccepted is true (1).

### Remaining LifeTime of Registration (faVisitorTimeRemaining)

Seconds remaining until the registration is expired.

Initial value is same as faVisitorTimeGranted, and is counted down by the foreign agent.

### Registration Flags (faVisitorRegFlags)

Registration flags send by the mobile nodes.

### 4 LSBs of Registration ID(faVisitorRegIDLow)

Low 32 bits of Identification used in the registration by the mobile node.

### 4 MSBs of Registration ID (faVisitorRegIDHigh)

High 32 bits of Identification used in the registration by the mobile node.

### Registration Accepted (faVisitorRegIsAccepted)

Indicates whether the registration is accepted.

Possible values are:

true (1) registration accepted.

false (2) registration is still pending for reply.