# Foreign Agent Asymmetric Link Support Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Foreign Agent Asymmetric Link Support Configs.

The following information appears:

> Care-of-address (faSupportedCOA)

> FA Advertise (cmiFaCoaInterfaceOnly)

> FA Transmit Only Status (cmiFaCoaTransmitOnly)

## Care-of-address (faSupportedCOA)

Foreign agent care-of-address.

### FA Advertise (cmiFaCoaInterfaceOnly)

Specifies whether the foreign agent interface associated with this care-of-address (CoA) should advertise this CoA only or not. If true, other configured care-of-addresses will not be advertised.

### FA Transmit Only Status (cmiFaCoaTransmitOnly)

Specifies whether the foreign agent interface associated with this CoA is a transmit-only (uplink) interface or not. If true, the foreign agent treats all registration requests received (on any interface) for this CoA as having arrived on the care-of interface. This object can be set to true for serial care-of-interfaces only.