# Foreign Agent Visitors List

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Configure button.
4. Select category Foreign Agent Visitors List.

The following information appears:

> Visitor Identifier Type (CmiEntityIdentifierType)

> Visitor Identifier Associated (cmiFaRegVisitorIdentifier)

> Home IP Address (cmiFaRegVisitorHomeAddress)

> Home Agent IP Address (cmiFaRegVisitorHomeAgentAddress)

> Lifetime (cmiFaRegVisitorTimeGranted)

> Time to Expire (cmiFaRegVisitorTimeRemaining)

> ID Low Bits (cmiFaRegVisitorRegIDLow)

> ID High Bits (cmiFaRegVisitorRegIDHigh)

> Registration Acceptance (cmiFaRegVisitorRegIsAccepted)

> Challenge Value (cmiFaRegVisitorChallengeValue)

> Visitor Registration Flags (CmiFaRegVisitorRegFlagsRev1)

### Visitor Identifier Type (CmiEntityIdentifierType)

A value that represents a type of mobile IP entity identifier:

other(1) | Identifier that is not in one of the formats defined in this list.
ipaddress(2) | IP address as defined by InetAddressIPv4 textual convention in INET-ADDRESS-MIB.
nai(3) | A network access identifier as defined by the CmiEntityIdentifier textual convention.

### Visitor Identifier associated (cmiFaRegVisitorIdentifier)

The identifier associated with the visitor.

### Home IP Address (cmiFaRegVisitorHomeAddress)

Home (IP) address of visiting mobile node.

### Home Agent IP Address (cmiFaRegVisitorHomeAgentAddress)

Home agent IP address for that visiting mobile node.

### Lifetime (cmiFaRegVisitorTimeGranted)

The lifetime granted to the mobile node for this registration. Only valid if faVisitorRegIsAccepted is true (1).

### Time to Expire (cmiFaRegVisitorTimeRemaining)

The time remaining until the registration expireS. It has the same initial value as cmiFaRegVisitorTimeGranted and is counted down by the foreign agent.

### ID Low Bits (cmiFaRegVisitorRegIDLow)

Low 32 bits of identification used in that registration by the mobile node.

### ID High Bits (cmiFaRegVisitorRegIDHigh)

High 32 bits of identification used in that registration by the mobile node.

### Registration Acceptance (cmiFaRegVisitorRegIsAccepted)

Whether the registration has been accepted or not. If it is false(2), this registration is still pending for reply.

### Challenge Value (cmiFaRegVisitorChallengeValue)

Challenge value forwarded to the mobile node in the previous registration reply, which can be used by the mobile node in the next Registration request.

### Visitor Registration Flags (CmiFaRegVisitorRegFlagsRev1)

Registration flags sent by the mobile node.