# Information of Mobile Networks Associated with Home Agent

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Information of Mobile Networks Associated with HA from the Category list.

The following information appears:

> Mobile Network Address Type (cmiHaMobNetAddressType)

> Mobile Network IP Address (cmiHaMobNetAddress)

> Mobile Network Prefix Length (cmiHaMobNetPfxLen)

> Dynamic Registration Status (cmiHaMobNetDynamic)

> Create/Delete Row (cmiHaMobNetStatus)

### Mobile Network Address Type (cmiHaMobNetAddressType)

The type of IP address stored in cmiHaMobNetAddress. Only IPv4 address type is supported.

### Mobile Network IP Address (cmiHaMobNetAddress)

The IP address of the mobile network. Only IPv4 addresses are supported.

### Mobile Network Prefix Length (cmiHaMobNetPfxLen)

The prefix length associated with the mobile network IP address.

### Dynamic Registration Status (cmiHaMobNetDynamic)

Indicates whether the mobile network has been registered dynamically or not.

### Create/Delete Row (cmiHaMobNetStatus)

The row status for the mobile network entry.