# IMA Group Configuration Table

The table displays the following information:

> Group Index (imaGroupIndex)

> Row Status (imaGroupRowStatus)

> Interface Index (imaGroupIfIndex)

> Tx Links (imaGroupMinNumTxLinks)

> Rx Links (imaGroupMinNumRxLinks)

> Near-End ImaID (imaGroupTxImaId)

> Far-End ImaID (imaGroupRxImaId)

> Symmetry (imaGroupSymmetry)

> TxFrameLength (imaGroupTxFrameLength)

> Rx Frame Length (imaGroupRxFrameLength)

> Near-End Transmission Clocking mode (imaGroupNeTxclkmode)

> Far-End Transmission Clocking mode (imaGroupFeTxclkmode)

> Last Change (imaGroupLastChange)

> Alpha Value (imaGroupAlphaValue)

> Beta Value (imagGroupBetaValue)

> Gamma Value (imaGroupGammaValue)

### GroupIndex (imaGroupIndex )

Indicates the unique value of the IMA group.

### Row Status (imaGroupRowStatus)

Indicates the status of the imaGroupTable entries. Row Status allows create, change, and delete operations on imaGroupTable entries.

### Interface Index (imaGroupIfIndex)

Indicates the logical interface number assigned to an IMA group. Interface Index is used to identify corresponding rows in the interface MIB.

Note: Re-initialization of the management agent may cause a client's imaGroupIfIndex to change.

### Tx Links (imaGroupMinNumTxLinks)

Indicates the minimum number of transmit links required to be active for the IMA group to be operational.

### Rx Links (imaGroupMinNumRxLinks)

Indicates the minimum number of receive links required to be active for the IMA group to be operational.

### Near-End ImaID (imaGroupTxImaId)

Indicates the IMA ID in use by the near-end IMA function.

### Far-End ImaID (imaGroupRxImaId)

Indicates the IMA ID in use by the far-end IMA function.

### Symmetry (imaGroupSymmetry)

Indicates the symmetry of the IMA group.

### Tx FrameLength (imaGroupTxFrameLength)

Indicates the length of the frame to be used by the IMA group in the transmit direction.

Note: The value can be set only when the IMA group is startup.

### Rx FrameLength (imaGroupRxFrameLength)

Indicates the length of the IMA frame received from the IMA function.

### Near-End Transmission Clocking mode (imaGroupNeTxClkmode)

Indicates the transmit clock mode used by the near-end IMA group.

### Far-End Transmission Clocking mode (imaGroupFeTxClkMode)

Indicates the transmit clock mode used by the far-end IMA group.

### Last Change (imaGroupLastChange)

Indicates the time-of-day the IMA group last changed the operational state.

### AlphaValue (imaGroupAlphaValue)

Indicates the alpha value that specifies the number of consecutive invalid ICP cells to be detected before moving to the IMA HUNT state from the IMA SYNC state.

### BetaValue (imaGroupBetaValue)

Indicates the beta value that specifies the number of consecutive erred ICP cells to be detected before moving to the IMA HUNT state from the IMA SYNC state.

### GammaValue (imaGroupGammaValue)

Indicates the gamma value that specifies the number of consecutive valid ICP cells to be