# Copy Config File (Catalyst 5000 SupIIG and SupIIIG)

Device>Configure>File Copy>Copy Config File

Use the CiscoView Copy Config File window to copy to and from a remote host to Flash or runtime memory. Use these settings:

Protocol (fileCopyProtocol)

TFTP or rcp for any remote copy.

From (fileCopyAction)

Set this option to:

- Flash to Runtime Copy the configuration file to the runtime configuration locally.

- Runtime to Flash Copy the runtime configuration to a configuration file on the Flash memory locally.

- Host to Flash Copy the configuration file from host to the runtime configuration over the network through TFTP/rcp.

- Flash to Host Copy the configuration file on the Flash memory to host over the network through TFTP/rcp.

Remote Host (fileCopyRemoteServer)

IP address or hostname of TFTP/rcp remote server from or to which to copy file. The accepted value of this object is 'cfg1' or 'cfg2' when the requested action is Flash to Runtime or Flash to Host.

Source File Name (fileCopySrcFileName)

Source filename (including the path, if applicable) of file. The accepted value of this object is 'cfg1' or 'cfg2' when the requested action is Runtime to Flash or Host to Flash .

Destination File Name (fileCopyDstFileName)

Destination filename (including path, if applicable) of file.

rcp User Name (fileCopyUserName)

Remote user name for copy via rcp protocol.