# CDMA PDSN System Statistics

From this dialog box, you can view Packet Data Serving Node (PDSN) system statistics.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN System Statistics.

The following information is displayed:

> Currents Sessions Ratio [Current Number of Sessions(cCdmaSessionTotal) Vs Max Number of Sessions (cCdmaSessionMaxAllowed)]

> Current PCF Ratio [Current Number of PCF(cCdmaPcfTotal) Vs Max Number of PCF (cCdmaPcfMaxAllowed)]

> Simple IP Flows (cCdmaSimpleIpFlowTotal)

> Mobile IP Flows (cCdmaMobileIpFlowTotal)

> Proxy MoIP Flows (cCdmaProxyMobileIpFlowTotal)

> Session Failures Count (cCdmaSessionFailTotal)

> The following objects are available only in PDSN 2.0:

> Active Sessions (cCdmaActiveSessions)

> Dormant Sessions (cCdmaDormantSessions)

### Currents Sessions Ratio [Current Number of Sessions(cCdmaSessionTotal) Vs Max Number of Sessions (cCdmaSessionMaxAllowed)]

Ratio of number of current sessions to the maximum number of sessions:

> Current Number of Sessions (cCdmaSessionTotal): total number of sessions established with the system.

> Max Number of Sessions (cCdmaSessionMaxAllowed): maximum number of sessions allowed by the system.

### Current PCF Ratio [Current Number of PCF(cCdmaPcfTotal) Vs Max Number of PCF (cCdmaPcfMaxAllowed)]

Ratio of current packet control functions (PCF) to the maximum number of PCF:

> Current Number of PCF (cCdmaPcfTotal): total number of PCF interacting with the system.

> Max Number of PCF (cCdmaPcfMaxAllowed): maximum number of PCF allowed by the system.

### Simple IP Flows (cCdmaSimpleIpFlowTotal)

Number of flows using simple IP service.

### Mobile IP Flows (cCdmaMobileIpFlowTotal)

Number of flows using Mobile IP service.

### Proxy MoIP Flows (cCdmaProxyMobileIpFlowTotal)

Number of flows using proxy Mobile IP service.

### Session Failures Count (cCdmaSessionFailTotal)

Number of A10/A11 session failures that have occurred since the PDSN agent restarted.

Note: sysUpTime can be polled to determine if the agent was restarted.

### Active Sessions (cCdmaActiveSessions)

Number of sessions in the active state.

### Dormant Sessions (cCdmaDormantSessions)

Number of sessions in the dormant state.