# MR Statistics

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select MR Statistics from the Category list.

The following information appears:

> New HA Registration (cmiMrRegNewHa)

> Better Interface Detected (cmiMrBetterIfDetected)

> Packets on MR-HA Tunnel (cmiMrTunnelPktsRcvd)

> Packets Sent (cmiMrTunnelPktsSent)

> Bytes Received (cmiMrTunnelBytesRcvd)

> Bytes Sent (cmiMrTunnelBytesSent)

> Active Redundancy State (cmiMrRedStateActive)

> Passive Redundancy State (cmiMrRedStatePassive)

### New HA Registration (cmiMrRegNewHa)

The number of times a mobile router registers with a different home agent due to changes in home agent / home agent priority.

### Better Interface Detected (cmiMrBetterIfDetected)

The number of times that the mobile router has detected a better interface.

### Packets on MR-HA Tunnel (cmiMrTunnelPktsRcvd)

The number of packets received on the mobile router-home agent tunnel.

### Packets Sent (cmiMrTunnelPktsSent)

The number of packets sent through the mobile router-home agent tunnel.

### Bytes Received (cmiMrTunnelBytesRcvd)

The number of bytes received on the mobile router-home agent tunnel.

### Bytes Sent (cmiMrTunnelBytesSent)

The number of bytes sent through the mobile router-home agent tunnel.

### Active Redundancy State (cmiMrRedStateActive)

The number of times the redundancy state of the mobile router changed to active.

### Passive Redundancy State (cmiMrRedStatePassive)

The number of times the redundancy state of the mobile router changed to passive.