# SSG Service Route Table

This dialog box displays details on the Service Selection Gateway (SSG) service route table.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Service Route Table from the Category list.

The following information is displayed:

> Service Name (cssgServiceName)

> Service Route Type (cssgServiceRouteType)

> Service Route Address (cssgServiceRouteAddr)

> Service Mask Type (cssgServiceRouteMaskType)

> Service Mask Address (cssgServiceRouteMask)

> Service Action (cssgServiceRoutePermission)

### Service Name (cssgServiceName)

Name of the service profile.

### Service Route Type (cssgServiceRouteType)

Value that represents the type of address stored in cssgServiceServRouteAddr.

### Service Route Address (cssgServiceRouteAddr)

IP address of the networks available to you.

### Service Mask Type (cssgServiceRouteMaskType)

Value that represents the type of address stored in cssgServiceServRouteMask.

### Service Mask Address (cssgServiceRouteMask)

Mask to be combined with the destination address before the destination address is compared to the value in cssgServiceRouteAddr.

### Service Action (cssgServiceRoutePermission)

Action to be taken on packets when the destination address matches with the cssgServiceRouteAddr.

Action can be:

Value | Description
1 | permit
2 | deny