# GGSN - SGSN Throughput

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category GGSN – SGSN T hroughput.

The following information appears:

> Remote Address (cGtpPathAddress)

> Remote Port (cGtpPathPort)

> Collection Interval (cGgsnSgsnThruPutInterval)

### Remote Address (cGtpPathAddress)

Address that uniquely identifies the remote node to which this path is established.

### Remote Port (cGtpPathPort)

Port on the remote node. A value of zero is invalid.

### Collection Interval (cGgsnSgsnThruPutInterval)

One of the values set in the objects cGgsnThruputIntervalOne or cGgsnThruputIntervalTwo except for value zero (0) which means that throughput collection is disabled.