# MIP Security Violations Table

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select MIP Security Violations Table.

The following information is displayed:

> Total Number of Security Violations (mipSecTotalViolations)

> Violator's Ip Address (mipSecViolatorAddress)

> Security Violations Count (mipSecViolationCounter)

> Latest Security Violation's SPI (mipSecRecentViolationSPI)

> Latest Security Violation's Time (mipSecRecentViolationTime)

> Latest Security Violation's 4 LSBs (mipSecRecentViolationIDLow)

> Latest Security Violation's 4 MSBs (mipSecRecentViolationIDHigh)

> Latest Security Violation's Reason (mipSecRecentViolationReason)

### Total Number of Security Violations (mipSecTotalViolations)

Total number of security violations for the entity.

### Violator's Ip Address (mipSecViolatorAddress)

Violator's IP address.

### Security Violations Count (mipSecViolationCounter)

Total number of security violations for the peer.

### Latest Security Violation's SPI (mipSecRecentViolationSPI)

Security parameter index (SPI) of the most recent security violation for the peer:

> If the security violation is due to an identification mismatch, then this is the SPI from the mobile-home authentication extension.

> If the security violation is due to an invalid authenticator, then this is the SPI from the offending authentication extension.

> In all other cases, the value is set to zero.

### Latest Security Violation's Time (mipSecRecentViolationTime)

Time of the most recent security violation for the peer.

### Latest Security Violation's 4 LSBs (mipSecRecentViolationIDLow)

Low-order 32 bits of identification used in requests or replies to the most recent security violation for the peer.

### Latest Security Violation's 4 MSBs (mipSecRecentViolationIDHigh)

High-order 32 bits of identification used in requests or replies to the most recent security violation for the peer.

### Latest Security Violation's Reason (mipSecRecentViolationReason)

Reason for the most recent security violation for the peer. There are six possible values:

> noMobilitySecurityAssociation (1)

> badAuthenticator (2)

> badIdentifier (3)

> badSPI (4)

> missingSecurityExtension (5)

> other (6)