# RS232A Port Configuration Information

The CiscoView Configure window displays the following information for an RS232A port:

Index

Bits Per Char

Bits

Parity

Auto Baud

# Index (rs232AsyncPortIndex)

Specifies the rs232PortIndex number of the port.

# Bits Per Char (rs232AsyncPortBits)

Specifies the number of bits in a character.

# Stop Bits (rs232AsyncPortSTopBits)

Specifies the number of stop bits. Possible values are 1, 2, 1 1/2, or dynamic.

# Parity (rs232AsyncPortParity)

Specifies the type of parity bit for each character. Possible values are none, odd, even, mark, or space.

# Autobaud (rs232AsyncPortAutobaud)

Specifies whether the port is enabled for autobaud transmission. Enabled means that the port senses input speed, parity, and character size automatically.