# CDMA PDSN Controller General

The CDMA PDSN Controller General category of the Device Configuration dialog box displays the general controller details of the packet data servicing node (PDSN).

## Procedure

1. Right-click the device, then select Configure. The Device configuration dialog box appears.

2. Select CDMA PDSN Controller General from the Category list.

The following information appears:

Max Sessions Allowed (cCdmaClusterSessHighThreshold)

Low Sessions Allowed (cCdmaClusterSessLowThreshold)

Record Count (cCdmaClusterTotalMembers)

### Max Sessions Allowed (cCdmaClusterSessHighThreshold)

Maximum number of allowed sessions. The agent generates a notification when this threshold is reached during call setup.

### Low Sessions Allowed (cCdmaClusterSessLowThreshold)

Minimum number of allowed sessions. The agent generates a notification when this threshold is reached during call release.

### Record Count (cCdmaClusterTotalMembers)

Total number of records in the PDSN cluster controller.