# GTP VS PDP Context

Use this dialog to view active Packet Data Protocol (PDP) traffic for various GTP versions.

## Procedure

In the Chassis view, right-click the device and select Monitor from the popup menu.

The following information appears:

> Active GTP v0 PDP (cGgsnActiveGtpVersion0Pdps)

> Active GTP v1 PDP (cGgsnActiveGtpVersion1Pdps)

### Active GTP v0 PDP (cGgsnActiveGtpVersion0Pdps)

Number of active GTP v0 PDP contexts.

### Active GTP v1 PDP (cGgsnActiveGtpVersion1Pdps)

Number of active GTP v1 PDP contexts.