# Home Agent Registration Group - Mobile Binding Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Home Agent Registration Group - Mobile Binding Configs.

The following information appears:

> MN's Home IP Address (haMobilityBindingMN)

> MN's CoA (haMobilityBindingCOA)

> MN Identifier Type (cmiHaRegMnIdentifierType)

> MN Identifier Associated (cmiHaRegMnIdentifier)

> Mobile Binding Registration Flags (cmiHaRegMobilityBindingRegFlags)

> Access Type (cmiHaRegMnIfDescription)

> Bandwidth (cmiHaRegMnIfBandwidth)

> Roaming Interface Identifier (cmiHaRegMnIfID)

> Multiple Path Metric Type (cmiHaRegMnIfPathMetricType)

> ### MN's Home IP Address (haMobilityBindingMN)

> Home IP address for the mobile node.

> ### MN's CoA (haMobilityBindingCOA)

> Care of address for the mobile node.

### MN Identifier Type (cmiHaRegMnIdentifierType)

The type of the mobile node's identifier.

### MN Identifier Associated (cmiHaRegMnIdentifier)

The identifier associated with the mobile node.

### Mobile Binding Registration Flags (cmiHaRegMobilityBindingRegFlags)

Registration flags sent by the mobile node.

### Access Type (cmiHaRegMnIfDescription)

Description of the access type for the roaming interface of the registering mobile node or router.

### Bandwidth (cmiHaRegMnIfBandwidth)

Bandwidth of the roaming interface through which the mobile node or router is registered.

### Roaming Interface Identifier (cmiHaRegMnIfID)

A unique number identifying the roaming interface through which the mobile node or router is registered. This is also used as an unique identifier for the tunnel from the home agent to the mobile router.

### Multiple Path Metric Type (cmiHaRegMnIfPathMetricType)

Specifies the metric to use when multiple path is enabled.