# Monitoring X.25 Circuits on a QLLC Interface

To monitor X.25 Circuits on a QLLC interface from the CiscoView Configure Port window, select X.25 Circuits from the CATEGORY popup menu. The following information is displayed:

In Interrupts (x25CircuitInInterrupts)

Out Interrupts (x25CircuitOutInterrupts)

In Octets (x25CircuitInOctets)

Out Octets (x25CircuitOutOctets)

Data RTx Timeouts(x25 CircuitDataRetransmissionTimeouts)

Reset Timeouts (x25CircuitResetTimeouts)

Interrupt Timeouts (x25CircuitInterruptTimeouts)

# In Interrupts (x25CircuitInInterrupts)

Displays the number of interrupt packets received.

# Out Interrupts (x25CircuitOutInterrupts)

Specifies the number of interrupt packets sent.

# In Octets (x25CircuitInOctets)

Specifies the number of octets of user data delivered to the upper layer.

# Out Octets (x25CircuitOutOctets)

Specifies the number of octets of user data sent.

# Data RTx Timeouts(x25 CircuitDataRetransmissionTimeouts)

Displays the number of times the T25 data retransmission timer expired.

# Reset Timeouts (x25CircuitResetTimeouts)

Displays the number of times the T22 reset timer expired.

# Interrupt Timeouts (x25CircuitInterruptTimeouts)

Displays the number of times the T26 Interrupt timer expired.