# CDMA PDSN Closed RP Registration Statistics - 2

## Procedure

1. Right-click the device and then select Monitor.

2. Select CDMA PDSN Closed RP Registration Statistics from the Category list.

3. Select a row and click on Monitor.

4. Select CDMA PDSN Closed RP Registration Statistics - 2 from the Category list.

The following information appears:

> Incoming-Call-Connected Dropped (ccpcPcfDroppedIccns)

> Call-Disconnect-Notify Received (ccpcPcfRcvdCdns)

> Call-Disconnect-Notify Sent (ccpcPcfSentCdns)

> Call-Disconnect-Notify Dropped (ccpcPcfDroppedCdns)

> Zero-Length-Buffer Recieved (ccpcPcfRcvdZlbs)

> Zero-Length-Buffer Sent (ccpcPcfSentZlb)

### Incoming-Call-Connected Dropped (ccpcPcfDroppedIccns)

Total number of Incoming-Call-Connected messages accepted since the L2TP tunnel was established with PCF.

### Call-Disconnect-Notify Received (ccpcPcfRcvdCdns)

Total number of Call-Disconnect-Notify messages received to tear down L2TP session since the L2TP tunnel was established with PCF.

### Call-Disconnect-Notify Sent (ccpcPcfSentCdns)

Total number of Call-Disconnect-Notify messages sent to PCF to tear down L2TP session since the L2TP tunnel was established with PCF.

### Call-Disconnect-Notify Dropped (ccpcPcfDroppedCdns)

Total number of Call-Disconnect-Notify messages dropped since the L2TP tunnel was established with PCF.

### Zero-Length-Buffer Recieved (ccpcPcfRcvdZlbs)

Total number of Zero-Length-Buffer messages received since the L2TP tunnel was established with PCF.

### Zero-Length-Buffer Sent (ccpcPcfSentZlb)

Total number of Zero-Length-Buffer messages sent since the L2TP tunnel was established with PCF.