# GGSN CAC Traffic Class Table

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN CAC Policy Table from the Category drop-down box.

5. With an entry selected in the GGSN CAC Policy Table dialog box, click Traffic Class Details.

The following information appears:

> CAC Policy Name (cggsnUmtsQosCacPolicyName)

> Traffic Class (cggsnUmtsQosCacTcTrafClass)

> Bit Rate Type (cggsnUmtsQosCacTcBitRateType)

> Direction (cggsnUmtsQosCacTcDirection)

> Bit Rate (cggsnUmtsQosCacTcBitRate)

> Reject on Exceeding Max Bit Rate (cggsnUmtsQosCacTcReject)

### CAC Policy Name (cggsnUmtsQosCacPolicyName)

Call Admission Control (CAC) policy name that will be attached to one or more Access Point Names (APNs).

### Traffic Class (cggsnUmtsQosCacTcTrafClass)

Universal Mobile Telephone System (UMTS) traffic class to which the MBR/GBR in the uplink/downlink will be assigned. There are four possible values:

> conversational

> streaming

> interactive

> background

Note: When cggsnUmtsQosCacTcBitRateType is set to guaranteed, only the values conversational and streaming can be set for this object.

### Bit Rate Type (cggsnUmtsQosCacTcBitRateType)

Bit rate type applicable to the traffic class indicated by cggsnUmtsQosCacTcTrafClass. There are two possible values:

> maximum

> guaranteed

### Direction (cggsnUmtsQosCacTcDirection)

Indicates the direction of traffic. There are two possible values:

> uplink

> downlink

### Bit Rate (cggsnUmtsQosCacTcBitRate)

MBR/GBR allowed for the traffic class indicated by cggsnUmtsQosCacTcTrafClass.

### Reject on Exceeding Max Bit Rate (cggsnUmtsQosCacTcReject)

Indicates whether the requested MBR/GBR is downgraded or the requested Packet Data Protocol (PDP) is rejected when the requested MBR/GBR exceeds the value set in cggsnUmtsQosCacTcBitRate.

> When set to true, the request is rejected.

> When set to false, the requested MBR/GBR is downgraded.