Rate Limit Status

The Rate Limit Status dialog box displays the following information:

Packets Permitted (ccarStatSwitchedPkts)

Bytes Permitted (ccarStatSwitchedBytes)

Packets Exceeding Limit (ccarStatFilteredPkts)

Bytes Exceeding Limit (ccarStatFilteredBytes)

Burst Size (ccarStatCurBurst)

Packets Permitted(ccarStatSwitchedPkts)

The counter of packets permitted by the rate limit.

Bytes Permitted(ccarStatSwitchedBytes)

The counter of bytes permitted by the interface.

Packets Exceeding Limit(ccarStatFilteredPkts)

The counter of packets which exceeded the rate limit.

Bytes Exceeding Limit(ccarStatFilteredBytes)

The counter of bytes, which exceeded the rate limit.

Burst Size(ccarStatCurBurst)

The current received burst size.