# GGSN Charging Gateways

The GGSN Charging Gateways category of the Chassis Configuration dialog box lists the charging gateway details of the GGSN.

Note This dialog is visible only if cGtpGSNService is set to 'ggsn'.

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN Charging Gateways from the Category list.

The following information appears:

Gateway Identifier (cgprsCgGatewayIndex)

Address Type (cgprsCgGatewayAddrType)

Address (cgprsCgGatewayAddr)

Gateway Table Row Status (cgprsCgGatewayRowStatus)

Gateway Status (cgprsCgOperStatus)

Gateway Reachability (cgprsCgLinkState)

### Gateway Identifier (cgprsCgGatewayIndex)

Unique identifier for the CG.

### Address Type (cgprsCgGatewayAddrType)

Type of Internet address given in cgprsCgGatewayAddr.

### Address (cgprsCgGatewayAddr)

IP address that uniquely identifies the CG.

### Gateway Table Row Status (cgprsCgGatewayRowStatus)

Status of the row in the charging gateway table. Used to create a new row or delete an existing row in the table.

To create a row, set this object to createAndGo. cgprsCgGatewayAddrType and cgprsCgGatewayAddr are the mandatory objects in a create request.

To delete a row, set this object to destroy.

### Gateway Status (cgprsCgOperStatus)

Indicates whether the configured CG is active.

Value | Description
undefined (1) | Neither in the active nor in the standby mode
active (2) | In the active mode
standby (3) | In the standby mode

### Gateway Reachability (cgprsCgLinkState)

Indicates the status of the CG. The status can be:

Value | Description
on | CG is reachable
pending | CG is not reachable but the GGSN is trying to establish a connection with it
off | CG is not reachable