# CDMA PDSN Registration Denied Statistics

Use this option to view registration statistics of denied requests.

## Procedure

To access registration denied statistics information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN Registration Denied Stats from the Category menu.

Registration Denied Statistics dialog box displays:

Registration Request Denied (cCdmaRpRegDeniedReqs)

Registration Request Discarded (cCdmaRpRegDiscardedReqs)

Registration Request for New connection Denied (cCdmaRpInitRegDeniedReqs)

Registration Request for Refreshing connection Denied (cCdmaRpReRegDeniedReqs)

Registration Request for Disconnection Denied (cCdmaRpDeRegDeniedReqs)

### Registration Request for Disconnection Denied (cCdmaRpDeRegDeniedReqs)

Number of denied A-11 registration requests since system startup that are used for deactivating the established R-P connections.

The code field in the registration reply is set to non-zero.

### Registration Request Denied (cCdmaRpRegDeniedReqs)

Number of A-11 registration requests denied since system startup.

The code field in the registration reply is set to non-zero.

### Registration Request Discarded (cCdmaRpRegDiscardedReqs)

Number of A-11 registration requests discarded since system startup.

A registration reply is not returned for these A-11 registration requests.

### Registration Request for New connection Denied (cCdmaRpInitRegDeniedReqs)

Number of denied A-11 registration requests since system startup that are used for establishing new R-P connections.

These A-11 registration requests contain the connection setup airlink record.

The code field in the registration reply is set to non-zero.

### Registration Request for Refreshing connection Denied (cCdmaRpReRegDeniedReqs)

Number of denied A-11 registration requests since system startup that are used for refreshing the established R-P connections. The code field in the registration reply is set to non-zero.