# Brouter

Device>Configure>Brouter

To display or change brouter information from the CiscoView Configure Device window, select Brouter from the CATEGORY popup menu.

The following brouter configuration information is displayed:

Enable RIP (brouterEnableRip)

Whether the RIP protocol has been enabled on the device. Possible values are enabled or disabled.

Spanning Tree (brouterEnableSpanTree)

Whether the Spanning Tree Protocol has been enabled or disabled on the device.

Giant Pkg Check (brouterEnableGiantCheck)

Whether special handling of giant packets is enabled or disabled.

IP Fragmentation (brouterEnableIpFragmentation)

Whether IP fragmentation is enabled or disabled.

ICMP Unreachables (brouterEnableUnreachables)

Whether ICMP unreachable messages are sent.

IPX FDDI Snap to Ethernet (brouterIpxSnapToEther)

Default translation method for IPX packets when bridging from FDDI SNAP to Ethernet. Possible values are snap, ethernetII, iso8023, or raw8023.

IPX FDDI 802.2 to Ethernet (brouterIpx8022ToEther)

Default translation method for IPX packets when bridging from FDDI 802.2 to Ethernet. Possible values are snap, ethernetII, iso8023, or raw8023.

IPX Ethernet to FDDI (brouterIpx8023RawToFddi)

Default translation for IPX packets when bridging. Possible values are snap and iso8022.

CAM Mode (brouterCamMode)

Whether the CAM module is operating in filtering or forwarding mode.

Forwarding DB Aging (brouterCamAgingTime)

Aging time for the CAM table. Possible values are from 0 through 1,000,000.

Ethernet Receive Max Size (brouterEthernetReceiveMax)

Maximum number of Ethernet receive buffers processed at one time per port. Possible values are 1 through 120.

Ethernet Transmit Max Size (brouterEthernetTransmitMax)

Maximum number of Ethernet transmit buffers processed at one time per port. Possible values are from 1 through 120.

FDDI Receive Max Size (brouterFddiReceiveMax)

Maximum number of FDDI receive buffers processed at one time per port. Possible values are from 1 through 120.

FDDI Transmit Max Size (brouterFddiTransmitMax)

Maximum number of FDDI transmit buffers processed at one time per port.