# GGSN Access Point Throughput Statistics

## Procedure

1. Right-click the device and then select Monitor.

2. Select category GGSN Access Point Throughput Statistics.

3. Select a row and click Throughput Statistics.

The following information appears:

> Last Collected Time (cgprsAccPtThruPutLastCollected)

> Upstream Bytes (cgprsAccPtUpstrByteCount)

> Downstream Bytes (cgprsAccPtDownstrByteCount)

> Upstream Packets (cgprsAccPtUpstrPktCount)

> Downstream Packets (cgprsAccPtDownstrPktCount)

### Last Collected Time (cgprsAccPtThruPutLastCollected)

This object represents the delta value between the time when this data is collected and the time it is been retrieved.

### Upstream Bytes (cgprsAccPtUpstrByteCount)

This object represents the total payload volume in upstream traffic sent on this APN in the last sampling period specified by cgprsAccPtThruputInterval.

### Downstream Bytes (cgprsAccPtDownstrByteCount)

This object represents the total payload volume in downstream traffic sent on this APN in the last sampling period specified by cgprsAccPtThruputInterval.

### Upstream Packets (cgprsAccPtUpstrPktCount)

This object represents the number of upstream packets sent on this APN in the last sampling period specified by cgprsAccPtThruputInterval.

### Downstream Packets (cgprsAccPtDownstrPktCount)

This object represents the number of downstream packets sent on this APN in the last sampling period specified by cgprsAccPtThruputInterval.