# Circuits

The following circuit information is displayed:

> Channel Number (x25CircuitChannel)

> Status (x25CircuitStatus)

> Circuit Establish Time (x25CircuitEstablishTime)

> Direction of Call (x25CircuitDirection)

> Call Parameters Index (x25CircuitCallParamId)

> Called Address (x25CircuitCalledDteAddress)

> Calling Address (x25CircuitCallingDteAddress)

> Originally Called Address (x25CircuitOriginallyCalledAddress)

> Circuit Description (x25CircuitDescr)

Status (x25CircuitStatus)

Current status of the selected circuit.

Circuit Establish Time (x25CircuitEstablishTime)

Specifies the value of the sysUpTime MIB descriptor when the channel was associated with this circuit.

Direction of Call (x25CircuitDirection)

Specifies the direction of the call that established this circuit. Possible values are incoming, outgoing, and pvc.

Channel Number (x25CircuitChannel)

Channel number of the circuit.

Call Parameters Index (x25CircuitCallParamId)

Instance of the x25CallParamIndex for the entry in the X25CallParamTable which contains the call parameters in use with the circuit.

The entry must contain the values in use by the circuit. Null means the circuit is a PVC or is using all the default parameters.

Called Address (x25CircuitCalledDteAddress)

Called address.

For incoming calls, it is from the call indication packet.

For outgoing calls, it is if from the call confirmation packet.

This will be zero length for PVCs.

Calling Address (x25CircuitCallingDteAddress)

Calling address.

For incoming calls, it is from the call indication packet.

For outgoing calls,it is from the call confirmation packet.

This will be zero length for PVCs.

Originally Called Address (x25CircuitOriginallyCalledAddress)

Original call address when a call is deflected or redirected.

For incoming calls, it is the address in the redirection or call deflection notification facility if the call was deflected or redirected.

For outgoing calls, it is the address from the call request packet.

This will be zero length for PVCs.

Circuit Description (x25CircuitDescr)

Descriptive string associated with the circuit.

Provides a place for the agent to supply any descriptive information it knows about the use or owner of the circuit. The agent may return the process identifier and user name for the process using the circuit.

Alternatively, the agent may return the name of the configuration entry that caused a bridge to establish the circuit. A zero length values means the agent has no additional information.