# Flow Control Objects

## Navigation

Device > Configure > Flow Control

The following information appears:

> Notif Enable (cc6kxbarFlowCtrlNotifEnable)

> Threshold Mode (cc6kxbarFlowCtrlBusFIFOThrMode)

> Threshold Value (cc6kxbarFlowCtrlBusFIFOThrValue)

> Trans Time (cc6kxbarFlowCtrlBusFIFOTransTime)

### Notif Enable (cc6kxbarFlowCtrlNotifEnable)

Indicates whether notifications are generated for the flow control feature. If a bit corresponding to a notification is set to one, then that notification will be generated.

### Threshold Mode (cc6kxbarFlowCtrlBusFIFOThrMode)

Specifies the configuration mode of the system bus flow control FIFO threshold. There are three possible values:

> off—The flow control FIFO threshold is set to the original value defined by the system.

> on—The flow control FIFO threshold is set to the lower value defined by the system.

> auto—The system monitors the system bus flow control FIFO threshold. The system will change this threshold from the original value to the lower value the first time it detects that the threshold is being exceeded on a physical entity (such as a module).

### Threshold Value (cc6kxbarFlowCtrlBusFIFOThrValue)

Indicates whether the current value of the system bus flow control FIFO threshold is the original value or the lower value defined by the system. There are two possible values:

> original

> lower

### Trans Time (cc6kxbarFlowCtrlBusFIFOTransTime)

When the value of cc6kxbarFlowCtrlBusFIFOThrValue is set to lower, this object indicates the value of sysUpTime when the system bus flow control FIFO threshold is transitioned to a lower value. When the value of cc6kxbarFlowCtrlBusFIFOThrValue is set to original, the value of this object is zero.