# CDMA PDSN PCF Statistics

This dialog box is applicable to Member and Peer to Peer clusters.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN PCF Table.

4. With an entry selected in the CDMA PDSN PCF table, click Monitor.

The following information is displayed:

> PCF Sessions Count (cCdmaPcfSessionTotal)

> Max Num of PCF Sessions (cCdmaPcfSessionMaxTotal)

> PCF Session Errors (cCdmaPcfErrorTotal)

### PCF Sessions Count (cCdmaPcfSessionTotal)

Number of connections established with a packet control function (PCF).

### Max Num of PCF Sessions (cCdmaPcfSessionMaxTotal)

Maximum number of simultaneous connections for a PCF.

### PCF Session Errors (cCdmaPcfErrorTotal)

Number of session errors for a PCF.