# RP Update Failures

Use this option to view Packet Control Function (PCF) and Service Option (SO) based RP Update Failures.

## Procedure

To access RP Update Failures information:

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category menu.

3. Select any row and click on RP Update Statistics.

4. Select RP Update Failures from the Category menu.

The following information appears:

> Unknown Failures (cCdmaPcfSoRpUpdReaUnSpecFails)

> Administrative Failures (cCdmaPcfSoRpUpdAdmnFails)

> MN Authentication Failures (cCdmaPcfSoRpUpdMNAuthFails)

> ID Mismatch Failures (cCdmaPcfSoRpUpdIdMismatFails)

> Bad Request Failures (cCdmaPcfSoRpUpdBadReqFails)

### Unknown Failures (cCdmaPcfSoRpUpdReaUnSpecFails)

Number of registration updates that failed for an unspecified reason since system startup.

### Administrative Failures (cCdmaPcfSoRpUpdAdmnFails)

Since system startup, the number of registration updates that failed due to an administrative prohibition.

### MN authentication Failures (cCdmaPcfSoRpUpdMNAuthFails)

Since system startup, the number of registration updates that failed due to an Mobile Node (MN) authentication failure.

### ID mismatch Failures (cCdmaPcfSoRpUpdIdMismatFails)

Since system startup, the number of registrations that failed due to a registration identity mismatch since system startup.

### Bad request Failures (cCdmaPcfSoRpUpdBadReqFails)

Since system startup, the number of registration updates that failed due to a poorly formed request.