# Monitoring Serial Statistics on a QLLC Port Interface

To monitor serial statistics on a QLLC interface from the CiscoView Configure Port window, select Serial Stats from the CATEGORY popup menu. The following information is displayed:

Aborted Pkts (locIfInAbort)

Misaligned Pkts (locIfInFrame)

Carrier Sig Trans (locIfCarTrans)

Overruns (locIfInOverrun)

Checksum Err Pkts (locIfInCRC)

# Aborted Pkts (locIfInAbort)

Shows the number of input packets that were aborted.

# Misaligned Pkts (locIfInFrame)

Shows the number of input packets that were misaligned.

# Carrier Sig Trans (locIfCarTrans)

Shows the number of times the interface detected the carrier signal transition.

# Overruns (locIfInOverrun)

Shows the amount of input that arrived too quickly for the hardware to receive.

# Checksum Err Pkts (locIfInCRC)

Shows the number of input packets that had cyclic redundancy checksum (CRC) errors.