# Firewall Service Blade: Configure Firewall Interfaces

You can configure firewall interfaces, using this second option of the firewall service blade setup wizard, or the Configure Firewall Interface(s) option in the Firewall menu.

## Navigation

For the Firewall Service Blade Setup Wizard:

1. Right-click the blade, then select Firewall Service Blade Setup Wizard.

2. Click Next till the Configure Firewall Interfaces option, in the left pane, is selected.

For the Firewall menu:

1. Right-click the blade, then select Configure Firewall Interface(s).

The following information appears:

VLAN Name

Secured VLAN Interfaces

Security Level

IP Address

Subnet Mask

To create a new firewall interface click Create.

To delete a firewall interface, select a row, then click Delete.

To change the security level, IP address, and subnet mask of the interface, select a row, then click Modify.

In the Firewall Service Blade Setup Wizard:

To go to the previous wizard option click Back.

To go to the next wizard option, click Next.

### VLAN Name

Name of the VLAN.

### Secured VLAN Interfaces

Name of the secured firewall interface.

### Security Level

Level of security of the firewall interface.

### IP Address

IP address assigned to the VLAN

### Subnet Mask

Subnet mask of the VLAN IP address.