PATH=/ciscoview/Routershare/config/AAA.htm TITLE=AAA TEXT=(Authentication, Authorization, Accounting) This dialog box provides the following options : Lists the configured servers View configurations of individual Monitor communications and status Summary statistics Server sessions based ,Accounting. Procedure Right-click device, select information appears: (casIndex) (casProtocol) IP (casAddress) (casAuthenPort) (casAcctPort) (casState) (casPriority) row, Availability open dialog. Response Time Related Topics Availablity Table index. used with server. tacacsplus(1) represents TACACS+. radius(2) RADIUS address. UDP TCP port authentication configuration. Explicitly set Default IOS radius: 1645. accounting service For TACACS+, ignore casAuthenPort. value 1646. Current state 'up(1)' responding requests. 'dead(2)' means failed respond. marked when does not after maximum retransmissions. either waiting period some received. Initial system reinitialization. It transitions attempt communicate fails. Number that shows priority. Lower numbers higher
PATH=/ciscoview/Routershare/config/AAA_Accounting.htm TITLE=AAA_Accounting TEXT=AAA Accounting The AAA Accounting monitors accounting statistics of the server. The statistics is the delta value(present Right-click previous value) information polling interval and unit measurement Nos/Interval Procedure device, then select row (casAcctServerErrorResponses) Configuration Table, button following appears: (casAcctRequests) (casAcctRequestTimeouts) (casAcctUnexpectedResponses) (casAcctIncorrectResponses) Error Incorrect (casAcctTransactionSuccesses) Successes (casAcctTransactionFailures) Number requests. since system reinitialization. Retransmissions due timeouts are counted distinct timedout results retransmission request. stop when reaches maximum. unexpected responses received from reinitialization; example, delayed These indicate that identified its operation. unprocessed Reasons inability decrypt response, invalid fields, successful transactions performed includes multiple occur. responds with either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/config/AAA_Accounting_Sessions.htm TITLE=AAA_Accounting_Sessions TEXT=AAA Accounting Sessions The AAA Accounting Sessions provides data for accounting sessions based on Authentication, Authorization, Procedure Right-click device, select Sessions. Click following information appears: (casnSessionId) (casnUserId) Framed-IP-Address. Address (casnIpAddr) (casnIdleTime) Time (casnDisconnect) (casnCallTrackerId) Identifies protocols session. unique value within system even multiple are 'user'. that corresponds attributes: RADIUS represents 44, Acct-Session-Id TACACS + 'task_id' login ID zero length string unavailable. 1, User-Name. 0.0.0.0 cannot applicable 8, 'addr'. elapsed since last user-level was received transmitted. Protocol handshaking associated call idle. End of Setting true(1), initiates termination. casnActiveEntry removed after sesion ends. When set process be canceled by false(2). Index CISCO-CALL-TRACKER-MIB cctActiveTable Using this query more detailed about
PATH=/ciscoview/Routershare/config/AAA_Authentication.htm TITLE=AAA_Authentication TEXT=AAA Authentication AAA Authentication monitors the authentication statistics of the server. The statistics delta value(present Right-click previous value) information polling interval and unit measurement Nos/Interval Procedure device, select row (casAuthenServerErrorResponses) Configuration Table, following appears: (casAuthenRequests) (casAuthenRequestTimeouts) (casAuthenUnexpectedResponses) (casAuthenIncorrectResponses) Error Incorrect (casAuthenTransactionSucesses) Successes (casAuthenTransactionFailures) Number requests. when active. Retransmissions due timeouts are counted distinct timed since was made results retransmission request. stop reaches maximum. unexpected responses received For example, delayed These mean that identified with its operation. unprocessed Reasons inability decrypt response, invalid fields, successful transactions this includes multiple occur. responds either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/config/AAA_Authorization.htm TITLE=AAA_Authorization TEXT=AAA Authorization The AAA Authorization monitors authorization statistics of the server. The statistics delta value(present Right-click previous value) information polling interval and unit measurement Nos/Interval Procedure device, then select row (casAuthorServerErrorResponses) Configuration Table, Authorization. following appears: (casAuthorRequests) (casAuthorRequestTimeouts) (casAuthorUnexpectedResponses) (casAuthorIncorrectResponses) Error Incorrect (casAuthorTransactionSuccesses) Successes (casAuthorTransactionFailures) Number requests. since was made active. Retransmissions due timeouts are counted distinct It not instantiated protocols that do support function. timed results retransmission request. stop when reaches maximum. unexpected responses received from active; example, delayed These show identified its operation. unprocessed Reasons inability decrypt response, invalid fields, successful transactions with this includes multiple occur. responds either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/config/AAA_Response_Time.htm TITLE=AAA_Response_Time TEXT=AAA Response Time AAA Response Time provides the time required for the server to respond to Authentication, Authorization and Accounting. Procedure Right-click device, select row of Configuration Table, following information appears: (casAuthenResponseTime) (casAuthorResponseTime) (casAcctResponseTime) Average authentication requests sent since system reinitialization, excluding timeouts. It distinct not instantiated protocols that do support function. accounting
PATH=/ciscoview/Routershare/config/AAA_Server_Availability.htm TITLE=AAA_Server_Availability TEXT=AAA Server Availability The AAA Server Availability provides details on the current status of the server. Procedure Right-click device, then select AAA. row Configuration Table, following information appears: (casState) (casCurrentStateDuration) (casPreviousStateDuration) (casTotalDeadTime) (casDeadCount) Time Count state, 'up(1)' represents responding to requests. 'dead(2)' means failed respond. retransmissions. marked when does not after maximum either waiting period some response received. Initial value system reinitialization. It transitions attempt communicate fails. elapsed since reached its shown casState. previous prior most recent This zero if has changed state. although was reinitialized. Number times transitioned
PATH=/ciscoview/Routershare/config/AAA_Server_Statistics_Accounting.htm TITLE=AAA_Server_Statistics TEXT=AAA Server Statistics- Accounting The AAA Server Statistics- Accounting, allows comparison of various statistical details among servers. Procedure Right-click device, Authentication. select Click Summary following information appears: (casIndex) (casProtocol) IP (casAddress) (casAcctRequests) (casAcctRequestTimeouts) (casAcctUnexpectedResponses) (casAcctServerErrorResponses) Error (casAcctIncorrectResponses) (casAcctResponseTime) (casAcctTransactionSuccesses) Successes (casAcctTransactionFailures) Management station that initiates new configuration. It uses randomly value when creating instance casConfigEntry. casConfigRowStatus semantics prevents access conflicts. Snmp set fails existing entry chosen row creation. used with this server. tacacsplus(1) represents TACACS+ radius(2) RADIUS address. Number requests. since system reinitialization. Retransmissions due timeouts. are counted distinct unexpected responses received from reinitialization; example, delayed timed request. These indicate identified its operation. unprocessed Reasons inability decrypt response, invalid fields, Average reinitialization, excluding successful transactions performed includes multiple retransmission occur. responds either pass fail. failed failure occurs resends reach maximum aborts transaction.
PATH=/ciscoview/Routershare/config/AAA_Server_Statistics_Authentication.htm TITLE=AAA_Server_Statistics TEXT=AAA Server Statistics- Authentication The AAA Server Statistics- Authentication, allows comparison of various statistical details among servers. Procedure Right-click device, select Click Summary following information appears: (casIndex) (casProtocol) IP (casAddress) (casAuthenRequests) (casAuthenRequestTimeouts) (casAuthenUnexpectedResponses) (casAuthenServerErrorResponses) Error (casAuthenIncorrectResponses) (casAuthenResponseTime) (casAuthenTransactionSuccesses) Successes (casAuthenTransactionFailures) Table index. used with this server. tacacsplus(1) represents TACACS+ radius(2) RADIUS address. Number requests. when active. Retransmissions due timeouts. are counted distinct timed since was made results retransmission request. stop reaches maximum. unexpected responses received For example, delayed These mean that identified its operation. unprocessed Reasons inability decrypt response, invalid fields, Average system reinitialization, excluding successful transactions includes multiple occur. responds either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/config/AAA_Server_Statistics_Authorization.htm TITLE=AAA_Server_Statistics TEXT=AAA Server Statistics- Authorization The AAA Server Statistics- Authorization, allows comparison of various statistical details among servers. Procedure Right-click device, then select Click Summary Authorization. following information appears: (casIndex) (casProtocol) IP (casAddress) (casAuthorRequests) (casAuthorRequestTimeouts) (casAuthorUnexpectedResponses) (casAuthorServerErrorResponses) Error (casAuthorIncorrectResponses) (casAuthorResponseTime) (casAuthorTransactionSuccesses) Successes (casAuthorTransactionFailures) Table index. used with this server. tacacsplus(1) represents TACACS+ radius(2) RADIUS address. Number requests. since was made active. Retransmissions due timeouts. are counted distinct It not instantiated protocols that do support function. timed results retransmission request. stop when reaches maximum. unexpected responses received from active; example, delayed These show identified its operation. unprocessed Reasons inability decrypt response, invalid fields, Average system reinitialization, excluding successful transactions includes multiple occur. responds either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/config/AAA_Server_Statistics_Server_Availablity.htm TITLE=AAA_Server_Statistics_Server_Availability TEXT=AAA Server Statistics- Server Availability The AAA Server Statistics- server availability, allows comparison of various statistical details among servers. Procedure Right-click device, then select Click Summary Availability. following information appears: (casIndex) (casProtocol) IP (casAddress) (casCurrentStateDuration) (casState) (casPreviousStateDuration) Prev (casTotalDeadTime) (casDeadCount) Time Count Servers Table index. used with server. tacacsplus(1) represents TACACS+ radius(2) RADIUS address. state, 'up(1)' responding requests. 'dead(2)' means failed respond. marked when does not after maximum retransmissions. either waiting period some response received. Initial value system reinitialization. It transitions attempt communicate fails. elapsed since reached its current shown casState. previous prior most recent This zero if has changed state. although was reinitialized. Number times transitioned
PATH=/ciscoview/Routershare/config/address_allocated_config.htm TITLE=Address Allocated Config TEXT=Navigation Right-click the device, and select Configure . The Device Configuration window appears. Select from Category list. following information appears: (cIpLocalPoolAllocAddrType) (cIpLocalPoolAllocAddr) cIpLocalPoolAllocAddrType. Inet Allocation Interface (cIpLocalPoolAllocIfIndex) Person (cIpLocalPoolAllocUser) of cIpLocalPoolAllocAddr. IP address. this object described by which message was sent. cannot determined, value will zero. user name whom
PATH=/ciscoview/Routershare/config/AHDLC_Engine_Details.htm TITLE=AHDLC Engine Details TEXT=The AHDLC Engine Details category of the Configure dialog box displays details of the AHDLC (asynchronous high-level data link control) engine. Procedure Right-click device, then select double-click device. from list. following information appears: (cCdmaAhdlcEngineIndex) (cCdmaAhdlcEngineName) (cCdmaAhdlcEngineType) Operational (cCdmaAhdlcEngineOperState) Desired (cCdmaAhdlcEngineAdminState) Notification Status (cCdmaAhdlcEngineDownNotifEnabled) Service Adapter (cCdmaAhdlcPhysicalIndex) Arbitrary non-zero integer-value that uniquely identifies cannot (AHDLC) index implemented such engines Hardware: assigned consecutive monotonically increasing values. Textual name by local Asynchronous type. be: hardware-based requires use assist. Each peer one Software: software-based but relies system, cpu(s) perform framing. Unknown: determined. state. up down. means ready receive packets. If should also changed packets; remain only there fault prevents going Initially interfaces start result either explicit management action configuration retained managed Indicates will sent out when and object true. Entry ENTITY-MIB (RFC-2737) corresponding adapter. entPhysicalIndex corresponsing 0 applicable.
PATH=/ciscoview/Routershare/config/AHDLC_Engine_Statistics.htm TITLE=AHDLC Engine Statistics TEXT=The AHDLC Engine Statistics dialog box displays the asynchronous high-level data link control (AHDLC) statistics. Procedure Right-click device, then select Configured Category double-click device. Details from list. and More Info following information appears: Maximum (cCdmaAhdlcEngineMaxChannels) (cCdmaAhdlcEngineConfMaxChannels) number of channels that cannot supported by engine. user. This value higher than cCdmaAhdlcEngineMaxChannels.
PATH=/ciscoview/Routershare/config/BGP_General_Information.htm TITLE=BGP4 General Information TEXT=The BGP4 General Information dialog box displays the border gateway protocol version and the local autonomous system number. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Device Configuration appears. Protocols from Category list. SelectProtocol Details button. later: indexed Note left frame categories right details, table. If displayed, variable which key values of are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following appears: (bgpVersion) AS No. (bgpLocalAs) Related Topics Peer Received Paths Attributes Vector numbers supported. Each negotiates this vector. identified through string bits object. first octet; contains 0. 7, second 8 15, so on, with most significant (MSB) referring example, refers bit, say present set, (i+1) Number system.
PATH=/ciscoview/Routershare/config/BGP_Peer_Information.htm TITLE=BGP4 Peer Information TEXT=The BGP4 Peer Information dialog box displays information about the peer. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select (bgpPeerHoldTimeConfigured) device, double-click Device Configuration appears. Protocols from Category list. SelectProtocol standard Details button. later: Note left frame categories right table. If displayed, variable which indexed key values: of compared listed below category. view particular rows Multiple indexes table, any, nested manner. that, value. lowest indexing row. pane. following appears: (bgpPeerRemoteAddr) IP Address (bgpPeerIdentifier) Connection (bgpPeerState) Desired (bgpPeerAdminStatus) (bgpPeerNegotiatedVersion) Version (bgpPeerLocalAddr) (bgpPeerLocalPort) (bgpPeerRemotePort) (bgpPeerMinASOriginationInterval) No. (bgpPeerRemoteAs) (bgpPeerLastError) Error Code (bgpPeerConnectRetryInterval) (bgpPeerMinRouteAdvertisementInterval) (bgpPeerHoldTime) Timer (bgpPeerKeepAlive) (bgpPeerKeepAliveConfigured) Min Origination Route Advertisement Related Topics General Received Paths Attributes entry's connection. can be: Description 120 idle 30 active opensent openconfirm 6 established. state stop start transition generates Event. running between two peers. port TCP objects bgpPeerLocalAddr, bgpPeerLocalPort, bgpPeerRemoteAddr, provide appropriate reference MIB Number remote autonomous system. subcode. last seen 2-byte has occurred, this field zero. Otherwise, first octet string contains code, seconds. interval, timer. recommended seconds, hold with speaker calculates using smaller message. cases whereas not been zero, least keep Keepalive calculated such same bgpPeerHoldTimeConfigured. configured message, determines However, must greater equal 90 frequency messages relation actual given bgpPeerKeepAlive. maximum normally one-third periodical after minimum 15
PATH=/ciscoview/Routershare/config/BGP_Policy_Accounting.htm TITLE=BGP4 Policy Accounting TEXT=The BGP Policy Accounting dialog box displays the different types of traffic on a particular interface. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Device Configuration appears. Protocols from Category list. SelectProtocol and Details button. later: Note left frame categories right table. If displayed, variable which indexed key values are listed below category. view rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: Type (cbpAcctTrafficIndex) Related Topics General Peer Received Paths Attributes Integer with greater 0 uniquely identifies traffic-type. has no intrinsic meaning. It classifies coming into types. up you various traffic-types
PATH=/ciscoview/Routershare/config/BGP_Received_Paths_Attributes.htm TITLE=BGP4 Received Paths Attributes TEXT=BGP4 Received Paths - Attributes The BGP4 Received Paths Attributes dialog box displays the attributes of paths. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then selected Configure device, double-click Device Configuration appears. Protocols from Category list. SelectProtocol and Details button. later: indexed Note left frame categories right details, table. If displayed, variable which key values are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information. appears: IP Address (bgp4PathAttrIpAddrPrefix) Length, (bgp4PathAttrIpAddrPrefixLen) (bgp4PathAttrPeer) (bgp4PathAttrOrigin) (bgp4PathAttrASPathSegment) Segment Sequence Border Router (bgp4PathAttrNextHop) Metrics Disc. Multi. (bgp4PathAttrMultiExitDisc) Points Degree Preference (bgp4PathAttrLocalPref) Selection (bgp4PathAttrAtomicAggregate) (bgp4PathAttrAggregatorAS) No. (bgp4PathAttrAggregatorAddr) Calculated (bgp4PathAttrCalcLocalPref) (bgp4PathAttrBest) (bgp4PathAttrUnknown) Related Topics General prefix. networks layer reachability field. This object. containing specified by bgp4PathAttrIpAddrPrefixLen. Bits beyond bgp4PathAttrIpAddrPrefixLen, converted zeroes. bits, peer where learnt Information origin can be: Code Description igp (1) Internal egp (2) via incomplete (3) Undetermined Number remote autonomous system. used destination network. discriminate between exit adjacent -1 means not present. Originating speaker's advertised route. Indicates local has less specific rather more last performed aggregation. 0.0.0.0 receiving speaker. was chosen best false true Octets string size, 255 shows understood. zero, there were maximum recorded
PATH=/ciscoview/Routershare/config/card_config_entityInfo.htm TITLE=Entity Information TEXT=-Card This category provides information about the selected card. Procedure Right-click the card, then configure Select from list. following appears: (entPhysicalIndex) Description (entPhysicalDescr) (entPhysicalVendorType) Type of physical entitiy which CPUs, statistics entry maintained can be chip, group Identifies manufacturer's name entity. An indication vendor-specific hardware If unknown registration identifier exists value by agent, 00
PATH=/ciscoview/Routershare/config/cdma_pdsn_closed_rp_info.htm TITLE=CDMA PDSN Closed RP Information TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select CDMA from Category list. following appears: (ccpcEnabled) (ccpcSessionTotal) Sessions An indication of whether feature enabled. total number currently established with this system.
PATH=/ciscoview/Routershare/config/CDMA_PDSN_Cluster.htm TITLE=CDMA PDSN Cluster TEXT=The PDSN Cluster category of the Device Configuration dialog box allows you to view the packet data servicing node (PDSN) details. Procedure Right-click device, then select Configure double-click device. appears. from list. following information appears: (cCdmaClusterType) (cCdmaClusterRole) cluster. can be: Value Description 0 nonCluster 1 peerToPeer 2 controllerMember. plays within member type notApply Means does any role. has this if
PATH=/ciscoview/Routershare/config/CDMA_PDSN_Cluster_Controller_Table.htm TITLE=CDMA PDSN Cluster Controller Table TEXT=The PDSN Cluster Controller Table category of the Device Configuration dialog box allows you to view packet data servicing node (PDSN) details. Procedure Right-click device, then select notConfigured double-click device. appears. from list. following information appears: (cCdmaClusterCtrlAddressType) Type (cCdmaClusterCtrlAddress) (cCdmaClusterCtrlStatus) IP address particular controller. combined with used as index identify unique entry. along can Operational status maintained by member. be: Value Description 1 2 configured 3 alive
PATH=/ciscoview/Routershare/config/CDMA_PDSN_Cluster_Member_Table.htm TITLE=CDMA PDSN Cluster Member Table TEXT=The PDSN Cluster Member Table category of the Device Configuration dialog box allows you to view the packet data servicing node (PDSN). details. Procedure Right-click device, then select Configure double-click device. appears. from list. following information appears: (cCdmaClusterMemberAddressType) Type (cCdmaClusterMemberAddress) (cCdmaClusterMemberStatus) (cCdmaClusterMemberLoad) IP address member. combined with and used as index identify unique entry. Operational status. can be: Value Description 1 unknown controller does not 2 ready serve calls. setup, request. 3 adminProhibit new but maintains existing load aggregate percentage maximum that serviced.
PATH=/ciscoview/Routershare/config/CDMA_PDSN_Controller_General.htm TITLE=CDMA PDSN Controller General TEXT=The CDMA PDSN Controller General category of the Device Configuration dialog box displays the general details packet data servicing node (PDSN). Procedure Right-click device, then select Configure appears. from list. following information appears: Maximum Sessions Allowed (cCdmaClusterSessHighThreshold) (cCdmaClusterSessLowThreshold) Record Count (cCdmaClusterTotalMembers) number sessions. agent generates notification when this threshold reached during call setup. Minimum release. records cluster controller.
PATH=/ciscoview/Routershare/config/CDMA_PDSN_Fail_History_Table.htm TITLE=CDMA PDSN Fail History Table TEXT=Use this option to view CDMA PDSN failure history. Procedure To access CDMA PDSN fail history table information: Right-click the device and select Configure from popup menu. dialog box displays: (cCdmaFailSessionIndex) MSID Identifier (cCdmaFailSessionMsid) (cCdmaFailSessionMsidType) Electronic Station Number (cCdmaFailSessionEsn) HA IpAddress (cCdmaFailSessionA11HaIp) FA (cCdmaFailSessionA11FaIp) Connection (cCdmaFailSessionConnId) (cCdmaFailSessionKey) Date & (cCdmaFailHistFailTime) (cCdmaFailHistFailType) Related Topics System Information PCF MoIP Flows unique monotonically incrementing entry identifier. wraps zero. Mobile of failed session. that had user serial home agent address interface foreign GRE identification key time occurred. type current record.
PATH=/ciscoview/Routershare/config/CDMA_PDSN_feature_overview.htm TITLE=CDMA PDSN feature overview TEXT=CDMA PDSN Overview This overview module describes the Cisco Packet Data Serving Node (Cisco PDSN) feature. It includes following sections: System Benefits For More Information Related Features, Standard Technologies Documents hardware IOS software that enables 7500 series router, Protocol-Independent function IP-based gateway between wireless Radio Access Network (RAN) Internet. With enabled stationary roaming mobile user can Internet, corporate intranet, Application (WAP) services. supports both Simple IP. operation. Note operation, which referred types. available determined by offered provider. context PDSN, end CDMA2000 architecture defined TIA/EIA/IS-835 (also known 3GPP2 TSG-P TR45.6). typical terminal equipment, termination, transceiver stations (BTS), controllers (BSC), PDSNs, other entities. cellular network, interfaces. router. Common Services Layer Each aligned Second generation (2G) investment. third (3G) seamless delivery Core all Air Interfaces existing Consistent wireline evolution. hybrid, multi-standard networks. Proxy benefit from mobility. Improves customer experience minimizing disruption applications when handoff occurs. Intelligent Selection Selects best workload prior sessions. optimal performance. Scales without service. platforms proven some largest world. runs set, rich IP, security, QoS, voice-data integration capability. Routing Configuration Guide Protocols Configuring Release 12.1 No. 1078 Point-to-Point protocol (PPP) Authentication Authorization Accounting (AAA) Virtual Private (VPDN) Remote Dial-In (RADIUS) Security Command Reference Topics PCF Table Flows Session Failure History
PATH=/ciscoview/Routershare/config/CDMA_PDSN_Member_General.htm TITLE=CDMA PDSN Member General TEXT=The CDMA PDSN Member General category of the Device Configuration dialog box allows you to view details packet data switching node members. Procedure Right-click device, then select Monitor. appears. from list. following information appears: (cCdmaClusterTotalControllers) Controllers Count number cluster. within
PATH=/ciscoview/Routershare/config/cdma_pdsn_pcf_service_option_rp_session_upd.htm TITLE=CDMA PDSN PCF and Service Option based RP Session Update TEXT=CDMA PDSN PCF and Service Option-based RP Session Update Right-click the device, and select Configure . from category list. following information appears: IP Address (cCdmaPcfSoRpSessUpdIpAddr) (Packet Data (cCdmaPcfSoRpSessUpdServiceOption) of Control Function) that serves mobile node. packet specifies means between station radio network to establish maintain cdma2000 traffic channels service.
PATH=/ciscoview/Routershare/config/CDMA_PDSN_Service_Option_Table.htm TITLE=CDMA PDSN Service Option Table TEXT=The Service Option Table category of the Device Configuration dialog box allows you to view the service details. Procedure Right-click device, then select Configure double-click device. appears. from list. following information appears: (cCdmaServiceOptionIndex) Rp Session Success (cCdmaServiceOptionSucesses) (cCdmaServiceOptionFailures) (as defined by IOS 4.1. used uniquely index entries table. options 3GPP2 4.1) are: Value Description isdn64k smsRate1 19 loopback13K 12 asyncDataRate2 group3FaxRate2 packetData144k smsRate2 15 18 otapaRate1 otapaRate2 22 packetDataRs1fRs1r 23 packetDataRs1fRs2r 24 packetDataRs2fRs1r 25 packetDataRs2fRs2 32 is2000TestData 33 packetData3G 37 54 is2000Markov 55 is2000Loopback 4103 packetDataRev1 Number times succeeded setting radio (RP) particular failed
PATH=/ciscoview/Routershare/config/cfg00000.htm TITLE=Common Configuration Information TEXT=Card Configuration Port Configuration Chassis Configuration System Software Configuration File Configuration Status History
PATH=/ciscoview/Routershare/config/cfg00001.htm TITLE=CATEGORY TEXT=A pulldown menu that specifies the names of the group of management information. For example, in the configure ports window, may specify physical type, transmission medium protocol used. When you select name, configuration displayed. TTY types (in console and auxiliary ), CiscoView. displays terminal services Asynchronous must before configured they can managed with Card Type CSA Port RS-232 Fast Serial DS1 DS3 SONET Token Ring FDDI Frame Relay X.25 IP Device window)
PATH=/ciscoview/Routershare/config/cfg00002.htm TITLE=Displaying Card Configuration Information TEXT=To display card configuration information, double-click the card . The CiscoView configure card window appears. may vary, depending upon type. fields listed below Hardware typical. (cardIndex) (cardType) Type Description (cardDescr) (cardSerial) (cardSlotNumber) (cardHwVersion) Software (cardSwVersion) Slot For some cards, you can get additional by selecting from CATEGORY pulldown menu. Two examples types with FDDI station management and CSA card. Displays index table. functional text serial number revision level firmware microcode installed relative containing chassis. It -1 if neither applicable nor determinable.
PATH=/ciscoview/Routershare/config/cfg00010.htm TITLE=FDDI Station Management Information TEXT=In addition to the card interface-level information that is common to all cards, the CiscoView configure window displays two configuration fields are exclusive cards: ID (fddimibSMTStationId) 8-octet string uniquely identifies station. Operation (fddimibSMTOpVersionId) Specifies ANSI-defined version of being used operation.
PATH=/ciscoview/Routershare/config/cfg00012.htm TITLE=Displaying CSA Card Configuration Information TEXT=In addition to the card interface-level information that is common to all cards, the CiscoView configure window displays Compression Enabled field, which indicates whether services are disabled.
PATH=/ciscoview/Routershare/config/cfg00013.htm TITLE=Displaying Port Configuration Information TEXT=To display port configuration information, right-click the port, then select Configure from the popup menu. By default, this window displays interface level that defined MIB Interfaces Table. If more available you can name of physical type, transmission medium, protocol CATEGORY pulldown See Also Monitoring Performance
PATH=/ciscoview/Routershare/config/cfg00014.htm TITLE=Typical Interface Configuration Information TEXT=The CiscoView configure port window displays interface information for all router interface types, including Ethernet, Token Ring, FDDI, serial, ATM, high-speed T1, bandwidth E1 ports. Some fields hardware displayed only certain of devices. exact list therefore varies, depending upon type. following many types: (ifIndex) CATEGORY (the pulldown menu) Description (ifDescr) (ifType) Mtu(ifMtu) (ifSpeed) Physical Address (ifPhysAddr) (ifAdminStatus) (ifOperStatus) Operational (ifLastChange) Change Local (ifAlias) unique identifier interface. values ranges between ifNumber. each remains constant least from telephone re-initialization. entity.) network management system protocol, next Presents (for example, product name, manufacturer, version). Specifies defined MIB-II table. ethernet-csmacd indicates CSMA/CD Media Access Control (MAC) by Digital, Intel, Xerox DIX Refer SNMP reference book full types. Maximum transmission unit. size (in octets) largest data that cannot received An estimate current bits second. If measured, nominal used. greater than reported, (4,294,967,295) shown ifHighSpeed speed. Note: sublayer which has concept, zero. applicable, such address, number, Packet Net address. 0-length string. intended state. Possible up, down, testing. Users set value. actual operating hundredths seconds) sysUpTime when entered was before last alias interface, specified manager.
PATH=/ciscoview/Routershare/config/cfg00024.htm TITLE=RS-232 Port Configuration Information TEXT=The RS-232 port configuration dialog box shows the following information for an EIA/TA-232 port: Index Type Input Signals Output (rs232PortInSpeed) Flow Control (rs232PortIndex) Specifies unique values each port. If possible, should map directly connectors. external (rs232PortType) hardware type. (rs232PortInSigNumber) number of detectable (rs232PortOutSigNumber) can assert. speed bits per second. (rs232PortOutSpeed) is using.
PATH=/ciscoview/Routershare/config/cfg00032.htm TITLE=RS-232A Port Configuration Information TEXT=The RS232A port configuration information dialog box shows the following information for an EIA/TA-232A port: (rs232AsyncPortIndex) (rs232AsyncPortBits) per Char Stop (rs232AsyncSTopBits) (rs232AsyncPortParity) (rs232AsyncPortAutoBaud) Baud Specifies rs232PortIndex number of port. bits. character. (rs232AsyncPortSTopBits) Possible values are 1, 1/2, and dynamic. type parity, each none, odd, even, mark, space. Autobaud whether transmission. enabled means that senses input speed, size automatically.
PATH=/ciscoview/Routershare/config/cfg00038.htm TITLE=Fast Serial Port Configuration Information TEXT=The following information is displayed for a fast serial port: Type (locIfFSIPtype) RTS Signal (locIFSIPrts) CTS (locIFSIPcts) DTR (locIFSIPdtr) DCD (locIFSIPdcd) DSR (locIFSIPdsr) Indicates whether line uses (data communications equipment (DCE) terminal (DTE). (locIfFSIPrts) (request to send) up, down. Possible values are down, and not available. (locIfFSIPcts) (clear (locIfFSIPdtr) ready) (locIfFSIPdcd) carrier detect) (locIfFSIPdsr) set field
PATH=/ciscoview/Routershare/config/cfg00045.htm TITLE=Frame Relay Port Configuration Information TEXT=The dialog box displays the frame relay port configuration information for the selected port. Procedure 1. rear view, right-click standard A/S serial noLmiConfigured from pop Circuits(frDlcmiMaxSupportedVCs) menu. double-click appears. 2. Select Circuits Category following appears: Data link connection management information: (frDlcmiState) Address(frDlcmiAddress) Length(frDlcmiAddressLen) Status Enq Msg Intervals (frDlcmiPollingInterval) Max Errs (frDlcmiErrorThreshold) (frDlcmiMulticast) Service Virtual Identifier(frCircuitDlci) (frCircuitCreationTime) Change(frCircuitLastTimeChange) (frCircuitThroughput) identifier Oper (frCircuitState) Last Change (frCircuitCommittedBurst) Bits Uncommitted (frCircuitExcessBurst) (frDlcmiMonitoredEvents) Events This displayed CiscoView window Type of scheme that active, interface. Values are: lmiRev1 ansiT1-617-D ansiT1-617-B Shows address used. Possible follows: Format Meaning q921 13-bit DLCI q922March90 11-bit q922November90 10-bit final length four-octets. two-octets, three-octets, q922, includes control portions. number seconds between successive enquiry messages. value range 255. maximum unanswered inquiries allowed before declared down. 10. Indicates whether uses multicast service. nonBroadcast broadcast. operational state circuit. invalid, inactive. If you set entry deleted. sysUpTime changed. network agrees transferred under normal conditions during measurement interval. attempts polling over which error threshold counted. when was created, by SetRequest. average 'Frame Field' across user one direction, measured configured burst rate throughput both non-zero, (T) equal frCircuitCommittedBurst/frCircuitThroughput. frCircuitExcessBurst/ifSpeed.
PATH=/ciscoview/Routershare/config/cfg00057.htm TITLE=Token Ring Port Configuration Information TEXT=The configure port window displays the following information for a token ring port: Index (dot5IfIndex) Command (dot5Commands) Error Report (dot5RingStatus) Open/Close Result of Last Enter (dot5RingOpenStatus) (dot5RingSpeed) Upstream Neighbor MAC Address (dot5RingUpStream) Specifies ifIndex values from MIB interface. table this Name variable. used request state change. Possible are no-op, open, reset, close. means join ring; leave. Number errors specified port. Provides related entering/leaving ring. Indicates whether attempt was successful, not, shows reason failure. bandwidth 16 Mbps, 4 unknown. read-only neighbor.
PATH=/ciscoview/Routershare/config/cfg00065.htm TITLE=X.25 Port Configuration Information TEXT=Displays the following information for a port configured for X.25: X.25 Operational Status LAPB Status Circuits
PATH=/ciscoview/Routershare/config/cfg00066.htm TITLE=X.25 Operational Status TEXT=The X.25 operations status dialog box shows the parameters for a port configured for X.25. The following information appears: (x25OperInterfaceMode) Mode (x25OperMaxActiveCircuits) (x25OperProtocolVersionSupported) Circuits No (x25OperNumberPVCs) ID(x25OperDataLinkId) Link Protocol Version Identifies DCE/DTE which interface operates. value of dxe indicates role will determined by XID negotiation Layer and that has not yet taken place. Maximum numbers PLE (Packet Level Entity). can support. used channel from 1 this number. instance index object first table most device specific MIB Displays identifier refers packet protocol.
PATH=/ciscoview/Routershare/config/cfg00072.htm TITLE=LAPB Status TEXT=The following LAPB status information is displayed: Oper Station Type (lapbOperStationType) Oper Port OID (lapbOperPortId) (lapbOperProtocolVersionId) Ver (lapbFlowStateChanges) Changes Chg (lapbFlowChangeReason) Displays type. Possible values are DTE, DCE, and DXE. This objects identifies instance of index first group MIB specific physical device interface used. send receive frames. If agent does not support any such obejcets, it should return nullspec OBJECT IDENTIFIER {0 0}. that specifies protocol version being For example, 1.3.6.1.2.10.10.16.5.3 indicates 1984 CCITT number state changes, including resets. reason most recent change.
PATH=/ciscoview/Routershare/config/cfg00078.htm TITLE=Circuits TEXT=The following circuit information is displayed: Channel Number (x25CircuitChannel) Status (x25CircuitStatus) Establish (x25CircuitEstablishTime) (x25CircuitDirection) of (x25CircuitCallParamId) Parameters x25CallParamIndex (x25CircuitCalledDteAddress) (x25CircuitCallingDteAddress) Calling (x25CircuitOriginallyCalledAddress) Description (x25CircuitDescr) Current selected circuit. Specifies values sysUpTime MIB descriptor when was associated with this redirection calls,it that established Possible are incoming, outgoing, and pvc. Instance entry X25CallParamTable which contains user must by Null means PVCs. using default parameters. address. For from indication packet. confirmation will zero length deflected redirected. deflection notification facility request Descriptive string Provides place agent supply any knows about owner may return process identifier name Alternatively, configuration caused bridge has additional information.
PATH=/ciscoview/Routershare/config/cfg00082.htm TITLE=Console, Auxiliary, and TTY Port Configuration Information TEXT=The following configuration and session information is displayed for a console, auxiliary, or TTY port: Active (tsLineActive) (tsLineType) (tsLineAutobaud) Input (tsLineSpeedin) Output (tsLineSpeedout) (tsLineFlow) Controller (tsLineModem) Location (tsLineLoc) Terminal (tsLineTerm) Idle Timeout(secs) (tsLineTmo) Sessions (tsLineUser) (tsLineNses) (TACACS) Name Indicates whether specified line. not. type software which displayed. None following: Unknown Line-printer Virtual-terminal set autobaud detection enables it. adapt rate data being sent Values are: unknown(1), 0 speed running. flow that used can controlled from hardware. value coming device service. provided by Possible Software-input Software-output Software-both Hardware-input Hardware-output Hardware-both Describes physical Interval (in seconds) after connection closed when there traffic during session. Number current Displays Access System username. servers security remote access. using. none(2), call-in(3), call-out(4), cts-required(5), ri-is-cd(6), inout(7)
PATH=/ciscoview/Routershare/config/cfg00094.htm TITLE=Modem Control TEXT=The Modem Control (tsLineModem) field specifies the type of modem control the line is using. Possible values include Unknown None Call-in Call-out Cts-required Ri-is-cd Inout Indicates this dial-in/dial-out uses status DTR to determine whether answers incoming call. dial-out raises check CTS becomes high-speed indicate that host has noticed its signal. form requires while being used. Used lines with modems. high, CD reflect carrier presence, command wired ring input terminal service. configure outgoing calls. enables
PATH=/ciscoview/Routershare/config/cfg00100.htm TITLE=IP Port Address Table TEXT=To access the dialog box: 1. Right-click on the device and Select configure from the popup menu. Device configuration information appears. 2. Category drop-down list box. following appears: (ipAdEntIfIndex) Address(ipAdEntAddr) Subnet Mask(ipAdEntNetMask) Broadcast Format (ipAdEntBcastAddr) Specifies interface. number. 32-bit this entry. mask address. Possible values are all-1s all-0s format.
PATH=/ciscoview/Routershare/config/cfg00104.htm TITLE=Displaying Chassis Configuration Information TEXT=The dialog box displays the chassis configuration information. Procedure 1. Right-click on the Chassis and select Configure from pop up menu. device. appears. 2. Category drop-down list box. following appears: Model (chassisType) ID (chassisId) Hardware (chassisVersion) ROM Monitor (romVersion) System (romSysVersion) Processor (nvRAMsize) (processorRam) Memory (bytes) (nvRAMUsed) (configRegister) type software viewed For example, c4000 indicates Cisco router. unique number. chassis. This contains value, CPU serial (if available); otherwise, empty. 00160917 revision level, string unavailable. version. amount RAM, megabytes, nonvolatile bytes. Specifies use. description decimal, stored register.
PATH=/ciscoview/Routershare/config/cfg00113.htm TITLE=Displaying System Software Information TEXT=Select System Software from the CATEGORY pulldown menu in the CiscoView configure device window to display information. fields might vary according type. following displayed many types: IOS (sysConfigName) Reason Last (whyReload) Displays name boot image file. New versions can be downloaded over network with files. takes effect next time managed reloaded. printable octet string that explains was restarted.
PATH=/ciscoview/Routershare/config/cfg00116.htm TITLE=Displaying Configuration File Information TEXT=In the configure device window, select Configuration File from the CATEGORY pulldown menu to display about router files loaded network. servers. fields might vary, depending upon type. following displayed many types: Boot (netConfigAddr) Filename (netConfigName) Host (hostConfigAddr) (hostConfigName) Displays address of that supplied managed device. contains commands apply all terminal services Network resides IP are specific last used by
PATH=/ciscoview/Routershare/config/cfg00121.htm TITLE=Configuration Status TEXT=The values of Configuration Status objects reflect the status of configuration database. To access the dialog box: 11.1 Right-click devices and select configure from popup menu. information appears. 2. category drop-down list box. following appears: (ccmHistoryRunningLastChanged) (ccmHistoryRunningLastSaved) (ccmHistoryStartupLastChanged) ccmHistoryRunningLastSaved, Startup Maximum (ccmHistoryMaxEventEntries) (ccmHistoryEventEntriesBumped) Bumped This available only that support Cisco IOS Release later. sysUpTime when running was last changed. If greater than has been but not saved. (written). to. In general, default you use cold starting system. It could have by copy elsewhere. number entries can held ccmHistoryEventTable. recommended 10. times oldest entry. deleted make room new
PATH=/ciscoview/Routershare/config/cfg00127.htm TITLE=Configuration History TEXT=The Configuration History is a table of router configuration events, including the following items: Event (ccmHistoryEventTime) Source(ccmHistoryEventCommandSource) Source(ccmHistoryEventConfigSource) (ccmHistoryEventConfigDestination) Type(ccmHistoryEventTerminalType) (ccmHistoryEventTerminalNumber) (ccmHistoryEventTerminalUser) Location(ccmHistoryEventTerminalLocation) Address(ccmHistoryEventCommandSourceAddress) Name(ccmHistoryEventVirtualHostName) Host Address(ccmHistoryEventServerAddress) File(ccmHistoryEventFile) Remote Copy (rcp) User(ccmHistoryEventRcpUser) This category available. only devices that support Cisco IOS Release 11.1 later. value sysUpTime when occurred. source commandLine, initiated event. data for destination If variable terminal type. Otherwise, not applicable. number. -1 name. logged-in user. length 0.0.0.0 hard-wired location incoming connection. virtual, internet address connected system. 'snmp', requester. networkTftp networkRcp, storage file server. zero
PATH=/ciscoview/Routershare/config/cfg00141.htm TITLE=cfg00141 TEXT=Alternatively, do one of the following: Right-click the device. Select Configure from the popup menu.
PATH=/ciscoview/Routershare/config/cfg00142.htm TITLE=cfg00142 TEXT=Alternatively, do one of the following: Right-click the card, then select Configure from the popup menu.
PATH=/ciscoview/Routershare/config/cfg00143.htm TITLE=cfg00143 TEXT=Alternatively, do one of the following: Right-click the port, then select Configure from the dropdown menu.
PATH=/ciscoview/Routershare/config/cfg00146.htm TITLE=Displaying Configuration File Information TEXT=In the configure device window, select Configuration File from the CATEGORY pulldown menu to display about router files loaded network servers. fields might vary, depending upon type. following displayed many types: Boot Address Filename Host
PATH=/ciscoview/Routershare/config/cfg00147.htm TITLE=RSVP Session Table TEXT=RSVP Session Table displays all sessions seen by a system. The table displays the following information: Number (rsvpSessionNumber) (rsvpSessionType) Destination Address (rsvpSessionDestAddr) (rsvpSessionDestAddrLength) (rsvpSessionProtocol) (rsvpSessionPort) (rsvpSessionSenders) (rsvpSessionReceivers) (rsvpSessionRequests) of session. only SNMP Indexing. indicates has not relation any protocol value. For example: IP4, IP6, with flow information. used senders particular this object may changed when RowStatus active. CIDR prefix length address. host 32 and multicast addresses, 128. internet UDP TCP port. specific 50 (ESP) 51 (AH) represents virtual If zero, does have ports. distinct currently known reservations being requested requests sending upstream
PATH=/ciscoview/Routershare/config/cfg00148.htm TITLE=RSVP Sender Information TEXT=Displays the status information displayed by senders in PATH messages. Sender Number (rsvpSenderNumber) Type (rsvpSenderType) Destination Address (rsvpSenderDestAddr) (rsvpSenderAddr) (rsvpSenderDestAddrLength) (rsvpSenderAddrLength) (rsvpSenderProtocol) (rsvpSenderDestPort) (rsvpSenderPort) (rsvpSenderFlowId) CIDR (rsvpSenderPolicy) (rsvpSenderStatus) (rsvpSenderTTL) of specified sender. This value. used SNMP Indexing only and has not relation any protocol session. could IP4, IP6, with flow information. installing object, may changed when RowStatus active. Source prefix length bits. hosts multicast addresses 32. sender's Indicates internet Value UDP TCP port. If use, rsvpSenderProtocol, 50 (ESP) 51 (AH), represents virtual number. zero, does have using Ipv6 Contents policy uninterrupted string octets, including header. present. Active deleting last received
PATH=/ciscoview/Routershare/config/cfg00149.htm TITLE=RSVP TSpec Information TEXT=The table displays following information: Average Bit Rate (rsvpSenderTSpecRate) Peak Bit Rate (rsvpSenderTSpecPeakRate) Burst Size (rsvpSenderTSpecBurst) Minimum Messages (rsvpSenderTSpecMinTU) Maximum (rsvpSenderTSpecMaxTU) Refresh (rsvpSenderInterval) (rsvpSenderRSVPHop) (rsvpSenderLastChange) Change (units: bits, per second) of sender's data stream. Within transmission burst, arrival could between fast (if supported by service model); however, averaged across network. more intervals, should not exceed rsvpSenderTSpecRate. Traffic expected to this any time, apart from effects jitter If specified TSpec, returns zero noSuchValue. largest one time. flow. smaller than are considered messages. Admission algorithm rejects Tspecs with interface (MTU) greater sum and headers. advertised previous hop. Indicates whether Possible values True False. Description IP Time last PATH message. also means first was received most recent parameter change.
PATH=/ciscoview/Routershare/config/cfg00150.htm TITLE=RSVP ADSPEC Information TEXT=The table displays following information: rsvpSenderAdspecBreak Hop Count Path Bandwidth Minimum Path Latency Maximum Transmission Unit (rsvpSenderAdspecGuaranteedBreak) Service (rsvpSenderAdspecGuaranteedCtot) (rsvpSenderAdspecGuaranteedDtot)(units:microseconds) rsvpSenderAdspecguaranteedCsum rsvpSenderAdspecGuaranteedDsum) MTU Controlled (rsvpSenderAdspecCtrlLoadBreak) (rsvpSenderAdspecBreak) Indicates global 'break' (units:bits general characterization parameter. from ADSPEC. Possible values are True. False. nosuchValue, Description At least one non-IS was detected. path. No hops were (rsvpSenderAdspecHopCount) If zero nosuchvalue, invalid set. not present. (rsvpSenderAdspecPathBw) (units:bytes) per second) estimated (rsvpSenderAdspecMinLatency) microseconds) (rsvpSenderAdspecMtu) bytes) composed (rsvpSenderAdspecGuaranteedSvc) presence of fragment. contains does whether that more nodes along supports service. false, True, noSuchValue. displayed. end-to-end this 'c' returns since last reshaping point. rsvpSenderAdspecGuaranteedSve (rsvpSenderAdspecGuaranteedHopCount) service-specific override (rsvpSenderAdspecGuaranteedPathBw) (rsvpSenderAdspecGuaranteedMinLatency) (rsvpSenderAdspecGuaranteedMtu) (rsvpSenderAdspecCtrlLoadSvc) controlled-load any set, (rsvpSenderAdspecCtrlLoadHopCount) services-specific Contolled (rsvpSenderAdspecCtrlLoadPathBw) (rsvpSenderAdspecCtrlLoadMinLatency) status (rsvpSenderAdspecCtrlLoadMtu)
PATH=/ciscoview/Routershare/config/cfg00151.htm TITLE=RSVP Outgoing Interfaces Table TEXT=Displays information on Interface Status. Interface Status Interface Status (rsvpSenderOutInterfaceStatus) Indicates the of interface. active all PATH messages.
PATH=/ciscoview/Routershare/config/cfg00152.htm TITLE=RSVP RESV Message Table TEXT=Displays the information describing the state information displayed by receivers in RESV messages. Reservation Request (rsvpResvNumber) Session (rsvpResvType) Destination Address (rsvpResvSenderAddr) (rsvpResvDestAddrLength) (rsvpResvProtocol) (rsvpResvDestPort) Source QOS (rsvpResvService) RowStatus Time Live (rsvpResvFlowId) CIDR Indicates number. of request. This SNMP indexing only and has not relation any value. type session, example IP4, IP6, with information. (rsvpResvDestAddr) used 'all senders'. session. may changed when active. sender's selected reservation. zeroes prefix length address. host multicast 32. object (rsvpResvSenderAddrLength) addresses. UDP TCP ports. If use, specified rsvpResvProtocol, 50(ESP) (ESP) 51 (AH), represents virtual desination Zero that protocol does have (rsvpResvPort) generalized identifier (GPI). classification requested receiver. (rsvpResvStatus) status install static delete (rsvpResvTTL) last received header. flow using Ipv6
PATH=/ciscoview/Routershare/config/cfg00153.htm TITLE=RSVP Resv TSpec and RSpec Information TEXT=The table displays the following information: Average Bit Rate Peak Bit Rate Burst Size Minimum Message Maximum Clearing Delay (rsvpResvRSpecSlack)(units: Refresh (rsvpResvInterval) (rsvpResvScope) (rsvpResvShared) Reservation (rsvpResvExplicit) Senders hop. (rsvpResvLastChange) Change (rsvpResvPolicy) (rsvpResvTSpecRate)(units: bits per second) Indicates of sender's data stream. Within transmission burst, arrival could beyond fast rsvpResvTSpecPeakRate. Averaged across network more intervals, should not exceed rsvpResvTSpecRate. (rsvpResvTSpecPeakRate) Traffic expected to this any time, except effects jitter If specified Tspec, zero noSuchValue displayed. (rsvpResvTSpecBurst) largest from time. lesser than advertised size, receiver asking provided flow. pacing what would under normal circumstances. (rsvpResvTSpecMinTU) Messages with considered messages. (rsvpResvTSpecMaxTU) admission algorithm will reject TSpecs whose unit, plus interface headers, MTU. (rsvpResvRSpecRate)(units: requested. rate. that service available. microseconds) slack, guaranteed. between messages, by Next Hop. Specifies contents scope object including header. uninterrupted string octects. series IP4 IP6 addresses value present. whether shared specifications. user. Description True among False how selected. request. Individual listed filter All implicitly (rsvpResvRSVPHop) previous last mean first was received most recent parameter change. policy
PATH=/ciscoview/Routershare/config/cfg00154.htm TITLE=RSVP Resv Forward Table TEXT=Specifies the state of information displayed upstream in RESV messages. Table displays the following information: Session (rsvpResvFwdNumber) (rsvpResvFwdType) Destination Address (rsvpResvFwdSenderAddr) (rsvpResvFwdDestAddrLength) (rsvpResvFwdProtocol) (rsvpResvFwdDestPort) QoS (rsvpResvFwdService) RowStatus Time Live (rsvpResvFwdFlowId) ID number. reservation. request. Note: This SNMP indexing only and has not relation any value. type (IP4, IP6, etc.). (rsvpResvFwdDestAddr) Indicates used by all senders. session. should changed when active. source selected zeroes may length bits. (rsvpResvFwdSenderAddrLength) Inidicates sender's protocol secure sessions security. UDP TCP ports. specified If use, rsvpResvFwdProtocol, 50 (ESP) 51 (AH), represents virtual zero, does have object (rsvpResvFwdPort) generalized identifier (GPI). service Classification requested. (rsvpResvFwdStatus) status delete information. (rsvpResvFwdTTL) last received header. flow receiver IPv6
PATH=/ciscoview/Routershare/config/cfg00155.htm TITLE=RSVP Resv Forward TSpec and RSpec Information TEXT=The table provides the following information: Average Bit Rate Peak Bit Rate Burst Size Minimum Message Maximum Clearing Delay (rsvpResvFwdRSpecSlack)(units: Refresh (rsvpResvFwdInterval) (rsvpResvFwdScope) (rsvpResvFwdShared) Reservation (rsvpResvFwdExplicit) Senders hop. (rsvpResvFwdLastChange) Change (rsvpResvFwdPolicy) (rsvpResvFwdTSpecRate)(units: bits per second) Specifies of sender's data stream. Within transmission burst, arrival could beyond fast rsvpResvFwdTSpecPeakRate. However, averaged across network's more intervals, should not exceeds rsvpResvFwdTSpecRate. (rsvpResvFwdTSpecPeakRate)(units: Indicates This traffic expected any time, except effects jitter. If value zero noSuchValue, specified TSpec. (rsvpResvFwdTSpecBurst largest from one time. less than advertised size, receiver asking to flow. pacing what would provided under normal circumstances. option. (rsvpResvFwdTSpecMinTU) Maximun (rsvpResvFwdTSpecMaxTU) admission algorithm rejects TSpecs whose unit, plus interface headers, MTU. (rsvpResvFwdRSpecRate)(units: bytes requested. when service guaranteed. microseconds) slack between messages Previous Hop. contents scope object including header. present. status Description True shared among False specifications. how selected. Individual listed using filter All implicitly retains that need purpose routing message. (rsvpResvFwdRSVPHop) type next IP may last request. first was most recent parameter change. policy
PATH=/ciscoview/Routershare/config/cfg00156.htm TITLE=RSVP Specific Attributes TEXT=The table displays the following information: UDP neighbors IP neighbors Total neighbors RSVP Enable Encapsulation Value Kb Time to Live (rsvpIfRefreshBlockadeMultiple Message (rsvpIfRefershInterval (rsvpIfUdpNbrs (rsvpIfTTL) Indicates number of perceived using only encapsulation. (rsvpIfIpNbrs (rsvpIfNbrs currently any kind will exceed + by both encapsulations. (rsvpIfEnabled Inidcates status. interface. Description True enabled False not (rsvpIfUdpRequired Manual configuration forces uses used zero. minimum refreshed intervals that blockade state last once (units: entered. (rsvpIfRefreshMultiple must elapse before PATH RESV being aged out SEND_TTL node originates. set zero, determines TTL. milliseconds) period between transmission given
PATH=/ciscoview/Routershare/config/cfg00157.htm TITLE=RSVP Neighbor Table TEXT=The table displays the following details: Neighbor Address (rsvpNbrAddress) Neighbor Protocol (rsvpNbrProtocol) Status (rsvpNbrStatus) IP4 IP6 used by neighbor. This object may not be changed when RowStatus active. encapsulation neigbor. of neighbors. Active for all configuring In presence configured. neighbors, implementation might limit set valid those already
PATH=/ciscoview/Routershare/config/cfg00158.htm TITLE=GGSN and SGSN Configuration Parameters TEXT=GGSN Configuration Parameters The table displays following information: T3-Tunnel Timer (cgprsGtpT3TunnelTimer) T3-Response (cgprsGtpT3ResponseTimer) N3-Requests (cgprsGtpN3Request) N3-Buffer-Size (cgprsGtpN3BufferSize) (cgprsGtpEchoRequestTimer) (cgprsGtpGSNTotalBandwidthResrc) Resource (cgprsGtpMaxNumPDPCxts) Contexts Monitor Duration (cgprsGtpDroppedPktsMonTime) GTP Failed Trap (cgprsGtpNoRespToEchoNotifEnable) Charging cgprsGtpPDPCxtActivationRejNotif. Rejection (cgprsGtpPDPCxtActRejNotifEnable) (units: seconds) mobility management. started bytes, old SGSN. When running, T-PDUs received. any buffered are forwarded new response back-off retransmission. signalling cgprsGtpN3requests transmitted, GGSN. used messaged normally times expires. total wait must between shorter than mobile system. Retries Attach RA updates. product less minimum values, (T3310) Routing Area (T3330). recommends adaptive mechanism, using increasing example, 1,2,4, 8 seconds. Indicates maximum number retransmitted corresponding size, G-PDUs messages. If packets exceed capacity, excessive discarded. message. An echo there request, notification. identifies peer that fails respond. bandwidth allowed. context contains session mangement necessary transfer SGSNs Inter procedure. time, seconds, monitoring generates which dropped because unknown header problem. whether failure false prevents CGPRS from being generated produces this
PATH=/ciscoview/Routershare/config/cfg00159.htm TITLE=GGSN Configuration Parameters TEXT=Dialog box displays following information: APN Address Allocation Method APN Address Allocation Method (cgprsGtpAPNAddrAllocMethodGlobDef) Indicates the global default value. of method. individual overrides
PATH=/ciscoview/Routershare/config/cfg00160.htm TITLE=Charging Gateway Table for GGSN TEXT=The table displays the following information: IP Address (cgprsGtpChargingGWid) Name (cgprsGtpChargingGWName) Type (cgprsGtpChargingGWType) Operation (cgprsGtpChargingGWOperState) Up-Down Trap (cgprsGtpChargingGWNotifEnable) (cgprsGtpChargingGWRowStatus) Status Specifies being used. by unique gateway. Indicates of value can set to 'primary'. and one backup are default operating state Description up. down. Unknown not determined, example, from time actual detected as functional. whether system produces cgprsGtpCharginGWNotif. row. considered create delete table.
PATH=/ciscoview/Routershare/config/cfg00161.htm TITLE=APN Table for GGSN TEXT=The table displays the following information: APN Id (cgprsGtpAPNId) APN Name (cgprsGtpAPNName) Address Allocation (cgprsGtpAPNAddrAllocMethod) (cgprsGtpAPNRowStatus) Status Indicates index. name. Specifies method. default to use global setting. of row. value considered create delete table.
PATH=/ciscoview/Routershare/config/cfg00163.htm TITLE=GSN Table for GGSN and SGSN TEXT=GSN Table for GGSN The table displays the following information: GSN Node IpAddress (cgprsGtpGSNid) Echo Test Failure Count (cgprsGtpGSNEchoFailedNotifCnt) unique IP address of node. before entry deleted.
PATH=/ciscoview/Routershare/config/cfg00165.htm TITLE=IP Address table for GGSN TEXT=The table displays following information: APN IpAddresses (cgprsGtpNumAllocIpAddr) APN IpAddresses (cgprsGtpNumAllocIpAddr) Indicates allocated number of dynamic addresses, associated with an APN.
PATH=/ciscoview/Routershare/config/cfg00166.htm TITLE=GTP Status Information for GGSN TEXT=The table displays the following information: GTP Version (cgprsGtpVersion) Last Non responding Peer (cgprsGtpLastGSNidNoRespToEcho) (cgprsGtpLastGSNidRecovered) Unexpected (cgprsGtpGSNidOfLastUnexpPDPCxt) Context (cgprsGtpTIDOfLastUnexpPDPCxt) Rejection (cgprsGtpRejReasonOfLastUnexpPDPCxt) Indicates supported by device. Specifies that did not reply to an echo message. whose unexpected. of activation. reason rejecting
PATH=/ciscoview/Routershare/config/cfg00167.htm TITLE=IMA Group Configuration Table TEXT=The table displays the following information: Group Index (imaGroupIndex) Row Status (imaGroupRowStatus) Interface (imaGroupIfIndex) (imaGroupMinNumTxLinks) (imaGroupMinNumRxLinks) (imaGroupRxImaId) Near-End ImaID (imaGroupTxImaId) Far-End (imaGroupSymmetry) (imaGroupTxFrameLength) (imaGroupRxFrameLength) Transmission Clocking (imaGroupNeTxclkmode) (imaGroupFeTxclkmode) (imaGroupLastChange) Change (imaGroupAlphaValue) (imagGroupBetaValue) (imaGroupBetaValue) (imaGroupGammaValue) Indicates unique value time-of-day group. imaGroupTable entries. allows create, change, and delete operations logical number assigned to used identify corresponding rows MIB. Note: Re-initialization management agent may cause client's change. minimum transmit links required active operational. received by function. symmetry length frame direction. can set only when startup. from clock last changed state. alpha that specifies consecutive invalid ICP cells detected before moving HUNT SYNC beta erred gamma
PATH=/ciscoview/Routershare/config/cfg00168.htm TITLE=IMA Link Configuration Table TEXT=The table displays the following information: Interface Index Row Status Group Index Near End Transmission State Reception Far (imaLinkNeRxState) (imaLinkNeRxFailureStatus) Id Relative (imaLinkRelDelay) (imaLinkTestProcStatus) (imaLinkTimeElapsed) Elapsed (imaLinkIfIndex) Indicates logical number assigned to link. (imaLinkRowStatus) of table. (imaLinkGroupIndex) (imaGroupIndex) which this member. (imaLinkNeTxState) near-end transmit receive (imaLinkFeTxState) far-end reported through ICP cells. (imaLinkFeRxState) current failure (imaLinkFeRxFailureStatus) (imaLinkTxLid) outgoing used by local end. valid, only when belongs group. (imaLinkRxLid) incoming remote via latest measured delay. with least For both links should same pattern procedure. Value Description Disabled (1) not running. Operating. (2) and error has been found interface. LinkFail (3) An detected during test. After occurs, latched, until object read, imaGroupTestProcStatus moved disabled. if longer persists, subsequent will reports Elasped time since beginning measurement period seconds.
PATH=/ciscoview/Routershare/config/cfg00169.htm TITLE=Rate Limit Configuration TEXT=Dialog box displays following information: Data Source (ccarConfigDirection) Type (ccarConfigType) Access List Index(ccarConfigAccIdx) (ccarConfigAccIdx) Comitted Rate(ccarConfigRate) (ccarConfigLimit) Extended Limit(ccarConfigExtLimit) Action(ccarConfigConformAction) Action(ccarConfigExceedAction) Exceed Source(ccarConfigDirection) The object. Type(ccarConfigType) of traffic, rate-limited against. index to if either quick standard access. Committed rate. This sustained permitted bytes, limit. amount excess rate, which will be instantaneously burst limit, may conditionally probability that not increases. received taken when within exceeds
PATH=/ciscoview/Routershare/config/cfg00170.htm TITLE=Queues on Cisco Interface TEXT=The Queues on a Cisco Interface dialog box displays the following details: Type Maximum Number of messages No sub-Queues (cQIfQType) queuing used. Hold Queue. First Out Queuing, Priority Custom Weighted Fair implies that always transmits order they hardware received. sorts by access lists. higher sub-queue get preference over lower selected round robin as either drained given octets moved from subqueue transmission 'conversation', which source-destination pair addresses and sockets ports, defined network layer protocol. (cQIfTxLimit) placed into This come serve queue, fed (cQIfSubqueues) built. constant for each value cQIfQType.
PATH=/ciscoview/Routershare/config/cfg00171.htm TITLE=SubQueues Statistics Table TEXT=Sub-Queues Statistics Table The Sub Queue Statistics Table provides the following information: Queue Number of sub-queue. messages Maximum Discarded Messages (cQStatsQNumber) within set. In FIFO queuing, this value always 2. Priority corresponds Custom various priorities. high = 0, medium 1, normal 2, 3. referenced access list. Weighted Fair associated traffic stream (conversation) that gets identified. (cQStatsDepth) indicates (cQStatsMaxDepth) permitted (cQStatsDiscards) from since restart by reason enqueue time > cQStatsMaxDepth.
PATH=/ciscoview/Routershare/config/cfg00172.htm TITLE=Custom Queue Rotation Table TEXT=The table displays following information: Transmitted Octets (cQRotationOctets) Transmitted Octets (cQRotationOctets) Number of that may from queuing sub-queue before yielded another queue.
PATH=/ciscoview/Routershare/config/cfg00173.htm TITLE=IP Precedence Table TEXT=The IP Precedence Table displays the following information: Data Source (cipPrecedenceDirection) IP (cipPrecedenceIpPrecedence) Source(cipPrecedenceDirection) object. Precedence(cipPrecedenceIpPrecedence) value collected upon.
PATH=/ciscoview/Routershare/config/cfg00174.htm TITLE=IP MAC Table TEXT=The IP MAC Table displays the following information: Data Source (cipMacDirection) MAC Address (cipMacAddress) object. address.
PATH=/ciscoview/Routershare/config/cfg00175.htm TITLE=CDMA PDSN System Information TEXT=Use this option to view PDSN system information. Procedure To access CDMA PDSN system information: Right-click the device and select Configure from popup menu. dialog box appears. Category list. following appears: (cCdmaSessionMaxAllowed) Number of Sessions (PCF) (cCdmaPcfMaxAllowed) (cCdmaServingPdsnHostname) Name (cCdmaSystemVersion) Authentication (cCdmaSessionPdsnAuthenTimer) Notification (cCdmaSessionMaxNotifEnabled) (cCdmaPcfMaxAllowedNotifEnabled) Invalid Registration (cCdmaRegReqFailedNotifEnabled) (cCdmaSystemStatus) (cCdmaSessionHighThreshold) (cCdmaSessionLowThreshold) Low Redundancy (cCdmaSrEnabled) Maximum allowed by subsystem. applicable member peer-peer. Displays zero node limitation sessions. packet controller, functions serving Data Node (PDSN). host CISCO switching release. version, example output: 1.1. Mobile (MoIP) users notification. using PPP authentication. timer Indicates whether send when reached. max Values are: true, failure. false. Do Default interconnected sent manager terminates because request Enabling Operational status agent generates threshold during call setup. Minimum feature enabled.
PATH=/ciscoview/Routershare/config/cfg00176.htm TITLE=CDMA PDSN PCF Table TEXT=Procedure Right-click the device, then select Configure or double-click the device. The Device Configuration dialog box appears. from Category list. following information appears: (cCdmaPcfIpAddress) IP address identifying Packet Control Function (PCF).
PATH=/ciscoview/Routershare/config/cfg00177.htm TITLE=CDMA PDSN Session Table TEXT=The table displays following information: Mobile Station ID (cCdmaSessionMsid) MSID Type (cCdmaSessionMsidType) Electronic Serial Number (cCdmaSessionEsn) Serving FAIpAddress (cCdmaSessionPdsnIp) FA (cCdmaSessionFaIp) MoIP HA (cCdmaSessionA11HaIp) (cCdmaSessionA11FaIp) (cCdmaSessionKey) Connection (cCdmaSessionConnId) (cCdmaSessionMoMtInd) Indicator PPP (cCdmaSessionPppCompressEnabled) (cCdmaSessionVJCompressEnabled) VJ (cCdmaSessionServiceOption) Option (cCdmaSessionConnStartTime) Time Identifier station. Format of ID. 'imsi' IMSI 15 digits max.) 'min' MIN 10 'irm' IRM other formats. address packet data node. as foreign agent home interface. identification key used. by IP/GRE protocol. sesssion. Consists four octets locally unique within session. originated/Mobile terminated indicator. Values area: (1) mobileOriginated(2) initiated mobileTerminated (3) Node intitiated compression status. are: true enabled. false not Van-Jacobson TCP/IP header. fales service and rate set starting date time, provided RAN. only propogates this information.
PATH=/ciscoview/Routershare/config/cfg00178.htm TITLE=CDMA PDSN IP Flows Table TEXT=The table displays following information: IpAddress (cCdmaSessionUserFlowIpAddress) N/W Access ID (cCdmaSessionNai) Addressing Scheme(cCdmaSessionAddressingScheme) Technology(cCdmaSessionFlowTechnology) HA IpAddress(cCdmaSessionHaIpAddress) Tunneling Protocol(cCdmaSessionTunnelProt) (cCdmaSessionTunnelProt) IpAddress(cCdmaSessionUserFlowIpAddress) flow. address. ID(cCdmaSessionNai) User's network identifier. User@domain construct, which identifies home of proxymobileIP user. station type. Values are: other (1) static (2) has configured. dynamically (3) assigned Relevant Routing technology used. by simpleIP routing. Mobile (4) MoIP with acting MC. agent Note: only Proxy protocol. between and packet data serving node. notunnel encapsulation. 12tp using 12f mobileip (5) GRE
PATH=/ciscoview/Routershare/config/cfg00179.htm TITLE=CDMA Mobile User Failure Information TEXT=The dialog box displays the following information: Index (cCdmaFailSessionIndex) MS Identifier (cCdmaFailSessionMsid) MSID Type(cCdmaFailSessionMsidType) Electronic Station Number(cCdmaFailSessionEsn) (cCdmaFailSessionEsn) HA IpAddress(cCdmaFailSessionA11HaIp) (cCdmaFailSessionA11HaIp) FA IpAddress(cCdmaFailSessionA11FaIp) Connection ID(cCdmaFailSessionConnId) Key(cCdmaFailSessionKey) Date & Time(cCdmaFailHistFailTime) Type(cCdmaFailHistFailType) Index(cCdmaFailSessionIndex) An arbitrary integer monotonically uniquely identify entry. Increases and pppAuthenticationFailure wrap zero. Identifier(cCdmaFailSessionMsid) of failed session. type number mobileIPAuthenticaitonFailure home agent address interface foreign GRE identification key time failure. current record. Possible values are: Other (1) (2) (3) mobileIPRegistrationTimeout (4) a10a11SessionTimeout (5) maxAllowedSessionReached (6) maxAllowedPcfReached (7) sessionFormatError (8)
PATH=/ciscoview/Routershare/config/cfg00180.htm TITLE=MIP(Mobile IP) System Group TEXT=The dialog box displays the following information: MoIP Entities (mipEntities) Enable MoIP (mipEnable) Encapsulation Method (mipEncapsulationSupported) supported by managed entity. Possible values are: mobileNode (0) foreignAgent (1) homeAgent (2) Note: may more than one For example, supports and Therefore, bit set protocol 1. Indicates whether should be enabled disabled, If both agent discovery registration functions. methods ipInIp within IP. gre Generic routing encapsulation. minEnc Minimal other (3) Other.
PATH=/ciscoview/Routershare/config/cfg00181.htm TITLE=MIP Security Associations table TEXT=The table displays the following information: Peer Entity's IpAddress (mipSecPeerAddress) Security Parameter Index(mipSecSPI) (mipSecAlgorithmType) (mipSecAlgorithmMode) Replay-Protection (mipSecReplayMethod) address of entity within which node shares mobility association. 4-byte opaque index selects specific parameters to be used authenticate peer. algorithm. Possible values are: other (1) md5 (2) mode prefixSuffix method supported this
PATH=/ciscoview/Routershare/config/cfg00182.htm TITLE=MIP Security Violations TEXT=The dialog box displays the following information: Total Number of Security Violations (mipSecTotalViolations) entity.
PATH=/ciscoview/Routershare/config/cfg00183.htm TITLE=MIP Security Violations Table TEXT=The table displays the following information: Violator's IpAddress (mipSecViolatorAddress) Security Count (mipSecViolationCounter) Latest Violation's (mipSecRecentViolationSPI) Time(mipSecRecentViolationTime (4) LSBs(mipSecRecentViolationIDLow MSBs (mipSecRecentViolationIDHigh) (mipSecRecentViolationReason) address. Total number offending peer. most recent violation If due an identification mismatch, Authentication this from Mobile-Home Extension. invalid authenticator, In all other cases, values set zero. Low-order 32 bits used request reply High-order Possible are: noMobilitySecurityAssociation (1) badAuthenticator (2) badIdentifier (3) badSPI missingSecurityExtension (5) (6)
PATH=/ciscoview/Routershare/config/cfg00184.htm TITLE=Mobility Agent Advertisement Table TEXT=The table displays the following information: Source IpAddress (maInterfaceAddress) Max Registration Lifetime (maAdvMaxRegLifetime) (maAdvPrefixLengthInclusion) Extension Destination (maAdvAddress) (maAdvMaxInterval) Interval(maAdvMinInterval) (maAdvMaxAdvLifetime) (maAdvResponseSolicitationOnly) Solicitation Row Status(maAdvStatus) IP adddress interface. longest lifetime, seconds, that willing to accept any Request. Indicates whether advertisements send over includes Prefix-Lengths extension. Possible values are: true All false advertisemens need not extensions. address between used sent from only permissible all-systems multicast (224.0.0.1) limited-broadcast (255.255.255.255) Maximum interval, successive transmissions of Minimum Time, placed field RFC 1256-portion should response message. satus table. If column status 'active', manager change row.
PATH=/ciscoview/Routershare/config/cfg00185.htm TITLE=Foreign Agent System Table TEXT=The table displays the following information: Care of Address (faSupportedCOA) Row Status (faCOAStatus) Care-of-Address supported by agent. entry.
PATH=/ciscoview/Routershare/config/cfg00186.htm TITLE=Foreign Agent Advertisement Group TEXT=The dialog box displays the following information: FA Busy (faIsBusy) Registration Required (faRegistrationRequired) Indicates whether to accept additional registrations. Possible values are: true (1) busy. Any advertisements send from this should have 'B' bit set 1. false (2) not Required(faRegistrationRequired) requires even mobile nodes that acquired their own colocated care-of-address. and 'R' required.
PATH=/ciscoview/Routershare/config/cfg00187.htm TITLE=Foreign Agent Visitors Table TEXT=The table displays the following information: Visitor IP Address (faVisitorIPAddress) Visitor Home Address (faVisitorHomeAddress HA (faVisitorHomeAgentAddress) Total LifeTime of Registration (faVisitorTimeGranted) (faVisitorTimeRemaining) (faVisitorRegFlags) 4 LSBs ID(faVisitorRegIDLow) MSBs (faVisitorRegIDHigh) (faVisitorRegIsAccepted) Source Visitor's request. visiting mobile node. lifetime, seconds, granted registration. Note: Valid only true (1). Seconds remaining until expired. Initial values same as faVisitorTimeGranted, and counted down by agent. flags send nodes. 32 bits Identification used Indicates whether accepted. Possible are: false (2) still pending reply.
PATH=/ciscoview/Routershare/config/cfg00188.htm TITLE=Home agent mobility Table TEXT=The table displays the following information: MN IpAddress (haMobilityBindingMN) MN Care of Address (haMobilityBindingCOA) (haMobilityBindingSourceAddress) Registration (haMobilityBindingRegFlags) 4 LSBs Identifier (haMobilityBindingRegIDLow MSBs (haMobilityBindingRegIDHigh) Total Lifetime, (haMobilityBindingTimeGranted), (haMobilityBindingTimeRemaining) IP mobile node. node's care-of-address. One can have multiple bindings with different care-of-addresses. request has received by agent. This either co-located foreign flags send 32 bits identification used seconds, granted to registration. Seconds remaining until expires. It same intial value and counted down
PATH=/ciscoview/Routershare/config/cfg00189.htm TITLE=Home Agent Registration Table TEXT=The table displays the following information: Latest Regn Accepted Time (haRecentServiceAcceptedTime) denied (haRecentServiceDeniedTime) (haRecentServiceDeniedCode) which most recent request was by mobile node. indicating reasonUnspecified(128) rejection of agent. Possible values are: admProhibited(129) insufficientResource(130) mnAuthenticationFailure(131) faAuthenticationFailure(132) idMismatch(133) poorlyFormedRequest(134) tooManyBindings(135) unknownHA(136)
PATH=/ciscoview/Routershare/config/cfg00190.htm TITLE=APN Table for GGSN TEXT=The table displays following information: APN Index (cgprsGtpAPNId) APN Name (cgprsGtpAPNName) APN Address Alloction (cgprsGtpAPNAddrAllocMethod) (cgprsGtpAPNRowStatus Status Index. name. IP allocation method. radius (1) dhcp (2) disable (3) notconfig (4) Default global setting. status. object used to create new row, and delete modify existing table.
PATH=/ciscoview/Routershare/config/cfg00191.htm TITLE=SRP MAC Info TEXT=rmation Use this option to view generic information about specific spatial reuse protocol (SRP) interface. Procedure access information: Double-click right-click either supports and select Configure from pop-up menu. Category displays: configuration information. dialog box (srpMACAddress) (srpPriorityThreshold) Threshold Values Number of (srpNodesOnTheRing) (IPS) (srpIpsState) (srpIpsLockedOut) Wrapped Timer(srpIpsWaitToRestoreTimer) (srpIfTimeElapsed) (srpIfValidIntervals) Interval Related Topics Using CiscoView Interface Main Menu Selecting Components Configuring Devices Monitoring Hardware address. compared within high-priority packet header. greater than equal value, placed transmit transit queue. unless low-priority nodes. ring. Zero means unavailable. Intelligent protection-switch switching. status. are: Idle (1) ready perform It sends messages. itself; source field neighboring PassThrough. (2) participates by passing wrapped traffic long path signaling through based received (3) wrap; request issued locally When unavailable, True disabled. does not side False enabled. Time, seconds, remain state after cause removed. timer prevents oscillations. Default 60. elapsed since beginning current measurement interval. exceeds maximum displayed. 15-minute; intervals which data was collected. Minimum 4; 96. 32. < > (re-)started last *15) minutes.
PATH=/ciscoview/Routershare/config/cfg00192.htm TITLE=SRP Interface Sides TEXT=Use this option to view information about a particular side of spatial reuse protocol (SRP) interface. Procedure Double-click right-click whether port and select Configure from popup menu. Category displays: configuration side. dialog box (srpMACInterfaceSide) (srpMACNeighborAddress) Neighbor (srpMACSideWrapped) State IPS (srpMACIpsMgmtRequestedMode) noRequest Currently Detected (srpMACIpsAutoDetectMode) Received (srpMACIpsRemoteMode) (srpMACIpsRemoteType) (srpMACIpsActiveMode) Unwrap Tranisitions (srpMACIpsWrapCounter) (srpMACIpsLastWrapTimeStamp) (srpMACIpsLastUnWrapTimeStamp) (srpMACClockSourceMode) Source (srpMACTopologyTimer) Discovery Timer Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring containing information. address. Node wrapped state. Values are: True (1) False (2) not mode. requested by management local that can affect node. manualSwitch forcedSwitch automatically signalFail signalDegrade waitToRestore messages ring, which Shows object value belongs nonadjacent ShortPath LongPath active changes due in: Number transitions sysUpTime. clock Internal internal. Used when connecting two routers dark fiber WDM system. Line source. SONET/SDH ADM. ring. frequency topology sent around identify nodes. always Default 10 seconds. You set 600
PATH=/ciscoview/Routershare/config/cfg00193.htm TITLE=SRP Ring Topology Table TEXT=Use this option to view specific information about a particular node on SRP ring. Procedure To access information: Double-click right-click another reported and select Configure from pop-up menu. Category displays: configuration information. dialog box (srpNodeHopsNumber) LocalNode (srpNodeMACAddress) Address (srpNodeWrapped) State (srpNodeName) Related Topics Using CiscoView Interface Main Menu Selecting Components Configuring Devices Monitoring of hops local counted clockwise. Value between 0 (srpNodesOnTheRing 1). node. Shows whether wrapped. Displays name by SRP. Blank unknown.
PATH=/ciscoview/Routershare/config/cfg00194.htm TITLE=SRP Configure Source TEXT=Use this option to view packet count and number of packets rejected for a source address on a particular interface. Procedure access information: Right-click there port select Interface Statistics from pop-up menu. (srpMACCountPktsBySourceFlag) Layer Traffic dialog box appears. Category displays: information. Accept (srpMACCountPktsBySourceAddress) Last Change (srpMACSourceDiscontTimeStamp) (srpMACRejectPktsBySourceFlag) (srpMACRejectPktsBySourceAddress) Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring Shows that are counted address. which when corresponding instances true. sysUpTime srpMACCountPktsBySourceAddress.
PATH=/ciscoview/Routershare/config/cfg00195.htm TITLE=SRP Configure Destination TEXT=Use this option to view packet count and number of packets rejected for a destination address on a particular interface. Procedure access information: Right-click there port select Interface Statistics from pop-up menu. (srpMACCountPktsByDestinationFlag) Layer Traffic dialog box appears. Category displays: information. Send (srpMACCountPktsByDestAddress) Last Change (srpMACDestDiscontTimeStamp) (srpMACRejectPktsByDestFlag) (srpMACRejectPktsByDestAddress) Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring Shows that are counted address. which when corresponding instances true. sysUpTime was either srpMACCountPktsByDestFlag.
PATH=/ciscoview/Routershare/config/cfg00196.htm TITLE=Error Statistics TEXT=SRP Error Statistics - History Use this option to monitor error statistics of an interface side with specific interval. number. Procedure access information: N-1. Right-click the and select Configure from popup menu. Port dialog box appears. 2. Category displays: (srpErrCntIntInterfaceSide) (srpErrCntIntNumber) view that particular Related Topics Physical Layer Errors Higher containing row information. A between 96, which identifies available statistics. means most recent completed 15 minute precedes
PATH=/ciscoview/Routershare/config/cfg00197.htm TITLE=SRP Higher Layer Interval Statistics TEXT=- History Use this option to monitor higher layer interval statistics of an interface side with a specific number. Procedure access information: N-1. Right-click the and select Configure from popup menu. Ports dialog box appears. 2. Category displays: (srpHostIntInterfaceSide) (srpHostIntNumber) view error that particular interval. Related Topics CiscoView Window Monitoring Devices Environment Components containing row information. between 96, which identifies available statistics. means most recent completed 15 minute precedes
PATH=/ciscoview/Routershare/config/cfg00199.htm TITLE=Media Dependent Statistics TEXT=SRP Media Dependent Statistics - History Use this option to monitor media dependent statistics of an interface side with specific interval. number. Procedure access information: N-1. Right-click the and select Configure from popup menu. Port dialog box appears. 2. Category displays: (srpRingIntInterfaceSide) (srpRingIntNumber) view that particular Related Topics Unwrap Wrap State Transition containing row information. Interval A between 96, which identifies available statistics. means most recent completed 15 minute precedes
PATH=/ciscoview/Routershare/config/dcca_profile.htm TITLE=DCCA Profile TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Name (cGgsnSADccaProfileNam) (cGgsnSADccaAuthorization) (CCFH) Attribute (cGgsnSADccaCcfh) (cGgsnSADccaDestinationRealm) Realm (cGgsnSADccaSessionFailover) Failover Retransmit Timer (cGgsnSADccaTxTimeout) SGSN State (cGgsnSADccaTriggerSgsnChange) (cGgsnSADccaTriggerQosChange) QOS (cGgsnSADccaRowStatus) Status Specifies Diameter Credit Control Application (DCCA) name. If set charging profile, GGSN contacts server. online billing. Must behavior Protocol valid value upon transition entry active. state. Defines authorization) method (provided by AAA referencing group, which defined group. Governs client. fault situations. When response not received, within configured timer, what happens next specified Failure Handling session: continue: Allows Packet Data (PDP) context. traffic. terminate: Terminates session. retryTerminate: alternate and, fail-to-send condition occurs, Sent (initial) Request (CCR) request. This mandatory while defining row can changed still For subsequent CCRs, original-realm AVP last Answer (CCA) used destination-realm. whether supported. true, will moved false, timeout messages. specification (Tx) that supervise communication server, because, prepaid services, user expects network reasonable time. Thus, react faster than underlying base protocol. elapses, takes action depending current started each (update). Since multiple are possible, vodafone-specific pending, restarts timer. answers all stopped. effect generic implementations. only, therefore has triggers quota reauthorization. does Modifying object affected existing PDPs using profile. Only new contexts. modifications. place change. affects create delete table.
PATH=/ciscoview/Routershare/config/DFP_Agent_Info.htm TITLE=DFP Agent Info TEXT=This dialog box provides information about the Dynamic Feedback Protocol (DFP) agents that reports to server load balancing (SLB) managers. Procedure Right-click device, then selected, Configure > Statistics With instance following displayed. IP (slbDfpAgentIpAddress) (slbDfpAgentPort) (slbDfpAgentState) (slbDfpAgentTimeout) Manager (slbDfpAgentRetryCount) count interval (slbDfpAgentInterval) (slbDfpAgentRowStatus) status address of agent. state times during which must send least one message manager. number attempts reestablish connection before retries connecting DFP. management station uses row create delete entry slbDfpAgentTable textual convention.
PATH=/ciscoview/Routershare/config/DFP_Password_Info.htm TITLE=DFP Password Info TEXT=This dialog box helps you modify or reset the password used in the Dynamic Feedback Protocol (DFP). Procedure Right-click device, authentication selected, Configure > (SLB) Statistics With server load balancing instance following information displayed. (slbDfpPasswordPending) setting Period (slbDfpPasswordTimeout) (slbDfpPasswordRowStatus) status pending uses MD5 within timeout ticks. should between slbDfpPasswordTimeout. If modified twice interval given by slbDfpPasswordTimeout, and of first modification are forgotten replaced second. removing current password. management station row create delete entry slbDfpPasswordTable, textual convention.
PATH=/ciscoview/Routershare/config/DiffServ_Code_Point_Map_Table.htm TITLE=DiffServ Code Point Map Table TEXT=GGSN DiffServ Code Point Map Table Use this dialog view Per Hop Behaviour (PHB) group mapping to Diff Server (DSCP). Procedure In the Chassis view, right-click device and select Configure from popup menu. following: information appears: Values (cggsnQosDiffServPhb) (cggsnQosDscp) Denotes various possible of PHB. value can bestEffort(15) any one signallingClass(1) Signalling class efClass(2) Expedited forwarding afClass1Low(3) Assured with drop precedence afClass1Medium(4) medium afClass1High(5) high afClass2Low(6) afClass2Medium(7) afClass2High(8) afClass3Low(9) afClass3Medium(10) afClass3High(11) afClass4Low(12) afClass4Medium(13) afClass4High(14) Best effort defined by cggsnQosDiffServPhb. recommended are: 101000 101110 001010 001100 001110 010010 010100 010110 011010 011100 011110 100010 100100 100110 000000
PATH=/ciscoview/Routershare/config/foreign_agent_ad_challenge_values.htm TITLE=Foreign Agent Advertisement Challenge Values TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Interfaces (ifIndex) (cmiFaAdvertChallengeIndex) (cmiFaAdvertChallengeValue) unique value, greater than zero, each interface. sublayer must remain constant least one reinitialization. of entity's network management system to next number last that can used by mobile node registration request sent this window
PATH=/ciscoview/Routershare/config/foreign_agent_ad_config.htm TITLE=Foreign Agent Advertisement Configurations TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Interfaces (ifIndex) Status (cmiFaAdvertIsBusy) Registration (cmiFaAdvertRegRequired) Last (cmiFaAdvertChallengeWindow) Values unique value, greater than zero, each interface. sublayer must remain constant least one reinitialization. of entity's network management system to next Indicates whether busy. When set true (1), advertisements sent by this will have bit 1. Specifies required number challenge that can used mobile node request
PATH=/ciscoview/Routershare/config/foreign_agent_asym_link_support_configs.htm TITLE=Foreign Agent Asymmetric Link Support Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Care-of-address (faSupportedCOA) FA Advertise (cmiFaCoaInterfaceOnly) (cmiFaCoaTransmitOnly) Status supported by this agent. Specifies whether interface) associated with (CoA) should transmit-only not. If true, other configured care-of-addresses will be advertised. (uplink) treats all registration requests received (on any having arrived interface. object can set to serial care-of-interfaces only.
PATH=/ciscoview/Routershare/config/foreign_agent_interface_configs.htm TITLE=Foreign Agent Interface Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Interfaces (ifIndex) (cmiFaReverseTunnelEnable) Tunnel Capability FA (cmiFaChallengeEnable) CHAP_SPI Number (cmiFaAdvertChallengeChapSPI) unique value, greater than zero, each interface. sublayer must remain constant least one reinitialization. of entity's network management system to next Specifies whether reverse enabled not. challenge authentication.
PATH=/ciscoview/Routershare/config/foreign_agent_system_configs.htm TITLE=Foreign Agent System Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Reverse (cmiFaRevTunnelSupported) Status FA (cmiFaChallengeSupported) (cmiFaEncapDeliveryStyleSupported) Delivery Style Indicates whether tunnel supported not.
PATH=/ciscoview/Routershare/config/foreign_agent_visitors_list.htm TITLE=Foreign Agent Visitors List TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cmiFaRegVisitorIdentifierType) Type Associated (cmiFaRegVisitorIdentifier) (cmiFaRegVisitorHomeAddress) (IP) (cmiFaRegVisitorHomeAgentAddress) Lifetime (cmiFaRegVisitorTimeGranted) Expire (cmiFaRegVisitorTimeRemaining) (cmiFaRegVisitorRegIDLow) Low Bits (cmiFaRegVisitorRegIDHigh) Registration Acceptance (cmiFaRegVisitorRegIsAccepted) (cmiFaRegVisitorChallengeValue) Value (CmiFaRegVisitorRegFlagsRev1) of visitor's identifier. with visitor. home address visiting mobile node. that granted this registration. Only valid faVisitorRegIsAccepted true (1). remaining until expires. It has same initial counted down by agent. 32 identification used Indicates whether been accepted not. If false (2), still pending reply. challenge forwarded previous reply, which can next request. flags sent
PATH=/ciscoview/Routershare/config/Frame_Relay_Circuits.htm TITLE=Frame Relay Circuits TEXT=The table displays the frame relay circuit information. Procedure Right-click on the serial port and select Configure from popup menu double-click port. configuration appears. Category drop-down list box. Dialog following information: DLCI (frCircuitDlci) Oper (frCircuitState) (frCircuitCreationTime) (frCircuitLastTimeChange) Last Change Max (frCircuitCommittedBurst) Bits Uncommitted (frCircuitExcessBurst) (frCircuitThroughput)
PATH=/ciscoview/Routershare/config/Frame_Relay_DLC.htm TITLE=Frame Relay - DLC TEXT=The table displays the frame relay data link connection information. Procedure Right-click on the serial port and select Configure from popup menu double-click port. configuration appears. Category drop-down list box. Dialog following information: (frDlcmiState) (frDlcmiAddress) Length (frDlcmiAddressLen) Status Enq Msg Intervals (frDlcmiPollingInterval) (frDlcmiMaxSupportedVCs) Errs (frDlcmiErrorThreshold) (frDlcmiMulticast) Service Virtual Circuits (frDlcmiMonitoredEvents) Events
PATH=/ciscoview/Routershare/config/GGSN_Access_Point.htm TITLE=GGSN Access Point TEXT=Statistics The GGSN Access Point category of the Chassis Configuration dialog box gives details of the points configured GGSN. Note This can be viewed Identifier cGtpGSNService set Monitor 'ggsn'. Procedure Right-click device and then select from list following information appears: (cgprsAccPtIndex) Unique local
PATH=/ciscoview/Routershare/config/GGSN_Access_Point_configure.htm TITLE=GGSN Access Point TEXT=The GGSN Access Point category of the Chassis Configuration dialog box gives details of the access points configured GGSN. Procedure Right-click device. Dial-on-Demand Authentication select Configure row, double-click from list. following information appears: Identifier (cgprsAccPtIndex) (cgprsAccPtRowStatus) Row (cgprsAccPtName) (cgprsAccPtType) (cgprsAccPtMode) Dynamic (cgprsAccPtIpAddressPool) Allocation Method Primary (cgprsAccPtDHCPServerPri) (cgprsAccPtDHCPServerSec) Secondary Gateway (cgprsAccPtDHCPGwAddr) (cgprsAccPtIPAccListGroupIn) Towards MS. (cgprsAccPtIPAccListGroupOut) (cgprsAccPtAccessViolation) Subscription (cgprsAccPtAutoAggregation) (cgprsAccPtSubrRequired) (cgprsAccPtNetworkInitiated) Interface (cgprsAccPtPppTunnelDialerIfIndex) (cgprsAccPtIdlePdpPurgeTimer) Connection (cgprsAccPtPppRegenSetupTime) (cgprsAccPtBlockMsRoaming) (cgprsAccPtAnonymousUserName) (cgprsAccPtAnonymousUserPassword) Password MS-ISDN ID (cgprsAccPtMsIsdnSuppressed) Mobile Stations Replacement (cgprsAccPtMsIsdnSuppressedValue) Radius (cgprsAccPtAaaAuthServerGroup) (cgprsAccPtAaaAccountingEnable) (cgprsAccPtAaaAccountServerGroup) Enabled APN. VRF (cgprsAccPtVrfName) (cgprsAccPtDhcpAddrSpace) Used (cgprsAccPtPppRegenEnable) Maximum Regenerated PPP (cgprsAccPtPppRegenMaxSessions) Tolerance Aggregation Unique local table. This objects createAndGo. deleted. conceptual set. There nontransparent mandatory request. destroy. cgprsAccPtAnonymousUserName. name consists parts: fully qualified domain that conforms DNS naming conventions. example would be: company.com.mncyyyy.mcczzzz.gprs'. Operator optional. It three labels, last which must mncyyyy.mcczzzz.gprs. without both network. identifiers null string, not specified. allowed PDN, through access-point. type can Description Users authenticated by addresses allocated. globally No defined specifically server. user dhcp disabled subscriber assignment case available, used. available. giaddr field determined pool specified, associated. Gn (ACL) uses compare packets received forwarding ACLs level control between violations packet, cause either dropped its PDP sessions terminated. action taken value cgprsAccPtAccessViolation. were originated PDN. Specifies how should treated. occurs violates rules cgprsAccPtIPAccListGroupOut. dealt one ways: discardPacket discarded terminateSession Indicates needs before accessing it. (PDN) initiated false, tunnel end-to-end external dial-up number consecutive seconds, context have idle GTP 0 means timer roaming blocked when entries non-transparent supplying password. corresponding For security reasons, retrieving returns zero-length string. id, MS, suppressed authenticating only transmitted station's id. cgprsAccPtMsIsdnIdSuppressed true. Valid characters 9, a, b, c, * #. object, sent AAA group accounting, enabled, mode. true, accounting. mode, always is, default. virtual, physical target other parameters ignored. real corresponds space Enables regenerate each time, within come up. automatically cgprsAccPtAggregTable, false. any,
PATH=/ciscoview/Routershare/config/GGSN_Access_Point_Extension.htm TITLE=GGSN Access Point Extension TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following details Service-Aware displayed: (cgprsAccPtIPAccListInEnable) (cgprsAccPtRedirInterMobilAddrTyp) (cgprsAccPtIPAccListOutEnable) cgprsAccPtIPAccListGroupOut RADIUS (cgprsAccPtAaaAccountingEnable) Server Response (cgprsAccPtGtpRespMesgWaitAcctng) TPDU cgprsAccPtSourceAddrViolTpdus cgprsAccPtIpAddressPool Verification (cgprsAccPtVerifyUpStrTpduSrcAddr) Destination (cgprsAccPtVerifyUpStrTpduDstAddr) Mobile (cgprsAccPtAdvDownlinkNextHopAddrType) (cgprsAccPtRedirInterMobilAddr) Request Suppressed (cgprsAccPtSuppressRadiusAttribs) AAA (cgprsAccPtInterimAccountinEnable) (cgprsAccPtSetRadiusAttributes) Values (cgprsAccPtPdpInServicePolicyName) (cgprsAccPtOperationMode) (cgprsAccPtAbsoluteSessionTimer) Session Timer NAS (cgprsAccPtRadiusAttrNasId) Inbound Policy (cgprsAccPtPppRegenVerifyDomain) (cgprsAccPtIpAddrLocalPoolName) Pool Billing (cgprsAccPtServiceAware) (cgprsAccPtAdvDownlinkNextHopAddr) cgprsAccPtAdvDownlinkNextHopAddrType. Hop When reset to true ACL denoted by cgprsAccPtIPAccListGroupIn becomes inactive. false waits before sending create PDPs contexts SGSN, requests received. particular APN. sends after start message (without waiting server). checks upstream against previously assigned this user. If addresses different, dropped incremented. enables restrict users fake identity. checking performed GGSN. ranges of reserved PLMN devices. there match, cgprsAccPtDestAddrViolTpdus scope MIB. protect GPRS networks hackers who may try flood nodes intense data traffic. type Internet which reachable. inter-mobile redirected. redirection APN, downstream, packets exit GGSN, they screened see other GTP-tunneled tunnels. so, gets device. zero, redirected, i.e., switched through going any Gi interface. that authorization server. used updates will triggered whenever object can only enabled. Indicates various attributes while communicating none value. using options below: 'userNameMsisdn' MSISDN Represents user-name attribute. 'accSessIdChargingId' accounting Denotes operational mode Each has deactivation behaviors given 'inService' Normal allowed. functions cgprsAccPtInServiceNotif notification indicate state. change. 'maintenance' new activated cgprsAccPtMaintenanceNotif (#27) Access-Accept packet. deactivate expires. same '0' disabled. length string needs unconfigure Per feature ensures exceed bandwidth negotiated procedure. service contains classification policing parameters. applicable pertaining PPP regen creation would rejected domain PCO field name. cgprsAccPtPppRegenEnable local. (Diameter Credit Control Application [DCCA] support) access-point. cGgsnSAServiceAware downlink address. Advertises destined routed.
PATH=/ciscoview/Routershare/config/ggsn_access_pt_cac_config.htm TITLE=GGSN Access Point CAC Configuration TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following information appears: Identifier (cgprsAccPtIndex) (cgprsAccPtCacPolicyName) Name Upstream Bandwidth (cgprsAccPtCacUpStrBandWidthPool) Downstream (cgprsAccPtCacDnStrBandWidthPool) Locally unique this Gateway GPRS support node (GGSN). policy that will be used by Call Admission Control (CAC) Packet Data Protocol (PDP) contexts associated with (APN). zero-length string indicates configured. of pool traffic. user-defined provides pre-allocation details like amount available percentage specific class. uses during activation modification procedures.
PATH=/ciscoview/Routershare/config/ggsn_access_pt_chrg_param.htm TITLE=GGSN Access Point Charging Parameters TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following information appears: Identifier (cgprsAccPtIndex) (MS) (cgprsAccPtMsType) (cgprsAccPtChgProfile) Number (cgprsAccPtChgProfOverride) (SGSN) Values Locally unique this Gateway GPRS support node (GGSN). Mobile station type applied to profile indicated by Name (APN). There are six possible values: home IMSI correspond same Public Land Network (PLMN) roamingTrusted belongs which has different visitingTrusted Note: roaming/visiting considered trusted. APN. Valid range 15. object must set when creating table entry. true characteristics supplied Serving ignored provided used instead.
PATH=/ciscoview/Routershare/config/ggsn_access_pt_gen_server_table.htm TITLE=GGSN Access Point Generic Server Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following information appears: Identifier (cgprsAccPtIndex) Primary DNS (cgprsAccPtPriDnsServer) Secondary (cgprsAccPtSecDnsServer) NetBIOS (cgprsAccPtPriNetbiosServer) (cgprsAccPtSecNetbiosServer) Locally unique this Gateway GPRS support node (GGSN). IP address of server. Note: can been configured. only when has already name (NBNS). NBNS.
PATH=/ciscoview/Routershare/config/ggsn_access_pt_route_probe_table.htm TITLE=GGSN Access Point Route Probe Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following information appears: Identifier (cgprsAccPtIndex) Destination IP Address (cgprsAccPtRpDestAddr) (cgprsAccPtRpProtocol) Type (cgprsAccPtRpDestPort) TTL Value (cgprsAccPtRpTtl) Locally unique this Gateway GPRS support node (GGSN). which packet. will sent. of There are two possible values: udp icmp object can set. only after has first been number when Indicates
PATH=/ciscoview/Routershare/config/GGSN_Address_Duplication.htm TITLE=GGSN IP Table TEXT=GGSN Address Duplication The GGSN Address Duplication category of the Chassis Configuration dialog box displays range. addresses used following GPRS PLMN. This helps to avoid duplication. Note can be viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device. and then select Configure row, double-click from list. information appears: Starting (cGgsnMsExcludeRangeStartIpType) (cGgsnMsExcludeRangeStartIp) Ending (cGgsnMsExcludeRangeEndIpType) (cGgsnMsExcludeRangeEndIp) Create/Delete (cGgsnIpDupProtectRowStatus) Internet by which reachable. value object same cGgsnMsExcludeRangeEndIpType. cGgsnMsExcludeRangeStartIpType. row protect table. createAndGo. new delete existing destroy.
PATH=/ciscoview/Routershare/config/GGSN_Aggregate_Routes_Table.htm TITLE=GGSN Aggregate Routes Table TEXT=The GGSN Aggregate Routes Table category of the Chassis Configuration dialog box displays details of table. Note This can be viewed if cGtpGSNService set to 'ggsn'. Procedure Right-click device. and then select Configure row, double-click from list. following information appears: (cGgsnDefaultAggregIpAddrType) Address Type IP (cGgsnDefaultAggregIpAddr) (cGgsnDefaultAggregIpMask) Create/Delete (cGgsnDefaultAggregRowStatus) Internet denoted by cGgsnDefaultAggregIpAddr. whose network prefix defined cGgsnDefaultAggregIpMask. Net mask pertaining row object used createAndGo. new delete existing destroy. values createAndWait notInService are supported.
PATH=/ciscoview/Routershare/config/GGSN_APN_Aggregate_Routes.htm TITLE=GGSN APN Aggregate Routes TEXT=The GGSN APN Aggregate Routes category of the Chassis Configuration dialog box lists the APN details including aggregation. Note This can be viewed specified. cGtpGSNService set to 'ggsn' Procedure Right-click device. and then select Configure , double-click from list. following information appears: Internet Address (cgprsAccPtAggregIpAddrType) IP (cgprsAccPtAggregIpAddr) Net-mask (cgprsAccPtAggregIpMask) (cgprsAccPtAggregRowStatus) Status denoted by cgprsAccPtAggregIpAddr. whose network prefix defined cgprsAccPtAggregIpMask. When object must pertaining row route table. Used createAndGo. new delete existing destroy.
PATH=/ciscoview/Routershare/config/GGSN_APN_Generic.htm TITLE=GGSN APN Generic TEXT=The GGSN APN Generic category of the Chassis Configuration dialog box lists the access point system information. Note This can number viewed Notification cGtpGSNService set History 'ggsn'. Procedure Right-click device. and then select Configure However, double-click from list. following appears: Controller (cgprsAccPtCfgNotifEnable) (cgprsAccPtCfgNotifHistMax) cgprsAccPtCfgNotifHistTable. Size (cgprsAccPtCfgNotifLatestIndex) Entries cgprsAccPtCfgNotifIndex Controls generation notifications. are generated irrespective value object. Maximum event table When full, oldest removed make space new entries. most recently created entry
PATH=/ciscoview/Routershare/config/GGSN_APN_History.htm TITLE=GGSN APN History TEXT=The GGSN APN History category of the Chassis Configuration dialog box lists the access point notifications. Note This can been viewed cGtpGSNService set 'ggsn' Procedure Right-click device. and then select Configure created, double-click from list. following information appears: Notification Identifier (cgprsAccPtCfgNotifIndex) (cgprsAccPtCfgNotifAccPtIndex) (cgprsAccPtCfgNotifReason) Arbitrary nonzero integer value that uniquely identifies reaches previously sent by GPRS. increases monotonically with GGSN. When object maximum 4294967295 wraps 1. changed modified. notification. be: modification(1) creation(2) deletion(3)
PATH=/ciscoview/Routershare/config/ggsn_cac_policy_table.htm TITLE=GGSN CAC Policy Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following: information appears: (cggsnUmtsQosCacPolicyName) Maximum Pdp-context (cggsnUmtsQosCacMaxPdp) (cggsnUmtsQosCacPdpThreshold) Traffic-Class (cggsnUmtsQosCacMaxTrafficClass) Handling Priority (cggsnUmtsQosCacMaxTrafHandPrio) Peak-throughput (cggsnUmtsQosCacMaxThruPut) (cggsnUmtsQosCacMaxThruPutReject) Exceeding Delay-class (cggsnUmtsQosCacMaxDelayClass) (cggsnUmtsQosCacMaxDelayClassRej) Call Admission Control (CAC) name that will number attached Protocol none more Access Point Names (APNs). of Packet Data (PDP) contexts can created. When set. zero, there note limit creation. threshold defined by this object, reached, only with allocation/retention priority1 are accepted. Note after has already been values: should lower than cggsnUmtsQosCacMaxPdp. checked. Indicates highest acceptable traffic class. four possible conversational streaming interactive background If requested higher configured class, rejected. Also downgraded. cggsnUmtsQosCacMaxTrafficClass. priority2 priority3 applicable type any peak particular APN. used GPRS Tunneling (GTP) v0 v1 containing R97/98 Quality Service (QoS). specified either set, mapped based R99 bit rate rules determining attributes (as 23.107). addition, parameter applied request. true its exceeds cggsnUmtsQosCacMaxThruPut. false non-zero value. delayClass1 QoS. five delayClass2 delayClass3 delayClass4 cggsnUmtsQosCacMaxDelayClass. other
PATH=/ciscoview/Routershare/config/ggsn_cac_traffic_class_table.htm TITLE=GGSN CAC Traffic Class Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN Policy from Category drop-down box. With entry selected following dialog box, Details information appears: (cggsnUmtsQosCacPolicyName) (cggsnUmtsQosCacTcTrafClass) (cggsnUmtsQosCacTcBitRateType) (cggsnUmtsQosCacTcBitRate) Type (cggsnUmtsQosCacTcDirection) (cggsnUmtsQosCacTcReject) Exceeding Max Call Admission Control (CAC) name that will be attached Protocol Telephone more Access Point Names (APNs). Universal Mobile System (UMTS) which MBR/GBR uplink/downlink assigned. There are four possible values: conversational streaming interactive background Note: When set guaranteed only can this object. rate applicable indicated by cggsnUmtsQosCacTcTrafClass. two maximum Indicates direction of traffic. allowed whether requested downgraded. Packet Data (PDP) rejected. exceeds cggsnUmtsQosCacTcBitRate. true false
PATH=/ciscoview/Routershare/config/ggsn_cac_virtual_bw_pool.htm TITLE=GGSN CAC Virtual BW Pool TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following information appears: (cggsnUmtsQosCacBWPoolName) Total Bandwidth (cggsnUmtsQosCacBWPoolBWVal) of which will be attached to Access Point (APN). Indicates this pool. Note: value object must set each table entry.
PATH=/ciscoview/Routershare/config/GGSN_Charging_Alarms.htm TITLE=GGSN Charging Alarms TEXT=The GGSN Charging Alarms category in the Chassis Configuration dialog box provides a history of the gateways and Monotonically charging-related alarms. Note This can be viewed identifies cGtpGSNService set 'ggsn'. Procedure Right-click device. then select Configure , double-click from list. following information appears: Gateway ID (cgprsCgAlarmHistIndex) (cgprsCgAlarmHistType) (cgprsCgAlarmHistAddress) (cgprsCgAlarmHistAddrType) IP (cgprsCgAlarmHistSeverity) Detailed (cgprsCgAlarmHistInfo) increasing integer that indexes value object wrapped back one when reaches maximum 4294967295. GPRS alarm. internet address given cgprsCgAlarmHistAddress. uniquely gateway. Indicates severity generated.
PATH=/ciscoview/Routershare/config/GGSN_Charging_Gateways.htm TITLE=GGSN Charging Gateways TEXT=The GGSN Charging Gateways category of the Chassis Configuration dialog box lists the charging gateway details GGSN. Note This visible only Identifier cGtpGSNService set mandatory 'ggsn'. Procedure Right-click device. standby then select Configure row, double-click from list. following information appears: (cgprsCgGatewayIndex) Address (cgprsCgGatewayAddrType) (cgprsCgGatewayAddr) Table (cgprsCgGatewayRowStatus) (cgprsCgOperStatus) Reachability (cgprsCgLinkState) Unique CG. Internet given cgprsCgGatewayAddr. IP that uniquely identifies row table. Used createAndGo. new delete existing objects are request. To destroy. Indicates whether configured active. Value Description undefined (1) Neither nor mode (2) (3) status can be: reachable pending not but trying establish connection with off
PATH=/ciscoview/Routershare/config/ggsn_charging_gateway_status.htm TITLE=GGSN Charging Gateway Status TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following information appears: (cgprsCgChargingCharReject) No-profile Match (cgprsCgServiceMode) (cgprsCgCharSelectionMode) Generate (cgprsCgPartialCdrGenEnable) CDRs. (cgprsCgSwitchOverPriority) Over Priority (cgprsCgActiveChgGatewayAddress) Characteristic Selection (cgprsCgReconnect) Timer (PTC) IE (cgprsCgPtcEnable) Send (cgprsCgPtcPossiblyDupEnable) Duplicate Record cgprsCgActiveChgGatewayAddrType. Previous (cgprsCgOldChgGatewayAddress) Specifies whether incoming Packet Data Protocol (PDP) create request. rejected. when either matching cannot configured overriding present. If set true false accepted default, applied limit. Indicates currently service mode gateways. There are network possible values: operational operate was they normally do. maintenance transmission other does take place. However, collection continues expected. generates partial secondary which some fields that becomes modified during life included. primary refers first opened response Subsequent CDRs, called closed (by trigger event such exceeding volume This object used enabled. switch mechanism. with higher than comes up, gateway. remains so, up. added CDR. reconnect feature enabled, will attempt unreachable due transient link failures. available using UDP path respond to, but send, echo requests. Note: disabled. includes Transfer Command message. possibility has been ruled out. directed CGF generating node) because working properly. relevant only IP address type indicated active
PATH=/ciscoview/Routershare/config/ggsn_charging_gateway_stat_contd.htm TITLE=GGSN Charging Gateway Status Contd TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Maximum (cgprsCgCdrOptionServiceRecord) Records (cgprsCgPartialCdrGenEnableAll) (S-CDR) Enable All Real APN. (cgprsCgCdrOptionApn) (cgprsCgCdrOptionVirtualApn) Selection (cgprsCgCdrOptionApnSelMode) (cgprsCgCdrOptionDynamicAddr) (cgprsCgCdrOptionPdpAddress) Network Initiated (PDP) Context (cgprsCgCdrOptionNip) Served (cgprsCgCdrOptionPdpType) (MSISDN, Number (cgprsCgCdrOptionSerMsisdn) SGSNs PLMN, ID). (cgprsCgCdrOptionSgsnPlmn) CAMEL (cgprsCgCdrOptionCamelCharInfo) International Mobile Equipment Identity (cgprsCgCdrOptionImeisv) (cgprsCgCdrOptionMsTimeZone) Zone Radio Access (cgprsCgCdrOptionRatType) (cgprsCgCdrOptionUserLocInfo) Location GPRS Support Node-Call Detail (G-CDRs) contains part, entire duration, (Software Packet Data Protocol context. includes such (as subscriber. IMSI), used, QoS applied, location), timestamp volume recorded. separately upstream downstream direction, thresholds intermediate generation tariff switches. addition above, enhanced service-record without usage each flow. by session (specified For example, per default this feature cannot enabled. can before closed. partial opened. When offset true enables copy release prior 4 (cgprsCgRelease). change limit trigger cgprsCgCdrSgsnChangeLimit must well. only false currently address, may present G-CDR. included accounting records. Point Name disabled G-CDRs. option CHARGING_RELEASE 98 99. virtual mode field gateway. indicates which was selected: non-subscribed that station. (NIP) inclusion network-initiated. omitted case mobile-activated IMSI. layer type; version 6. parameter shall except both PPP, dynamic assignment used. defines IP, IHOSS:OSP. provides Station (MS) (MSISDN) create request party; refers involved transaction does (MCC MNC) Identifier have been connected during record. implies moves another has -- Tag Length SGSN's call received (IMEISV): Version) Element will handled transparent manner 5.0-compliant any modification. between universal local steps 15 minutes where resides. (RAT) whether serves (UE) Terrestrial (UTRAN) GSM/EDGE (GERAN). Cell Global (CGI)/Service Area (SAI) located.
PATH=/ciscoview/Routershare/config/GGSN_Charging_Information.htm TITLE=GGSN Charging Information TEXT=The GGSN Charging Information category of the Chassis Configuration dialog box gives the general charging information. Note This 'can-close-cdr' Number viewed (cgprsCgTariffTimeMaxEntries) cGtpGSNService set to 'ggsn'. Procedure Right-click device. and then select Configure true, double-click from list. following appears: Process State (cgprsCgEnable) (cgprsCgCdrLocalSeqNumEnable) Record Sequence (cgprsCgCdrNodeIdEnable) ID Open New (cgprsCgClearCdrPartialCdr) G-CDRs Trigger (cgprsCgAlarmHistTableMax) SGSN Changes G-CDR (cgprsCgSgsnChangeLimit) (cgprsCgFlowControlEcho) Controls Packet Statistics (cgprsCgCdrPktsStatEnable) Non-primary (cgprsCgCdrNonPrimaryEnable) (cgprsCgChargeForRoamersOnly) charge (cgprsCgCdrAggreLimit) Data (cgprsCgTransInterval) Upper Entries (cgprsCgTariffTimeNextIndex) Entry cgprsCgTariffTimeIndex (cgprsCgAlarmEnable) Used enabled disable transaction feature GGSN. When objects. that uses local field, contain. true. using include partial Closes all existing CDRs, transfers them CG. opens any PDP context. Value Description 'close-cdr' closed. only state. cannot-close-cdr closing-cdr are closing. Maximum closure record. reached, opened. zero, every change, flow between enables element private extension echo request. maintaining packets transmitted collection statistics. cgprsGtpChargingPktsUplink cgprsGtpChargingPktsDownlink generation nonprimary control follows: (1) false, (2) Disables CDRs. have same content Indicates needs generates non-roamers. option affects contexts. ones already been created. affected. aggregated message interval, seconds, two GPRS (user session). sent by gateway. limit cgprsCgTariffTimeTable. creating 0 means rows Otherwise, recommended values assigned contiguously, starting 1. cgprsCgAlarmNotif notifications
PATH=/ciscoview/Routershare/config/GGSN_Charging_Info_Extension.htm TITLE=GGSN Charging Info Extension TEXT=Use this dialog to view GGSN charging information details. Procedure Right-click the device and then select Configure, double-click device. from category list following appears: (cgprsCgAlarmHistLatestIndex) Gateway Id Maximum SGSN changes Time-trigger G-CDR (cgprsCgCdrSgsnChangeLimit) (cgprsCgRelease) GTP (cgprsCgGtpShortHeaderEnable) Header Data Record Transfer Format (cgprsCgTransFormNumRespEnable) (cgprsCgContainerTimeLimit) value, profile cgprsCgAlarmHistIndex most recently created entry cgprsCgAlarmHistTable. number that closure partial record. When reached, closed. new opened. zero, every change, If set '-1', not associated with creation specific parameters need used communicating CG. example, Qos information, characteristics field, etc. Enables 6-byte short transactions. Toggle possible there are pending CDR's. true means response IE. uses one 2-octet which contains records responded. false length active MS sessions GGSN.The collect related packet GPRS mobile Traffic Volumes attribute consists containers, can certain trigers conditions like, volume limit duration object some non-zero time updation reached.
PATH=/ciscoview/Routershare/config/ggsn_charging_profile.htm TITLE=GGSN Charging Profile Table TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from (cgprsCgProfileCategory) list. following information appears: Number (cgprsCgProfileNum) Description (cgprsCgProfileDesc) (cgprsCgProfileCdrSuppress) CDRs (cgprsCgProfileVolumeLimit) (cgprsCgProfileVolumeLimitReset) (cgprsCgProfileDurLimitReset) Timer Duration (cgprsCgProfileDurLimit) Enable (cgprsCgProfileTariffTime) Maximum SGSN Changes (cgprsCgProfileSgsnChange) Suppression (cgprsCgProfileCdrSuppressPrepaid) (DCCA) Client (cgprsCgProfileContentDccaProfile) Close/Update PostPaid (cgprsCgProfileContentPostTime) Validity Timeout (cgprsCgProfileContentPostValTime) Count (cgprsCgProfileContentPostVolume) (cgprsCgProfileContentRulebaseId) IDs Represents bits characteristics. context. string that, describes this profile. Indicates current category. Therefore, are four possible values: hotRate billing). flat generated. prepaid. normal When to: true volume-based limit, which update must take place. Used reset specified another trigger, occurs. such reaching false will continue until reaches cgprsCgProfileVolumeLimit. timeout. zero, set. cgprsCgProfileDurLimit. enables tariff Denotes closure G-CDR. partial record. reached, closed. new opened. then every change, Specifies can only won't any users. Diameter Credit Control Application communicate with server name (cGgsnSADccaProfileName). presence object online required. regardless whether subscriber postpaid, contact If treated user, returns X user. valid value, using (offline condition profile, exceeded, causes collect upstream downstream traffic, bytes counts particular PDP By default, quota. has configured, applies both time-based maintains across disallow containers before closing updating Sets rulebase Rulebases rules defining categories decisions, how measure based. maps CSG plans. presented RADIUS Access Accept message overrides received initial
PATH=/ciscoview/Routershare/config/ggsn_charging_profile_map_table.htm TITLE=GGSN Default Charging Profile Map Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from (cgprsCgProfileMapCategory) drop-down box. following: information appears: (MS) Type Number (cgprsCgProfileMapNum) (cgprsCgProfileMapOverride) (SGSN). Values (cgprsCgProfileMapTrusted) Indicates mobile station type. There are four possible values: any home roaming visitor. that created by cgprsCgProfileTable. This objects holds valid represented cgprsCgProfileNum. Note: 0 cannot deleted using It other configuration such as cgprsCgContainerVolThresh, cgprsCgCdrSgsnChangeLimit, cgprsCgContainerTimeLimit. whether set should override received Serving GPRS Support Node profiles. trusted irrelevant when either all If true will roamer. false just
PATH=/ciscoview/Routershare/config/GGSN_Charging_Tariff_Details.htm TITLE=GGSN Charging Tariff Details TEXT=The GGSN Charging Tariff Details category in the Chassis Configuration dialog box lists the entry details for times. Note This cannot Number viewed cGtpGSNService set to 'ggsn'. Procedure Right-click device. and then select Configure , double-click from list. following information appears: (cgprsCgTariffTimeIndex) ID (cgprsCgTariffTimeRowStatus) of Row Hours (cgprsCgTariffTimeHour) Minutes (cgprsCgTariffTimeMin) Seconds (cgprsCgTariffTimeSec) Identifier Arbitrary nonzero integer value that uniquely identifies each time. table. Used createAndWait new delete existing You modify rows object. active. options notInService are supported given by part GPRS
PATH=/ciscoview/Routershare/config/GGSN_Charging_Transmission_Details.htm TITLE=GGSN Charging Transmission Details TEXT=The GGSN Charging Transmission Details category of the Chassis Configuration dialog box provides the details. Note This cannot number viewed if cGtpGSNService set (cgprsCgPathProtocol) 'ggsn'. Procedure Right-click device. outstanding select Configure queue, double-click from list. following information appears: GGSN's Queue (cgprsCgPktsQSize) Two TCP. Retry Interval (cgprsCgPathRequest) (cgprsCgContainerVolThresh) Triggered Threshold IP Mapping (cgprsCgMapDataTos) Transport (cgprsCgServerSwitchTimeout) Timeout Maximum (cgprsCgConditionLimit) Destination (cgprsCgGtpPrimePort) Transmit (cgprsCgN3BufferSize) size, terms requests transferring data. default value, 128. interval, minutes, between attempts establishing connection, communication with CG. 1460. Traffic volume threshold, bytes, that triggers addition container closure G-CDR. 1048576. Type (ToS) GPRS packets are: transmitted GGSN. service priority directly proportional being higher. when values not used mapping. 3. protocols receive udp. Time, seconds, which waits located become unusable. then switches over alternate A means object disabled. changes condition partial record. reached, existing closed new opened. both UDP 3386 transmitting GTP PDU.
PATH=/ciscoview/Routershare/config/GGSN_GSN_Addressing.htm TITLE=GGSN GSN Addressing TEXT=The GGSN GSN Addressing category in the Chassis Configuration dialog box lists the GGSN GSN addressing details. Note This can be viewed identifies cGtpGSNService set to 'ggsn'. Procedure Right-click device. and then select Configure node, double-click from list. following information appears: (cGtpGSNAddressType) (cGtpGSNAddress) GTP (cGtpGSNVersion) of Internet by which accessed. IP that uniquely node. version0 supported identified cGtpGSNAddress. Values are: represents version1
PATH=/ciscoview/Routershare/config/GGSN_GTP _Path_Table.htm TITLE=GGSN GTP Path Table TEXT=Use this dialog to view the path details of GGSN with SGSN or charging gateway. Procedure In the Chassis view, right-click device and select Configure from popup menu. following information appears: (cGtpPathAddressType) Type (cGtpPathAddress) (cGtpPathPort) (cGtpPathVersion) Related Topics Internet address by which reachable. An that uniquely identifies remote node. established. value zero invalid. version0 identified cGtpPathEntry. Values are: represents version1 1.
PATH=/ciscoview/Routershare/config/GGSN_GTP_Director.htm TITLE=GGSN GTP Director TEXT=The GGSN GTP Director category of the Chassis Configuration dialog box displays the GGSN GTP director information. Note This can before viewed ciscoGtpDirectorNotifications (cGtpGSNService) reset 'gtpdirector'. Procedure Right-click device. and then select Configure GDM, double-click from list. following appears: GPRS Type Retry same (cgdCreatePdpRequestInfoSaveTimer) Send (cgdNotifEnable) service enabled device: Value Description undefined functionality turned off. Device functions GGSN. sgsn SGSN. GDM. When configured all other objects CISCO-GTP-DIRECTOR-MIB will notification. accessible should used managing receives request. create PDP, processes forwards saves related timer defines during which maintained by Any subsequent retries within period forwarded GGSN, but occurs expires. Indicates whether sent generated true Enables false Prevents sending out
PATH=/ciscoview/Routershare/config/GGSN_GTP_Director_.htm TITLE=GGSN GTP Director TEXT=The GGSN GTP Director category of the Chassis Configuration dialog box displays the GGSN GTP director information. Note This can before viewed ciscoGtpDirectorNotifications (cGtpGSNService) reset 'gtpdirector'. Procedure Right-click device. and then select Configure GDM, double-click from list. following appears: GPRS Type Retry same (cgdCreatePdpRequestInfoSaveTimer) Send (cgdNotifEnable) service enabled device: Value Description undefined functionality turned off. Device functions GGSN. sgsn SGSN. GDM. When configured all other objects CISCO-GTP-DIRECTOR-MIB will notification. accessible should used managing receives request. create PDP, processes forwards saves related timer defines during which maintained by Any subsequent retries within period forwarded GGSN, but occurs expires. Indicates whether sent generated true Enables false Prevents sending out
PATH=/ciscoview/Routershare/config/GGSN_GTP_Information.htm TITLE=GGSN GTP Information TEXT=The GGSN GTP Information category of the Chassis Configuration dialog box displays the GGSN GTP information. Note This can be: viewed cGtpNotifications (cGtpGSNService) set gtp-director 'ggsn'. Procedure Right-click device. (cGtpGSNTotalBandwidthResrc) then select Configure retransmitted, double-click from list. following appears: GPRS Type (cGtpVersion) (cGtpMaximumPdps) Retransmissions (cGtpN3Request) Receive (cGtpN3BufferSize) Size Resource PDP Contexts Availability (cGtpNotifEnable) (cGtpLastNoRespToEchoGSNIpAddrTyp) Unreachable Address IP (cGtpLastNoRespToEchoGSNIpAddr) Indicates service that enabled Description undefined (0) functionality disabled (1) Device functions sgsn (2) (3) GDM version supported. bytes GSN. number times signaling request messages. notification corresponding response received within specified cGtpT3ResponseTimer. buffer G-PDUs If packet contains more data than contain, discarded. amount bandwidth total depends various factors such system throughput, memory size, maximum portion resources allocated user's context activation time, based Qos class. activated whether are sent when generated Value true Enables sending false Prevents Internet which reached. last peer did reply local
PATH=/ciscoview/Routershare/config/GGSN_GTP_Path_Table.htm TITLE=GGSN GTP Path Table TEXT=Use this dialog to view the path details of GGSN with SGSN or charging gateway. Procedure In the Chassis view, right-click device and select Configure from popup menu. following information appears: (cGtpPathAddressType) Type (cGtpPathAddress) (cGtpPathPort) (cGtpPathVersion) Internet address by which reachable. An that uniquely identifies remote node. established. value zero invalid. version0 identified cGtpPathEntry. Values are: represents version1 1.
PATH=/ciscoview/Routershare/config/GGSN_GTP_Timer.htm TITLE=GGSN GTP Timer TEXT=The GGSN GTP Timer category of the Chassis Configuration dialog box lists details of the GGSN GTP timer. Note This can before viewed notification cGtpGSNService set (cGtpDynamicEchoTimerSmoothFactor) 'ggsn'. Procedure Right-click device. and then select Configure timer, double-click from list. following information appears: T3-RESPONSE (cGtpT3ResponseTimer) Availability (cGtpEchoRequestTimerEnable) (cGtpEchoRequestTimer) (cGtpDynamicEchoTimerEnable) Minimum (cGtpDynamicEchoTimerMinTime) Smooth Used retransmission. starts upon signaling request message. retransmitted, normally response received expires. Indicates echo by GGSN. Value Description true. false Disables interval, seconds, after which retransmitted. An event message, generated, identifying peer (that is, Address), failed respond. object retrieved only dynamic Enables time, factor adjusted.
PATH=/ciscoview/Routershare/config/GGSN_History_Table.htm TITLE=GGSN History Table TEXT=The GGSN History Table category of the Chassis Configuration dialog box provides details of the GGSN Notification Table. Note This cannot be: viewed cGtpGSNService set 'ggsn' Procedure Right-click device. and authenticationFail select Configure bytes, double-click from list. following information. appears: (cGgsnHistNotifIndex) (cGgsnHistNotifType) (cGgsnHistNotifSeverity) Level (cGgsnHistNotifTimestamp) Address Reachable (cGgsnHistNotifGgsnIpAddrType) Device that generated. (cGgsnHistNotifGgsnIpAddr) Additional (cGgsnHistNotifInfo) Monotonically increasing integer indexes notifications. value object wrapped back (1) when reaches maximum 4294967295. issued by Description ggsnServiceUp service started ggsnServiceDown (2). shut down mapSgsnUp (3) MAP-SGSN mapSgsnDown (4) noResource (5) MS initiated network PDP count reached. limit noRadius (6) server configured noDHCPServer (7) ipAllocationFail (8) IP allocation failed (9) Authentication apnUnreachable (10) Access point Indicates severity notification. You cleared indeterminate sysUpTime was Internet which uniquely identifies Textual cGgsnHistNotifType. contains about alarm type. could also If message text exceeds 64 truncated. 63 asterisk (*) appended show been
PATH=/ciscoview/Routershare/config/GGSN_PLMN_Address_Range.htm TITLE=GGSN PLMN Address Range TEXT=Use this dialog to configure Public Land Mobile Networks (PLMN) address ranges used for General Packet Radio Service (GPRS). Procedure In the Chassis view, right-click device select from popup menu. following information appears: (cGgsnPlmnAddrRangeIpAddrType) (cGgsnPlmnAddrRangeFirstIp) (cGgsnPlmnAddrRangeLastIp) Rowstatus (cGgsnPlmnAddrRangeRowStatus) (cGgsnPlmnAddrRangeUsage) type addresses. Only ipv4(1) are supported. IP range. object 'createAndGo'. new row, deleted existing table. set 'destroy'. modify needs be created with values. Specifies how uses When 'security', i.e. any TPDU destination that falls will discarded. 'sgsn', denotes local which can check roaming MS.
PATH=/ciscoview/Routershare/config/ggsn_plmn_table.htm TITLE=GGSN PLMN Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN from Category drop-down box. following information appears: Mobile Country Code. (MCC) (cGgsnPlmnMcc) Network (MNC) (cGgsnPlmnMnc) (cGgsnPlmnScope) Segment of Public Land (PLMN) ID that indicates relevant scope PLMN. There are possible values: home trusted Note: At any given time, only one entry can have
PATH=/ciscoview/Routershare/config/GGSN_QOS.htm TITLE=GGSN QOS TEXT=The GGSN QOS category of the Chassis Configuration dialog box lists the quality of service parameters (QoS) following GPRS system. Note This canonical be: viewed (cggsnQosUmtsDscpUnmodified) cGtpGSNService set (cggsnQosPremiumMtDeviationFactor) 'ggsn'. Procedure Right-click device. (cggsnQosTotalBandwidthResrc) then select Configure throughput, double-click from list. information appears: (cggsnQosMappingMethod) Type Resource Deviation (cggsnQosBestEffrtBandWidthFactor) DSCP Status & Path last object UMTS. method mapped QoS. delay none(4) (best-effort) amount bandwidth GSN. total depends various factors such memory size, maximum number PDP contexts supported. A portion resources allocated user's time activation, based class. retrieved only (2). Mean used by calculate datagram that allowed premium applied Checks subscriber forwarded uplink downlink without modification. Values are: up(1) not down(2) all(3) both paths
PATH=/ciscoview/Routershare/config/GGSN_QOS_Mapping.htm TITLE=GGSN QOS Mapping TEXT=The GGSN QOS Mapping category of the Chassis Configuration dialog box displays the mapping of different classes to ToS precedence; IP header. Note This canonical(2): delay_best_effort viewed cGtpGSNService set 'ggsn'. tables: empty 'cggsnQosMappingMethod' 'none'. Procedure Right-click device. and then select Configure QoS, double-click from list. following information appears: (cggsnQosClass) (cggsnQosMappedIpTos) Specifies delay(3): based values cggsnQosMappingMethod. interpreted shown If Interpretation delay1 delay2 delay3 4 premium normal which mapped. service priority. directly proportional that is, higher precedence, 6 (internetwork_control) 7 (network_control) are not used mapping.
PATH=/ciscoview/Routershare/config/ggsn_redundancy_config.htm TITLE=Redundancy Configuration TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select the category following information appears: Keep-alive Threshold (cRFCfgKeepaliveThresh) (cRFCfgKeepaliveTimer) Notifications (cRFCfgNotifTimer) (cRFCfgAdminAction) (cRFCfgNotifsEnabled) Indicates (cRFCfgMaintenanceMode) (cRFCfgRedundancyMode) Description (cRFCfgRedundancyModeDescr) Operational (cRFCfgRedundancyOperMode) On platforms that support keep-alives, value designates number software lost tolerated before failure condition this declared. If occurs, SWACT 'notification' sent. object, has purpose effect. keepalives, timer used guard against keep-alives. subsystem expects received within period. period, terminology here. refers SNMP notification. As 'standbyHot' unit. progresses state, asynchronous messages from active must acknowledged receives acknowledgement during specified progression proceeds normal. expires unit, switch activity occurs. variable reset invoke action commands. useful (non-maintenance) upgrade activities. Allows enabling/disabling notifications. whether redundant units may communicate synchronization each other. communication permitted, 'true'. 'false'. 'true', considered mode operation. 'false', (true), will occur. When disabled (false), recover. maintenance-type operations. configured Further clarifies describes indicated cRFCfgRedundancyMode. Implementation-specific associated current presented
PATH=/ciscoview/Routershare/config/ggsn_redundancy_hist_table.htm TITLE=Redundancy History Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select category following information appears: Entries (cRFHistoryTableMaxLength) No. of System (cRFHistoryColdStarts) restarts. Standby Available (cRFHistoryStandByAvailTime) Previous (cRFHistoryPrevActiveUnitId) (cRFHistoryCurrActiveUnitId) Curent Switchover (cRFHistorySwitchOverReason) (cRFHistorySwactTime) Maximum number permissible table. value 0 will result no being maintained. Indicates cold This includes due failure manual cumulative time that redundant unit has been since last initialization. primary went down. secondary took active. reason switchover. Date & when occured.
PATH=/ciscoview/Routershare/config/ggsn_redundancy_status.htm TITLE=Redundancy Status TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select category following information appears: (cRFStatusUnitId) (cRFStatusPeerUnitId) (cRFStatusUnitState) (cRFStatusPeerUnitState) Is (cRFStatusPrimaryMode) Redundant Detected (cRFStatusDuplexMode) (cRFStatusManualSwactInhibit) Manual Switching (cRFStatusLastSwactReasonCode) Reason (cRFStatusFailoverTime) (cRFStatusPeerStandByEntryTime) standbyHot SWACTs. unique identifiers this unit. implementation-specific but method selecting must remain consistent throughout subsystem. Some example include: slot id, physical logical entity assigned internally current state. of peer primary Indicates whether has been detected. If detected, object true. not false. switchover. activity. permitted. allowed, Note that value inverse does indicate occurred. only user-controllable capability enabled. event which becomes active. previously standby. last sysUpTime when took will 0 until first entered initialization.
PATH=/ciscoview/Routershare/config/ggsn_sgsn_thruput.htm TITLE=GGSN - SGSN Throughput TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. – from Category list. following information appears: Remote (cGtpPathAddress) (cGtpPathPort) Collection (cGgsnSgsnThruPutInterval) An address that uniquely identifies node. to which this path established. values of zero invalid. cGgsnThruputIntervalOne set objects cGgsnThruputIntervalTwo, except (0) means disabled.
PATH=/ciscoview/Routershare/config/ggsn_system_info.htm TITLE=GGSN System Information (contd.) TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following: appears: (cGgsnMemoryThreshold) Memory (cGgsnServiceMode) (cGgsnServiceModeStatus) (cGgsnSessionTimeout) (cGgsnRadAttrSessTimeout) Value Throughput (cGgsnThruputIntervalOne) ONE TWO (cGgsnThruputIntervalTwo) (cGgsnCompliance3GppGgsn) Level (cGgsnCreateReqV1UpdExistPdp) Existing (cGgsnPdpNotifEnabled) has Update Turn Attribute 27, (cGgsnDownlinkVerifyMsDisable) Verify-MS Downlink Status (cGgsnGlobalErrorNotifEnabled) Error Notification (cGgsnAccessPointNotifEnabled) cGgsnAccessPointNameNotif cGgsnPacketDataProtocolNotif Data Protocol (GTP) SLB, (cGgsnSlbMode) CAC cacFailure (cGgsnSlbNotif) overload protection mechanism used prevent completely running of when near its capacity some taken place (for example, charging gateway down). This was into that triggers would below ignored, PDP created. requests rejected, result deletion contexts, available drops set object. supports General Radio (GPRS) service modes: inService Indicates nominal operation; there will changes operates. maintenance Restrictions are imposed configurations allowed by GGSN, new accepted. useful you want make without affecting contexts. Specifies timeout value. terminated after interval. specified passed. irrelevant true number notification. been received AAA server. Both specify which needs collected APN/SGSN. valid value, collection begins through configured PATH updated periodically corresponding objects (cGgsnSgsnStatTable cgprsAccPtThruputStatsTable APN). zero, scheduled stopped related deleted. tables. Note: identical cGgsnThruputIntervalOne. purpose provide option second different timer disabled. compliance version. cGgsnVersion. can backward previous possible values: default considered. release40 If currently release50 enabled, compatibility brought about implementation CR 311 (Release 5). these account handling Context already active. Enables sessionDeletion feature global (router) using cgprsAccPtAbsoluteSessionTimer, defined CISCO-GPRS-ACC-PT-MIB. also parses assignment/RADIUS present access-accept request. IP packets outside mobile station (MS), process switching CEF path. works only static added nodes MS. limitations: Since must MS, scalable. It address. dealing Tunneling v1, Traffic Flow Templates (TFTs) order direction. devices done within scope network. does hosts MWAM Cisco Catalyst 6500/7600 environment, should particular reachable. GGSN's internal mode. four outOfServiceInProgress handled cGgsnServiceMode. whether generated device. to: sending false Prevents dispatched Forwards changing destination (vserver) address) response comes same directed VT. behavior SLB. (1) required (2) message last associated IMSI
PATH=/ciscoview/Routershare/config/GGSN_System_Information.htm TITLE=GGSN System Information TEXT=The GGSN System Information category in the GGSN Chassis Configuration dialog box displays GGSN trap and history information. Note: This visible when cGtpGSNService set 'ggsn'. does notification. appears. 'undefined' 'gtpdirector'. Navigation Right-click device, select Configure Device from list. following appears: Current (GPRS Image (cGgsnVersion) cGgsnNotification (cGgsnNotifEnabled) (cGgsnNotifLeastSeverLevel) Severity Level Entries Retained cGgsnHistNotifTable. (cGgsnHistNotifMaxLength) (cGgsnHistNotifLatestIndex) of Recent Entry (cGgsnDefaultIpAllocationMethod) Used Obtain Address Waiting (cGgsnIdlePdpPurgeTimer) Before Purging AAA Authentication (cGgsnDefaultAaaAuthServerGroup) (cGgsnDefaultAaaAccServerGroup) Accounting PPP (cGgsnPppVirtualTemplate) (cGgsnPppRegenVirtualTemplate) Interfaces APNs GTP (cGgsnGtpEncapInterface) (cGgsnConfigVersion) (cGgsnPrepaidPDPs) (cGgsnPostpaidPDPs) Postpaid (cGgsnServiceNotifEnabled) (cGgsnMemoryNotifEnabled) PDF (cGgsnPdfNotifEnabled) release_1_4 number running GGSN. cannot be: Code Details (1) (2). release_3_0 release_4_0 Indicates whether sent generates Value Object Description true sends logs false out However, logged least which notifications. Notifications cleared generated alarms with less than object. You indeterminate maximum table full, oldest removed make space new entries. cGgsnHistNotifIndex most recently created default methods by obtains leases mobile user sessions. disabled. Dynamic dhcp server locate address. radius (3) Time, hours, that waits idle contexts. zero purge timer group all virtual template interface Type PDPs. Regeneration configured. specified. encapsulation. Only one version image, Version.Release.Maintenence, provides ability devices support operations. prepaid since last clearance statistics). service aware cGgsnInServiceNotif cGgsnMaintenanceNotif will device. to: Enables Prevents sending cGgsnMemThresholdReachedNotif cGgsnMemThresholdClearedNotif cGgsnPdfStateUpNotif cGgsnPdfStateDownNotif
PATH=/ciscoview/Routershare/config/ggsn_traffic_class_bw_alloc_table.htm TITLE=GGSN Traffic Class BW Allocation Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select GGSN CAC Virtual (cggsnQosBWPoolTrafClass) from Category drop-down box. With entry selected following dialog box, Details information appears: % of Allocated (cggsnQosBWPoolTrafClassPerVal) Absolute Value (cggsnQosBWPoolTrafClassAbsVal) Available Unused (cggsnQosBWPoolTrafClassAvailBw) Indicates which bandwidth This needed. There are four possible values: conversational streaming interactive background Percentage to set cggsnQosBWPoolTrafClass. object valid can be only when cggsnQosBWPoolTrafClassPercent true false left
PATH=/ciscoview/Routershare/config/ggsn_virtual_server_table.htm TITLE=GGSN Virtual Server Table TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cGgsnSlbVserAddress) (cGgsnSlbVserAddrType) (cGgsnSlbVserNextHopAddrType) (cGgsnSlbVserNextHopAddress) VRF (cGgsnSlbVserVrfName) (cGgsnSlbVserRowStatus) Status address type of vserver. Only IPv4 supported. GTP vservers; required directed mode. If SLB running this object notification configured, then feature remains disabled. dispatched mode, that forwarded create request known to thus it possible send directly reach name -- interface connected Creates new row. deletes existing
PATH=/ciscoview/Routershare/config/home_agent_mobile_network_grp_configs.htm TITLE=Home Agent Mobile Network Group Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: MR Address (cmiHaMrAddrType) Inet (cmiHaMrAddr) (cmiHaMrDynamic) Registration Create/Delete Row (cmiHaMrStatus) type of IPv4 stored cmiHaMrAddr. Only supported. TheIP router providing mobility one more networks. addresses are Specifies whether capable registering dynamically not. status entry.
PATH=/ciscoview/Routershare/config/home_agent_reg_grp_mobile_binding_configs.htm TITLE=Home Agent Registration Group - Mobile Binding Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: MN (cmiHaRegMnIdentifierType) (cmiHaRegMnIfPathMetricType) Associated (cmiHaRegMnIdentifier) (cmiHaRegMobilityBindingRegFlags) Access (cmiHaRegMnIfDescription) (cmiHaRegMnIfBandwidth) Roaming Interface (cmiHaRegMnIfID) Multiple Path Metric type of node's identifier. with node. flags sent by registering router. bandwidth through which registered. unique number identifying This also used as tunnel to Specifies when enabled.
PATH=/ciscoview/Routershare/config/home_agent_reg_process_configs.htm TITLE=Home Agent Registration Processing Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cmiHaRegDateMaxRegsProcLoc) Processed by (cmiHaRegDateMaxRegsProcByAAA) Average (cmiHaRegAvgTimeRegsProcByAAA) Maximum (cmiHaRegMaxTimeRegsProcByAAA) time which number of requests minute reached maximum. Includes only. those that were authenticated locally agent. server. taken to process request. Calculated based It considers
PATH=/ciscoview/Routershare/config/home_agent_reg_req_configs.htm TITLE=Home Agent Registration Request Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: MN Identifier (cmiHaRegMnIdType) Mobile Node Associated (cmiHaRegMnId) (cmiHaRegOverallServTime) Service (cmiHaRegRecentServAcceptedTime) (cmiHaRegRecentServDeniedTime) Acceptance Deny Requests Reason (cmiHaRegRecentServDeniedCode) type of node's identifier. with node. overall time that has accumulated since last rebooted. which most recent was accepted by this denied code indicating rejected agent.
PATH=/ciscoview/Routershare/config/info_mobile_networks_associated_with_HA.htm TITLE=Information of Mobile Networks Associated with HA TEXT=Information of Mobile Networks Associated with Home Agent Navigation Right-click the device, and select Configure appears. Device Configuration dialog box from Category list. following appears: (cmiHaMobNetAddressType) Type IPv4 (cmiHaMobNetAddress) Prefix Length (cmiHaMobNetPfxLen) (cmiHaMobNetDynamic) Registration (cmiHaMobNetStatus) Create/Delete Row addresses stored cmiHaMobNetAddress. Only supported. TheIP network. are address. Indicates whether has been registered dynamically not. status entry.
PATH=/ciscoview/Routershare/config/ip_pool_config.htm TITLE=IP Pool Config TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cIpLocalPoolName) (cIpLocalPoolAddressLo) (cIpLocalPoolAddrType) First Last (cIpLocalPoolAddressHi) Containment (cIpLocalPoolGroupContainedIn) (cIpLocalPoolRowStatus) An arbitrary non-empty string that uniquely identifies local pool. This named must belong among all pools even when they to different groups. Specifies addresses type of cIpLocalPoolAddressHi. range contained by entry. object described cIpLocalPoolAddrType. mapped, If only single being value equal cIpLocalPoolAddressLo. Relates its group. null indicates not group, but base can one Facilitates creation deletion conceptual row table.
PATH=/ciscoview/Routershare/config/ip_pool_containment.htm TITLE=IP Pool Containment TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cIpLocalPoolGroupName) (cIpLocalPoolChildIndex) Index A unique group. name that identifies null string represents base value of cIpLocalPoolName contained local pool.
PATH=/ciscoview/Routershare/config/ip_pool_group_config.htm TITLE=IP Pool Group Config TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cIpLocalPoolGroupName) A unique name that identifies group. null string represents base
PATH=/ciscoview/Routershare/config/mobile_ip_security_violation_configs.htm TITLE=Mobile IP Security Violation Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Violator's (cmiSecViolatorIdentifierType) Type (cmiSecViolatorIdentifier) (cmiSecRecentViolationSPI) SPI (cmiSecRecentViolationTime) Lower Order Identification Bits (cmiSecRecentViolationIDLow) Higher (cmiSecRecentViolationIDHigh) (cmiSecRecentViolationReason) offending identifier. violator not necessary cmiSecAssocTable. most recent this peer. If due to: An mismatch, Authentication Mobile-Home Extension. invalid authenticator, In all other cases, should be set zero. time Low-order 32 used request reply High-order reason
PATH=/ciscoview/Routershare/config/mobile_network_configs.htm TITLE=Mobile Network Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Interfaces (cmiMrMobNetIfIndex) Inet Address (cmiMrMobNetAddr) Prefix Length Associated (cmiMrMobNetPfxLen) (cmiMrMobNetAddrType) Create/Delete Row (cmiMrMobNetStatus) (cmiMrHaTunnelIfIndex) ifIndex value table of MIB II interface router. connected stored network. TheIP with address. type cmiMrMobNetAddr. status entry. tunnel (to HA)
PATH=/ciscoview/Routershare/config/mobile_node_reg_flag_configs.htm TITLE=Mobile Node Registration Flag Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (mnRegAgentAddress) IP Address (mnRegCOA) (cmiMnRegFlags) Care-of agent. as used destination Request. may be home foreign registration. flags sent byte node. It second message.
PATH=/ciscoview/Routershare/config/mobile_router_configs.htm TITLE=Mobile Router Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cmiMrCollocatedTunnel) Tunnel Indication Indicates whether single dual tunnels will between created home agent, when registers with CCoA.
PATH=/ciscoview/Routershare/config/mobile_router_discovery_configs.htm TITLE=Mobile Router Discovery Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: MAC (cmiMrMaAddressType) Type HA (cmiMrMaAddress) (cmiMrMaIsHa) Home foreignAgent Interfaces ifIndex (cmiMrMaAdvRcvIf) Advertising (cmiMrMaIfMacAddress) (cmiMrMaAdvSequence) No Advertisement (cmiMrMaAdvFlags) Longest Registration (cmiMrMaAdvMaxRegLifetime) (cmiMrMaAdvTimeReceived) offers Validity (cmiMrMaAdvMaxLifetime) Received (cmiMrMaAdvTimeFirstHeard) IPv4 addresses stored cmiMrMaAddress. Only supported. which was received. are Indicates whether not. true, one router's configured agents. value table MIB II interface address. sequence number most recently advertisement. ranges 0xffff. After attains 0xffff, rolls 256. contained 7th byte extension mobility advertisement: reverseTunnel supports tunneling gre Generic Routing Encapsulation minEnc Minimal Foreign homeAgent busy regRequired FA required lifetime seconds that willing accept any request. maximum during considered valid absence further advertisements. first
PATH=/ciscoview/Routershare/config/mobile_router_home_agent_address_list.htm TITLE=Mobile Router's Home Agent Address List TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: MN’s (mnHAAddress) (cmiMrHAPriority) (cmiMrHABest) IP of node's agent. priority) this Indicates whether best (in terms time when multiple agents have same not. true router tries to register with first.
PATH=/ciscoview/Routershare/config/mobile_router_interface_configs.htm TITLE=Mobile Router Interface Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cmiMRIfDescription) (cmiMrIfIndex) Access (cmiMrIfCCoaAddressType) Description Waiting Time (cmiMrIfHoldDown) (cmiMrIfRoamPriority) Priority Value (cmiMrIfSolicitPeriodic) Agent Solicitation (cmiMrIfSolicitInterval) (Initial Retransmission) (cmiMrIfSolicitRetransMax) (cmiMrIfSolicitRetransLimit) (cmiMrIfSolicitRetransCurrent) CCoA. (cmiMrIfCCoaAddress) (cmiMrIfCCoaDefaultGwType) Gateway IP (cmiMrIfCCoaDefaultGw) (cmiMrIfCCoaRegistration) (cmiMrIfCCoaRegRetry) Create/Delete Row (cmiMrIfStatus) (cmiMrIfCCoaOnly) (cmiMrIfCCoaEnable) (cmiMrIfRegisteredCoAType) (cmiMrIfRoamStatus) Care-of (cmiMrIfRegisteredCoA) (cmiMrIfRegisteredMaAddrType) Mobility (cmiMrIfRegisteredMaAddr) (cmiMrIfHaTunnelIfIndex) Roaming Identifier (cmiMrIfID) ifIndex Interfaces table. MIB II router. type interface. after which registers stored agents heard. this used among multiple send registrations request. Specifies whether periodically enabled not. When set true. (1), will solicitations according other configured parameters. interval. has before sent advertisements wait first retransmissions maximum limit timeout For each successive message, twice previous number allowed. currently address. cmiMrIfCCoaAddress. collocated Currently, primary cmiMrIfCCoaDefaultGw. with than serial static (fixed) between attempts failure. status that cmiMrIfCCoaRegistrationis: false through foreign agent. registration. Note: under either circumstances: CCoA-only state variable to: directly using even whenever heard, then Enables object Depending cmiMrIfCCoaOnly, might cmiMrIfRegisteredCoA. Indicates registered. by interface: zero Contains home uses cmiMrIfRegisteredMaAddr. registered: tunnel (to agent) unique identifying also
PATH=/ciscoview/Routershare/config/mobile_router_reg_configs.htm TITLE=Mobile Router Registration Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. category from list. following information appears: Time before (cmiMrRegLifetime) Expiration (cmiMrRegExtendExpire) Number of Retries (cmiMrRegExtendRetry) Waiting Reply (cmiMrRegExtendInterval) Requested (cmiMrRegRetransInitial) Retransmissions Maximum (cmiMrRegRetransMax) (cmiMrRegRetransLimit) remaining (milliseconds). to send requests. lifetime expiration. sent. after which another when received. wait retransmitting first time. retransmission allowed.
PATH=/ciscoview/Routershare/config/mobile_router_sys_n_mobile_agent_reg_configs.htm TITLE=Mobile Router System and Mobile Agent Registration Configs TEXT=Navigation Right-click the device, and select Configure. The Device Configuration dialog box appears. from Category list. following information appears: (cmiMrReverseTunnel) Tunneling Status (cmiMrRedundancyGroup) Group Name (cmiMaRegDateMaxRegsReceived) Received Date Advertisement (cmiMnAdvFlags) Specifies whether reverseTunnel enabled not. offers redundancy used to provide network availability router. time which maximum number requests minute were byte mobility agent. contained 7th extension most recently advertisement: gre Generic Routing Encapsulation minEnc Minimal foreignAgent Foreign homeAgent Home busy regRequired FA required supports
PATH=/ciscoview/Routershare/config/mobility_agent_advertisement_configs.htm TITLE=Mobility Agent Advertisement Configurations TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following: information appears: MA (cmiMaAdvInterfaceIndex) TheifIndex (cmiMaInterfaceAddressType) (cmiMaAdvAddressType) TheIP (cmiMaInterfaceAddress) (cmiMaAdvMaxRegLifetime) Registration (cmiMaAdvMaxAdvLifetime) (cmiMaAdvPrefixLengthInclusion) Prefix-Lengths Inclusion (cmiMaAdvAddress) Time (cmiMaAdvMaxInterval) between Advertisements (cmiMaAdvMinInterval) (cmiMaAdvResponseSolicitationOnly) Solicitation Only Row (cmiMaAdvStatus) values Interfaces table. of MIB II thisinterface. that advertising. type address stored cmiMaInterfaceAddress. longest lifetime seconds) will accept any request. Indicates whether should include Extension. If true, all-systems sent over this cmiMaAdvAddress. destination used permissible are: one multicast (224.0.0.1). Default value: router supports limited-broadcast (255.255.255.255). 255.255.255.255. maximum successive transmissions 600 which uses IEEE 802 style headers ATM Zero (0) other cases. minimum 0.75 * cmiMaAdvMaxInterval. (in placed field RFC 1256-portion 3 Flag response message. depends upon zero, set true. then zero. status column 'active', manager not change row. mandatory creating new already exist.
PATH=/ciscoview/Routershare/config/mobility_security_association_configs.htm TITLE=Mobility Security Association Configs TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cmiSecPeerIdentifierType) Entity's (cmiSecPeerIdentifier) (cmiSecAlgorithmType) SA (cmiSecSPI) (cmiSecAlgorithmMode) Mode Replay-Protection (cmiSecReplayMethod) Shared Secret (cmiSecKey2) Create/Delete Row (cmiSecStatus) type of peer. identifier. entity within which this node shares association. 4-byte index that selects specific parameters -- rest variables cmiSecAssocEntry authenticator be used authenticate authentication algorithm: other (1) Any not specified here. md5 (2) message-digest algorithm. hmacMD5 (3) HMAC prefixSuffix In mode, data value. needs calculated preceded followed 128-bit key. method. supported association: timestamps Timestamp-based nonces Nonce-based associations. Reading object will always return zero length. If given hex, should 16 bytes ASCII, can vary characters. status table.
PATH=/ciscoview/Routershare/config/new_ip_pool_config.htm TITLE=New IP Pool Config TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: High (cIpLocalPoolStatHiWaterUsedAddrs) Low Level Address (cIpLocalPoolStatInUseAddrThldLo) (cIpLocalPoolStatInUseAddrThldHi) Contains water mark of used addresses local since: was created system restarted this object reset whichever occurred last. can only number to zero, by doing so, its value, cIpLocalPoolStatInUseAddrs. Since reduced (for example, deleting one ranges), may greater than sum cIpLocalPoolStatFreeAddrs When falls below threshold ciscoIpLocalPoolInUseAddrNoti notification will rearmed. should never cIpLocalPoolStatInUseAddrThldHi. equal exceeds generated. Once generated, disarmed again until indicated cIpLocalPoolStatInUseAddrThldLo. less
PATH=/ciscoview/Routershare/config/NTP_Filter_Register.htm TITLE=NTP Filter Register TEXT=The NTP Filter Register dialog box displays details of the filter register table. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Protocols from Category list. SelectProtocol button. Configuration appears. and later: Note left frame indexed categories right If displayed, variables which key values, are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: (cntpPeersAssocId) Association ID (cntpFilterIndex) Clock (cntpFilterPeersOffset) Round-trip delay (cntpFilterPeersDelay) (cntpFilterPeersDispersion) Related Topics System Integer greater 0 uniquely identifies peer with local server associated. specified range used size fixed 8. Each entry. reading shift register. Entries added starting 1. wraps back, when reaches new overwrite old effectively deleting relative seconds. network path between them, This can take both positive negative depending precision skew-error accumulation. Maximum Only possible.
PATH=/ciscoview/Routershare/config/NTP_Peer_Clock_Configuration.htm TITLE=NTP Peer Clock Configuration TEXT=The NTP Peer Clock Configuration dialog box displays peer clock configuration details. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure displayed, double-click Protocols from Category list. SelectProtocol Details button. appears. and later: Note left frame indexed categories right table. If variable which key values offset nearest listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: Association ID (cntpPeersAssocId) (cntpPeersLeap) Indicator (cntpPeersStratum) (cntpPeersPrecision) (cntpPeersOffset) relative Local (cntpPeersRootDispersion) Primary Reference (cntpPeersDispersion) Round-trip (cntpPeersRootDelay) (cntpPeersDelay) (cntpPeersUpdateTimeRev1) (cntpPeersRefTime) Message Tx (cntpPeersOrgTime) Rx (cntpPeersReceiveTime) (cntpPeersTransmitTime) Related Topics Filter Register System Integer greater 50-Hz uniquely identifies with server associated. Two-bit code warns impending leap seconds. inserted timescale peer. clock. Signed indicates precision clock, power-frequency two. rounded next larger two; instance, (20 ms), 60-Hz (16.67 would assigned -5 (31.25 while 1000-Hz crystal-controlled -9 (1.95 ms). Estimated host determines this object using clock-filter algorithm. Maximum error seconds, source root synchronization subnet. Only positive zero. possible. over network path between them, fixed-point number indicating total delay when its was last updated. has never been synchronized, peer, latest sent. becomes unreachable time, arrived. sender. most recent received used calculate skew dispersion. represents 32-bit NTPTimestamp.
PATH=/ciscoview/Routershare/config/NTP_Peer_Configuration.htm TITLE=NTP Peer Configuration TEXT=The NTP Peer Configuration dialog box displays configuration details of the peer system. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select (cntpPeersConfigured) list, double-click Protocols from Category list. SelectProtocol button. appears. and later: device, Note left frame indexed categories (rightmost) table. If displayed, variable which key values are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: Association ID (cntpPeersAssocId) IP (cntpPeersPeerAddress) UDP (cntpPeersPeerPort) Number Local (cntpPeersHostAddress) (cntpPeersHostPort) (cntpPeersMode) (cntpPeersEntryStatus) Status Reference (cntpPeersRefId) Reachability (cntpPeersReach) host. Message Tx Interval (cntpPeersTimer) (cntpPeersFilterValidEntries) Register Table Valid Entries polls (cntpPeersPeerPoll) (cntpPeersHostPoll) Related Topics Clock System Integer greater 0 uniquely identifies with server. associated. object. true, indicates was created should not de-associated even becomes unreachable. address peer. When creating new association, set this before making active. supported receives messages. Multi-homing significant using mode unspecified object, defaults symmetricActive(1). be: Value Description operating sends periodic regardless state stratum bits By announces willingness synchronized passive type arrives persists only long level equal host; otherwise, dissolved. However, until least, one. has been sent reply. 3 client host, usually LAN workstation, by, 4 ordinarily upon arrival request, exists order after time server, synchronize, broadcast peers. high-speed medium, peers, them 6 reserved control 7 private used management row, made active(1). identifier Shift determine peer, entering end. considered protocol procedures fill data register. seconds, between transmitted filter Since, optional, implemented.
PATH=/ciscoview/Routershare/config/NTP_System_Configuration.htm TITLE=NTP System Configuration TEXT=The NTP System Configuration dialog box displays the system details. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Protocols from Category list. SelectProtocol Details button. appears. and later: device, Note left frame indexed categories right table. If displayed, variable which key values of nearest listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: (cntpSysLeap) Indicator Local (cntpSysClock) (cntpSysStratum) (cntpSysPrecision) Total Round-Trip (cntpSysRootDelay) (cntpSysRootDispersion) Reference ID (cntpSysRefId) Update (cntpSysRefTime) Server (cntpSysPoll) Interval Current Synchronization Source (cntpSysPeer) Related Topics Filter Register Two-bit code warns impending leap seconds, inserted timescale. clock. Signed integer indicating precision clock, power-frequency 2. rounded next larger 2; example, 50-Hz (20 ms), 60-Hz (16.67 would assigned -5 (31.25 while 1000-Hz crystal-controlled -9 (1.95 ms). fixed-point number indicates delay. delay, relation primary root subnet. Maximum error This object takes only positive greater zero. identifier when was last updated. has never been synchronized, polls other servers its source. contains unique association cntpPeersAssocId peer, acting taken corresponding entry cntpPeersVarTable. there no 0. derived hardware machine. increments intervals depending design used.
PATH=/ciscoview/Routershare/config/OSPF_Address_Range_Configuration.htm TITLE=OSPF Address Range Configuration TEXT=The OSPF Address Range dialog box displays the address range details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Protocols from Category list. SelectProtocol button. appears. and later: device, Note left frame indexed categories right table. If displayed, variable which key values are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: (ospfAreaRangeAreaID) ID Network (ospfAreaRangeNet) Subnet (ospfAreaRangeMask) Entry Validity (ospfAreaRangeStatus) Related Topics General Host Interface Link State Database Neighbor Stub ToS Metrics Nonvirtual Virtual within found. IP indicated by range. mask pertains subnet. Indicates invalidity entry. Setting has effect rendering inoperative. internal (row removal) implementation dependent.
PATH=/ciscoview/Routershare/config/OSPF_Area_Configuration.htm TITLE=OSPF Area Configuration TEXT=The Area Configuration dialog box displays the area configuration details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Protocols from Category list. SelectProtocol button. appears. and later: Note left frame indexed categories right table. If displayed, variable which key values listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: ID (ospfAreaId) Authentication (ospfAuthType) (ospfImportASExtern) AS-external-LSA Support Checksum (ospfAreaLSACksumSum) Related Topics Address Range General Host Interface Link State Database Neighbor Stub ToS Metrics Nonvirtual Virtual 32-bit integer uniquely identifies area. 0.0.0.0 used backbone. types specified Additional may assigned locally per basis. can be: Value Description none 1 simplePassword > reserved specification by IANA importing link-state advertisements. unsigned checksums. taken database. excludes (LS 5) determine there has been change router's database, compare two routers.
PATH=/ciscoview/Routershare/config/OSPF_General_Configuration.htm TITLE=OSPF General Configuration TEXT=The OSPF General Configuration dialog box provides the general configuration details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Protocols from Category list. SelectProtocol button. appears. and later: Note left frame indexed displays categories right table. If displayed, variable which key values area listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: (ospfRouterId) ID Admin. (ospfAreaBdrRtrStatus) (ospfAdminStat) (ospfVersionNumber) No. Area Border (ospfASBdrRtrStatus) AS-external-LSA CheckSum (ospfExternLSACksumSum) Type Service (ospfTOSSupport) Related Topics Address Range Host Interface Link State Database Neighbor Stub ToS Metrics Nonvirtual Virtual 32-bit integer uniquely identifying router's autonomous system. By convention, ensure uniqueness, object defaults one IP addresses. Administrative status router. can be: Value Description enabled process active least disabled all interfaces number protocol 2. Indicates unsigned link-state advertisements. checksums. taken database. excludes (LS 5) used determine there has been change database, compare two routers. supports type-of-service routing.
PATH=/ciscoview/Routershare/config/OSPF_Host_Configuration.htm TITLE=OSPF Host Configuration TEXT=The OSPF Host Configuration dialog box displays the host configuration details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configured device, double-click Protocols from Category list. SelectProtocol button. appears. and later: Note left frame indexed categories right table. If displayed, variable which key values are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: IP (ospfHostIpAddress) (ospfHostTOS) Route (ospfHostMetric) Advertised Entry Validity (ospfHostStatus) Related Topics Range Area General Interface Link State Database Neighbor Stub ToS Metrics Nonvirtual Virtual address host. Type service being configured. advertised. Indicates invalidity entry. Setting has effect rendering inoperative. internal (row removal) implementation dependent.
PATH=/ciscoview/Routershare/config/OSPF_Interface_Configuration.htm TITLE=OSPF Interface Configuration TEXT=The OSPF Interface Configuration dialog box displays the interface configuration details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure displayed, double-click Protocols from Category list. SelectProtocol button. appears. and later: Note left-adjusts frame categories right table. (ospfIfIpAddress) variable which indexed key values area listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: IP (ospfAddressLessIf) without connected (ospfIfAreaId) IDs (ospfIfType) Admin. Status (ospfIfAdminStat) (ospfIfRtrPriority) DR election (ospfIfTransitDelay) Delay link-state Update LSA Retransmission (ospfIfRetransInterval) (ospfIfHelloInterval) Packet Transmission (ospfIfRtrDeadInterval) packets. (ospfIfPollInterval) inactive NBMA (ospfIfState) (ospfIfDesignatedRouter) (ospfIfBackupDesignatedRouter) Backup Authentication (ospfIfAuthKey) Related Topics Range General Host Link Database Neighbor Stub ToS Metrics Nonvirtual Virtual addressed this interface. Used ease occurrances addressless interfaces; object takes 0.0.0.0 addresses, corresponding ifIndex having technologies address. 32-bit integer uniquely identifies connects. backbone. By default, field may intuited ifType. Broadcast LANs, such Ethernet IEEE 802.5, (1), X.25, Relay, similar (2), links definitively pointToPoint (3). Administrative can be: Value Description enabled relationships formed interface, advertised internal routers some disabled external multiaccess networks. It designatedRouter algorithm tie breakers. Estimated number seconds, retransmitting over Interval, between advertisement retransmissions neighbouring belonging also when request Length time, sends must same all attached common network. router's not seen before it's neighbors declare down. should hello interval. Larger sending non-broadcast multi-access neighbor. loopback waiting 4 6 backupDesignatedRouter 7 otherDesignatedRouter router. authorization. type simplePassword, shorter octets, agent zero-fills octets. read, always returns string zero.
PATH=/ciscoview/Routershare/config/OSPF_Link_State_Database.htm TITLE=OSPF Link State Database TEXT=The OSPF Link State Database dialog box gives the link state database information for OSPF. Procedure CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Protocols from Category list. SelectProtocol Details button. Configuration appears. and above: Note left frame displays categories right table. If displayed, variable which indexed key values of are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following appears: LSA Rx (ospfLsdbAreaId) (ospfLsdbLSID) (ospfLsdbType) Originating (ospfLsdbRouterId) (ospfLsdbSequence) (ospfLsdbAge) (ospfLsdbChecksum) Related Topics Address Range General Host Interface Neighbor Stub ToS Metrics Nonvirtual Virtual IP designated router. link-state advertisement. Each type. has separate format. can be: Value Description 1 routerLink networkLink 32-bit summaryLink 4 asSummaryLink asExternalLink identifies piece routing domain being described by This object depends bit numbers uniquely autonomous system. Signed integer used detect old duplicate advertisements. sequence ordered linearly. larger more recent advertisement, seconds. complete contents excepted age field. so advertisement's incremented without updating checksum. same ISO connectionless datagrams; commonly referred Fletcher
PATH=/ciscoview/Routershare/config/OSPF_Neighbor_Configuration.htm TITLE=OSPF Neighbor Configuration TEXT=The OSPF Neighbor Configuration dialog box displays the neighbour configuration details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Protocols from Category list. SelectProtocol button. appears. Standard later: Note left frame indexed categories right table. If displayed, variable which key values area. listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information; appears: IP Addressless (ospfNbrIpAddr) Interface (ospfNbrAddressLessIndex) Router Identifying ID (ospfNbrRtrId) (ospfNbrOptions) (ospfNbrPriority) DR election Algorithm Relationship (ospfNbrState) Related Topics Range Area General Host Link Database Stub ToS Metrics Nonvirtual Virtual address, neighbor. On having this object takes zero. interfaces, corresponding ifIndex Internet MIB. creation, can derived instance. 32-bit integer (represented type IpAddress) uniquely identifies neighboring autonomous system. Bit mask neighbor's options field. 0, set, indicates accepts operates external zero, 1, Service other 0. ignores all except metric. designated algorithm. signifies not eligible become network. router's with be: Value Description down attempt init 4 twoWay exchangeStart 6 7 loading 8 full
PATH=/ciscoview/Routershare/config/OSPF_Stub_Area_Configuration.htm TITLE=OSPF Stub Area Configuration TEXT=The OSPF Stub Area Configuration dialog box displays the stub area configuration details for OSPF. Procedure CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Protocols from Category list. SelectProtocol button. appears. and later: list, Note left frame indexed categories right table. If displayed, variable which key values of listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: (ospfStubAreaID) Type Service (ospfStubTOS) (ospfStubMetric) Value Entry Validity (ospfStubStatus) Related Topics Address Range General Host Interface Link State Database Neighbor ToS Metrics Nonvirtual Virtual 32 bit identifier area. On creation, this can derived instance. associated with metric. applied indicated service. By default, equals least among interfaces other areas. Indicates invalidity entry. Setting has effect rendering inoperative. internal (row removal) implementation dependent.
PATH=/ciscoview/Routershare/config/OSPF_ToS_Metrics_for_Nonvirtual_Interface.htm TITLE=OSPF ToS Metrics for Nonvirtual Interface TEXT=The OSPF ToS Metrics for Nonvirtual Inteface dialog box displays the type of service metrics for a non-virtual interface. Procedure CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Protocols from Category list. SelectProtocol Details button. Configuration appears. and later: Note left frame categories right table. (ospfIfMetricIpAddress) displayed, variable which indexed key values are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: IP Addressless (ospfIfMetricAddressLessIf) being Referenced (ospfIfMetricTOS) (ospfIfMetricMetric) Entry Valid (ospfIfMetricStatus) Related Topics Range Area General Host Link State Database Neighbor Stub Virtual addressed On creation, this can derived instance. Eases instancing interfaces. takes 10^8 with addresses, ifIndex having address. referenced. default / ifSpeed. FFFF means there route via ToS. Indicates invalidity entry. Setting object has effect rendering inoperative. internal (row removal) implementation dependent.
PATH=/ciscoview/Routershare/config/OSPF_Virtual_Neighbor_Configuration.htm TITLE=OSPF Virtual Neighbor Configuration TEXT=The OSPF Virutal Neighbor Configuration dialog box displays the virutal neighbor configuration details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Protocols from Category list. SelectProtocol button. appears. and later: Note left frame indexed categories right table. If displayed, variable which key values area. listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: Transit (ospfVirtNbrArea) Identifier Router Identifying ID (ospfVirtNbrRtrId) Neighbor's IP Address (ospfVirtNbrIpAddr) (ospfVirtNbrOptions) Relationship (ospfVirtNbrState) Related Topics Range General Host Interface Link Database Stub ToS Metrics Nonvirtual Identifies 32-bit integer uniquely neighboring autonomous system. used by neighbor. Bit map corresponding options field. Thus, 1, set, means supports type service routing; zero, other 0 relationship. can be: Value Description down attempt init 4 twoWay exchangeStart 6 7 loading 8 full
PATH=/ciscoview/Routershare/config/OSPF_Virutal_Interface_Configuration.htm TITLE=OSPF Virutal Interface Configuration TEXT=OSPF Virtual Interface Configuration Th OSPF Virtual Interface Configuration dialog box displays the details of Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure displayed, double-click Protocols from Category list. SelectProtocol button. appears. and later: Note left frame indexed categories right table. (ospfVirtIfAreaID) variable which key values area listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane. following information appears: (ospfVirtIfTransitDelay) Area ID Neighbor's Router (ospfVirtIfNeighbor) Delay link-state Update LSA Retransmission (ospfVirtIfRetransInterval) (ospfVirtIfHelloInterval) Packet Transmission (ospfVirtIfRtrDeadInterval) packets. (ospfVirtIfState) Authentication (ospfVirtIfAuthKey) Entry Valid (ospfVirtIfStatus) Related Topics Address Range General Host Link Database Stub ToS Metrics Nonvirtual traverses. By definition, this not 0.0.0.0. neighbor. Estimated number seconds, takes retransmitting over interface. between advertisement retransmissions adjacent belonging also used when description request should well expected round-trip time. Length time, sends must same router's seen before it's neighbors declare down. some interval. can (1) pointToPoint (4). verification. type simplePassword, adjusts zero. fills 8 octets. read, ospfVifAuthKey always returns string Indicates invalidity entry. Setting has effect rendering inoperative. internal (row removal) implementation dependent.
PATH=/ciscoview/Routershare/config/port_config_entityInfo.htm TITLE=Entity Information TEXT=-Port This category gives information on the selected port. Procedure Right-click the port, then select configure from list following appears: (entPhysicalIndex (entPhysicalName) Name Description (entPhysicalDescr) (entPhysicaVendorType) Type of physical entitiy which CPUs, statistics entry maintained. can number), chip, group card. textual entity. might name, such as, console simple component (for example, module depending naming syntax device. If there not local object otherwise applicable, will zero-length string. Identifies manufacturer's An indication vendor-specific hardware registration identifier exists value unknown by agent, 00.
PATH=/ciscoview/Routershare/config/PPPoE.htm TITLE=PPPoE TEXT=The PPPoE dialog provides details of the established PPPoE sessions within the system. Procedure Right-click device, then select following information appears: Active (cPppoeSystemCurrSessions) (cPppoeSystemHighWaterSessions) Water Mark Maximum (cPppoeSystemMaxAllowedSessions) (cPppoeSystemThresholdSessions) Value Related Topics VCL current number this high since was initialized. allowed Default equal to cPppoeSystemMaxAllowedSessions.
PATH=/ciscoview/Routershare/config/PPPoE_VCL_Sessions.htm TITLE=PPPoE_VCL_Sessions TEXT=PPPoE VCL Sessions The PPPoE VCL (Virtual Circuit Link) Sessions dialog box provides details about the established information an interface. Procedure Right-click device, then select row from Info Table, Choose required to view session details. following appears: Active (cPppoeVcCurrSessions) (cPppoeVcHighWaterSessions) Water Mark Maximum (cPppoeVcMaxAllowedSessions) (cPppoeVcThresholdSessions) Value current number of VCL. high allowed threshold Default equal cPppoeVcMaxAllowedSessions.
PATH=/ciscoview/Routershare/config/Protocols.htm TITLE=Protocols TEXT=Use this option when you want to use either BGP4, NTP or OSPF protocol. Procedure Right-click the device. Then select Configure double-click Device Configuration dialog box appears. from Category list. NTP, depending which one wish use. Click Details button. chosen.
PATH=/ciscoview/Routershare/config/psd_config.htm TITLE=PSD Configuration TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: (cPsdClientNotifEnable) Notification Specifies whether agent should generate notifications. defined this MIB module. When set to true enables false disables generating
PATH=/ciscoview/Routershare/config/psd_data_store_auto_retrieval.htm TITLE=PSD Data Store & Auto-retrieval TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Data-Store (cPsdClientDSName) Enable/Disable (CDR) (cPsdClientDSAutoRetrieve) Maximum Retrieval (cPsdClientDSMaxRetrieve) (cPsdClientDSRowStatus) Status name of configured data-store. Indicates whether Call Detail Record functionality enabled. When set true false disabled. Specifies value used auto-retrieve enabled, that is, corresponding instance create row. delete existing
PATH=/ciscoview/Routershare/config/psd_server.htm TITLE=PSD Server TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: Data-Store (cPsdClientDSName) (cPsdClientDSServerAddressTyp) Type (cPsdClientDSServerAddress) Write/Retrievable Service (cPsdClientDSRetrieveOnly) (cPsdClientDSServerRowStatus) Status name of configured data-store. Internet address server. Indicates whether cannot be as write/retrievable. only When set true (the value corresponding instance used writing Call Detail Records (CDRs). false well retrieving them. Creates row deletes existing table.
PATH=/ciscoview/Routershare/config/Real_Server_Info.htm TITLE=Real Server Info TEXT=This dialog box provides information about the real server,such as the IP address of the server, the port connections handled, name farm to which With belongs. Procedure Right-click device, then selected, Configured > (SLB) Statistics load-balancing balancing instance Servers following displayed. (slbRealServerFarmName) (slbRealIpAddress) (slbRealPort) (slbRealState) Reserved (slbRealNumberOfDummyConnections) Maximum (slbRealMaxConnections) (slbRealAdminWeight) Reassigned (slbRealReassign) (slbRealRetryInterval) Time Interval Fails (slbRealFailedConnections) (slbRealFailedClients) (slbRealRowStatus) status server. TCP UDP used if NAT. configured. Zero another using concurrent state. number idle dummy that are but accomplish slow-start. delivers user-configured weight algorithms. values shows new will Higher greater availability accept more work. consecutive unanswered SYNs sent before reassigning between retries while failed after goes When fails, timesout RST received from distinct client addresses management station uses row create delete entry slbRealTable text convention.
PATH=/ciscoview/Routershare/config/Server_Farm_Info.htm TITLE=Server Farm Info TEXT=This dialog box provides details about the server farms, such as the name of the server farm, details algorithm configured bind identification number, and real servers. present farm. Procedure Right-click device, then selected, Configure > (SLB) Statistics With load balancing instance following information displayed: (slbServerFarmName) (slbServerFarmPredictor) (slbServerFarmNat) No. (slbServerFarmNumberOfRealServers) (slbServerFarmBindId) (slbServerFarmRowStatus) Status local entity used by its type network address translation (NAT) identify one more which slbDfpRealWeight applies slbRealOperWeight server. Rows slbServerFarmTable matches slbDfpRealBindId are identified. management station uses row create delete entry textual convention.
PATH=/ciscoview/Routershare/config/service_aware_config.htm TITLE=Service Aware Configuration TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. following information appears: CSG Notification (cGgsnSACsgNotifEnabled) (DCCA) (cGgsnSADccaNotifEnabled) GGSN. Feature (cGgsnSAServiceAware) Vodafone Specific (cGgsnSADccaClci) Indicates whether cGgsnSACsgStateUpNotif cGgsnSACsgStateDownNotif notifications sent when path state between content gateway, quota server, changes UP/DOWN. set to true enables sending notification. false prevents any of these generated by device: cGgsnSADccaEndUsrServDeniedNotif cGgsnSADccaCreditLimReachedNotif cGgsnSADccaUserUnknownNotif cGgsnSADccaRatingFailed cGgsnSADccaAuthRejectedNotif Specifies service-aware features (for example, diameter credit control application). disables GPRS service. GGSN's implementation vodafone-specific; client add attributes request message: clci: non-vodafone-specific. a3Gpp:
PATH=/ciscoview/Routershare/config/SLB_Statistics.htm TITLE=SLB Statistics TEXT=Server Load Balancing (SLB) Statistics Procedure Right-click the device , then select Configure > SLB . dialog box, displays following information: Instance (slbEntity) list specifies buttons this Password well their function: With selected, Farm launch Info box. Real Servers Virtual DFP Agents (32-bit) Bit Monitor monitoring (64-bit) reference number server. Allows multiple SLBs exist same SNMP system.
PATH=/ciscoview/Routershare/config/SRP_Error_Statistics.htm TITLE=SRP Error Statistics TEXT=Use this option to monitor error statistics of an interface side with a specific interval number. Procedure access information: Right-click the port and select from popup menu. dialog box appears. Category displays: information. (srpErrorsIntervalInterfaceSide) (srpErrorsIntervalNumber) containing row between 15 96, which identifies available statistics. means most recent completed minute interval. precedes N-1. Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/config/SRP_Higher_Layer_Errors.htm TITLE=SRP Higher Layer Errors TEXT=Use this option to view higher layer error statistics traffic reception for a particular interval of side interface. Procedure 1. Right-click the and select Configure from popup menu. Port dialog box appears. 2. History Category Click button. displays following information: Discarded Packets (srpErrCntIntHostRxDiscardPkts) (srpErrCntIntHostRxShortPkts) (srpErrCntIntHostRxGiantPkts) Related Topics Physical Number due resource limitations, received medium during 15 minute past 24 hours. being short layer, too big
PATH=/ciscoview/Routershare/config/SRP_Higher_Layer_Interval_Statistics.htm TITLE=SRP Higher Layer Interval Statistics TEXT=Use this option to monitor higher layer interval statistics of a particular interface. Procedure To access information: Right-click the port and select (srpHostIntInterfaceSide) from popup menu. dialog box appears. Category displays: information. Side (srpHostIntNumber) containing row number between 15 96, which identifies available statistics. means most recent completed minute interval. precedes N-1. Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/config/SRP_Interface_Sides.htm TITLE=SRP Interface Sides TEXT=Use this option to view SRP interface information of a prticular side. Procedure Right-click the device and select Configure from popup menu. dialog box displays: (srpMACInterfaceSide) (srpMACNeighborAddress) Neighbor (srpMACSideWrapped) State IPS (srpMACIpsMgmtRequestedMode) {noRequest, Current (srpMACIpsAutoDetectMode) Received (srpMACIpsRemoteMode) (srpMACIpsRemoteType) Acive (srpMACIpsActiveMode) Unwrap Transitions (srpMACIpsWrapCounter) (srpMACIpsLastWrapTimeStamp) (srpMACIpsLastUnWrapTimeStamp) (srpMACClockSourceMode) Source (srpMACTopologyTimer) Timer Indication which row contains information. 48-bit individual address neighbor. Boolean flag that indicates node, wrapped state. mode requested by management local can affect according subset rules describing protocol. variables: value. following manualSwitch, forcedSwitch} automatically detected Components {SignalFail, SignalDegrade, WaitToRestore} indicated messages. It other nodes. ring. specifies belongs non-adjacent case shortPath longPath. changed based combined effect Number System time last unwrap. clock source. Internal internal. used when connecting between two routers discovery dark fiber WDM system. default Line line. Synchronous Optical NETwork (SONET) Digital Hierarchy (SDH) ADM. Shows frequently topology are sent around identify Toplogy always 10 seconds. Related Topics CiscoView Monitoring Window Ports Environment Devices
PATH=/ciscoview/Routershare/config/SRP_MAC_Info.htm TITLE=SRP MAC Info TEXT=Use this option to view generic information of a particular SRP interface. Procedure To access SRP MAC information: Right-click there device and select Configure from popup menu. dialog box displays: (srpMACAddress) (srpPriorityThreshold) Threshold Value Number (srpNodesOnTheRing) (IPS) (srpIpsState) (srpIpsLockedOut) out Wrapped (srpIpsWaitToRestoreTimer) (srpIfTimeElapsed) (srpIfValidIntervals) Interval 48-bit individual address. compared against 2493. bits priority contained each packet. header. greater equal threshold, that placed high transmit transit queue. unless than following Since only two types queues (High Priority) treated classifying either once ring. nodes determines what considered When down 0. Intelligent Protection Switching Components states: Idle means mode ready perform sends messages. both neighboring which include itself. source field {0, SELF, S}. PassThrough participates switch by passing wrapped traffic long path signalling through entered based received within present. request issued locally passThrough. Boolean flag indicating state. true then Swiching disabled does not Indicates length time-of-day seconds, remain state, after cause removed. mechanism prevents oscillations. Default 60 sec. including partial have elapsed beginning current measurement described RFC If, some reason, such adjustment system clock occurs, exceeds maximum agent returns value. previous 15-minute intervals. data. collected. must capable supporting least minimum 4. 32. 96. < > was (re-)started last *15) minutes, cases complete has certain (e.g., where proxy) possible unavailable. case, Related Topics CiscoView Monitoring Window Ports Environment Devices
PATH=/ciscoview/Routershare/config/SRP_Media_Dependent_Statistics.htm TITLE=SRP Media Dependent Statistics TEXT=Use this option to monitor media dependent statistics of an interface side with a specific interval number. Procedure access higher layer information: Right-click the port and select from popup menu. dialog box appears. Category displays: information. (srpRingIntInterfaceSide) (srpRingIntNumber) Indication which row contains between 15 96, identifies intervals set available. identified by most recently completed minute interval, immediately preceding Components N-1. Related Topics CiscoView Window Monitoring Ports Devices Environment
PATH=/ciscoview/Routershare/config/SRP_Overview.htm TITLE=SRP Overview TEXT=The Spatial Reuse Protocol (SRP) was developed by Cisco for use with ring-based media. It derives its name from properties of packet-based handling procedure. underlying technology used Dynamic Transport (DPT) family products. new generation, optimized optical transport. This combines bandwidth-efficient service-rich capabilities IP routing bandwidth-rich, self-healing fiber rings deliver fundamental cost functionality advantages over existing solutions. More Information Packet 7200 Applications OC-12c Interface Processor 7500 Related Topics MAC Configure Source Destination Sides Ring Topology Table Physical Layer Errors Higher Statistics History Media Dependent Unwrap Wrap State Transition
PATH=/ciscoview/Routershare/config/SRP_Physical_Layer_Errors.htm TITLE=SRP Physical Layer Errors TEXT=Use this option to view layer 1 physical medium traffic reception for a particular interval of a particular side interface. Procedure 1. Right-click the and select Configure from popup menu. Port dialog box appears. 2. Statistics History Category Click button. displays following errors, information: TTL Exp. Packets Discard (srpErrCntIntRingRxTtlExpPkts) (srpErrCntIntRingRxShortPkts) (srpErrCntIntRingRxGiantPkts) Aborted (srpErrCntIntRingRxAbortPkts) (srpErrCntIntRingRxCRC) Related Topics Higher Number expired packets, received during 15 minute past 24 hours. short giant with
PATH=/ciscoview/Routershare/config/SRP_Unwrap_to_wrap.htm TITLE=SRP Unwrap to Wrap TEXT=- State Transition Statistics Use this option to view number of transitions from unwrap to wrap state in particular intervals information: side interface. Procedure 1. Right-click the and select Configure popup menu. Port dialog box appears. 2. Media Dependent History Category Click button. displays following Unwrap-Wrap (srpRingIntWrapCounter) last < srpRingIntNumber. > described by
PATH=/ciscoview/Routershare/config/SSG_Excluded_APN_Table.htm TITLE=SSG Excluded APN Table TEXT=The SSG Excluded APN Table category of the Configure dialog box displays details on the service selection gateway (SSG) access point. name (APN). Procedure Right-click device, then double-click device. Select from list. following information appears: (cssgExcludedAPNName) (cssgExcludedAPNRowStatus) Status entry. You can use mandatory add delete conceptual row, table. createAndGo set objects There are no request. To destroy
PATH=/ciscoview/Routershare/config/SSG_Excluded_Domain_Table.htm TITLE=SSG Excluded Domain Table TEXT=The SSG Excluded Domain Table category of the Configure dialog box displays details on the service selection gateway (SSG) domains. Procedure Right-click device, then double-click device. Select from list. following information appears: (cssgExcludedDomainName) (cssgExcludedDomainRowStatus) domain. entry. You can use status mandatory createAndGo delete conceptual rows table. row, set objects There are no request. To destroy
PATH=/ciscoview/Routershare/config/SSG_General_Information.htm TITLE=SSG General Information TEXT=The SSG General Information category of the Configure dialog box displays general information on the service selection gateway (SSG). Procedure Right-click device, (cssgCfgRadiusAuthenPort) double-click device. Select from list. following appears: Time (cssgCfgAutoLogOffInterval) ICMP Ping (cssgCfgAutoLogOffIcmpRetries) Maximum (cssgCfgMaxServicesPerUser) (cssgCfgDefaultNetWorkType) Ip Address Type (cssgCfgDefaultNetWork) Access Request Receipt (cssgCfgRadiusAccountingPort) Accounting Authenticated (cssgCfgTCPRedirGrpForUnAuthUsers) Group Unauthorized (cssgCfgTCPRedirGrpForUnAuthServ) (cssgCfgTcpRedirGrpForSMTP) (cssgCfgTcpRedirGrpForInitialCapt) Captivation Advertising (cssgCfgTcpRedirGrpForAdvCapt) which connectivity host. checked. If not reachable, logs auto-logoff feature enabled. Number attempts made by services allowed per user. stored cssgCfgDefaultNetwork. subnet that users. can without authentication. This where Cisco dashboard subscriber-edge manager resides. receives packets remote dial-in clients. redirects directs unauthenticated traffic. initial captivation.
PATH=/ciscoview/Routershare/config/SSG_Network_and_Server_Group.htm TITLE=SSG Network and Server Group TEXT=The SSG Network and Server Group category of the Configure dialog box displays details on the service selection gateway (SSG) details. Procedure Right-click device, then double-click device. Select & from list. following information appears: Redirect-Group (cssgTcpRedirectGrpName) (cssgTcpRedirNetworkMapGrpName) Rowstatus (cssgTcpRedirNetworkGrpMapRowStat) redirection. group. createAndGo set groups that can be associated with TCP traffic Status table. entry. used mandatory create delete conceptual rows row, objects There are no request. To destroy
PATH=/ciscoview/Routershare/config/SSG_Network_Group.htm TITLE=SSG Network Group TEXT=The SSG Network Group category of the Configure dialog box displays the service selection gateway (SSG) details. Procedure Right-click device, then double-click device. Select from list. following information appears: (cssgNetworkGrpName) Address (cssgNetworkGrpNetIpType) (cssgNetworkGrpNetIpAddr) (cssgNetworkGrpNetMaskType) (cssgNetworkGrpNetMask) (cssgNetworkGrpNetRowStatus) group. group, which networks, associated with servers traffic redirection. Packets stored compared directed Value that represents type IP objects cssgNetworkGrpNetIpAddr. cssgNetworkGrpNetMask. before combined destination table. entry. can used createAndGo delete conceptual rows To row, set There no mandatory request. destroy
PATH=/ciscoview/Routershare/config/SSG_Port_Group.htm TITLE=SSG Port Group TEXT=The SSG Port Group category of the Configure dialog box displays details on the service selection gateway (SSG) group. Procedure Right-click device, then double-click device. Select from list. following information appears: (cssgPortGrpName) Number (cssgPortGrpPortNo) (cssgPortGrpPortRowStatus) defines ports to which TCP redirected. can table. entry. used createAndGo delete conceptual rows row, set object destroy
PATH=/ciscoview/Routershare/config/SSG_Port_Maps.htm TITLE=SSG Port Maps TEXT=The SSG Port Maps category of the Configure dialog box displays details on the service selection gateway (SSG) map. Procedure Right-click device, then double-click device. Select from list. following information appears: Address (cssgPortMapSourceIpType) (cssgPortMapSourceIp) Lower (cssgPortMapPortRangeFrom) Upper (cssgPortMapPortRangeTo) (cssgPortMapRowStatus) Value that represents type cssgPortMapSourceIP stored object. source addresses subscriber used while translating network downstream (traffic SSG). limit range ports table. entry. can createAndGo delete conceptual rows row, set mandatory are objects request. destroy
PATH=/ciscoview/Routershare/config/SSG_Port_Server_Association.htm TITLE=SSG Port Server Association TEXT=The SSG Port Server Association category of the Configure dialog box displays details on the service selection gateway (SSG) association. Procedure Right-click device, then double-click device. Select from list. following information appears: Redirect-Group (cssgTcpRedirectGrpName) Number (cssgTcpRedirPortNo) RowStatus (cssgTcpRedirPortNoMapRowStat) redirect group. associated with table. entry. can used mandatory createAndGo delete conceptual rows row, set object request. To destroy
PATH=/ciscoview/Routershare/config/SSG_Radius_Client_Table.htm TITLE=SSG Radius Client Table TEXT=The SSG Radius Client Table category of the Configure dialog box displays details on the service selection gateway (SSG) remote authentication dial-in user client. Procedure Right-click device, double-click device. Select from list. following information appears: (cssgRadiusClientAddrType) Address (cssgRadiusClientAddr) Rowstatus (cssgRadiusClientRowStatus) stored cssgRadiusClientAddr. Network layer (radius) which acts as radius-proxy. entry. can be used createAndGo delete conceptual rows table. To row, set objects There are no mandatory request. destroy
PATH=/ciscoview/Routershare/config/SSG_Server_and_Port_Group.htm TITLE=SSG Server and Port Group TEXT=The SSG Server and Port Group category of the Configure dialog box displays details on the service selection gateway (SSG) redirect-group. Procedure Right-click device, then double-click device. Select & from list. following information appears: Redirect-Group (cssgTcpRedirectGrpName) (cssgTcpRedirPortMapGrpName) RowStatus (cssgTcpRedirPortGrpMapRowStat) createAndGo set ports that can be associated with TCP traffic redirection. table. entry. used mandatory create delete conceptual rows row, objects There are no request. To destroy
PATH=/ciscoview/Routershare/config/SSG_Service_Bind_Table.htm TITLE=SSG Service Bind Table TEXT=The SSG Service Bind Table category of the Configure dialog box displays details on the service selection gateway (SSG) bind. Procedure Right-click device, then double-click device. Select from list. following information appears: (cssgServiceName) Interface (cssgServiceIfIndex) (cssgServiceIfRowStatus) profile. index mandatory which bound. entry. can be used createAndGo delete conceptual rows table. row, set object request. To destroy
PATH=/ciscoview/Routershare/config/SSG_Service_Route_Table.htm TITLE=SSG Service Route Table TEXT=The SSG Service Route Table category of the Configure dialog box displays details on the service selection gateway (SSG) table. Procedure Right-click device, then double-click device. Select from list. following information appears: (cssgServiceName) (cssgServiceRouteType) Address (cssgServiceRouteAddr) (cssgServiceRouteMaskType) (cssgServiceRouteMask) Action (cssgServiceRoutePermission) profile. Value that represents type stored cssgServiceServRouteAddr. IP networks available you. cssgServiceServRouteMask. before combined with destination compared cssgServiceRouteAddr. taken packets when matches can be: Description 1 permit 2 deny
PATH=/ciscoview/Routershare/config/SSG_Service_Table.htm TITLE=SSG Service Table TEXT=The SSG Service Table category of the Configure dialog box displays details on the service selection gateway (SSG) table. Procedure Right-click device, authentication. double-click device. Select from list. following information appears: (cssgServiceName) (cssgServiceMode) (cssgServiceType) (cssgServiceIdleTimeout) (cssgServiceSessionTimeout) (cssgServiceActiveSessions) Length Active (cssgServiceDNSPrimaryIpType) (cssgServiceDNSPrimary) (cssgServiceDNSSecondaryIpType) (cssgServiceDNSSecondary) (cssgServiceUpstreamQOSEnabled) Status Downstream (cssgServiceDownStreamQOSEnabled) (cssgServiceOpenGarden) Garden (cssgServicePrepaid) profile. An optional attribute that indicates whether (you cannot to another while using service. mode be: Value Description 1 unknown L2TP concurrent 3 sequential service) pass-through: Means user done during logon this default. tunnel: tunneled 4 proxy: performs Amount time, seconds, session idle before without times out. Maximum seconds. Number connections IP address type. primary server secondary upstream policing enabled open accessed pre-paid.
PATH=/ciscoview/Routershare/config/SSG_Status.htm TITLE=SSG Configure Status TEXT=SSG Status The SSG Status category of the Configure dialog box displays details on the service selection gateway (SSG). configuration. Procedure Right-click device, authentication, double-click device. Select from list. following information appears: State (cssgCfgSsgEnabled) (cssgCfgAutoDomainMode) (cssgCfgLocalForwardingEnabled) Forwarding Logoff (cssgCfgAutoLogOffMode) (cssgCfgRadiusProxyEnabled) Proxy TCP (cssgCfgTcpRedirectEnabled) NAT (cssgCfgAutoDomainNatEnabled) PortBundle-Host (cssgCfgPortBundleHostKeyEnabled) Transparent (cssgCfgTransPassThroughEnabled) (cssgCfgAccountingEnabled) (cssgCfgRadiusFwdAcctPktsEnabled) Reboot (cssgCfgRadiusClntRbtNotifEnabled) (cssgCfgAAAServerDownNotifEnabled) TAL(cssgCfgTalEnabled) Indicates whether enabled. auto-domain feature allows username. be: connected automatically based access-point name structured can Value Description 1 disabled 2 basic 3 extended locally forwards packets among subscribers. auto-logoff initiate connectivity bundle-host lost. checked using address resolution protocol. Internet control message (RADIUS) remote dial-in act generic RADIUS-proxy non-service-selection dashboard clients such GPRS node. redirects certain captive portals. network translation available users. determines gets IP assigned by service. key edge manager identify (combination and range ports) pass through unauthenticated traffic routed either direction. accounting generates records send them authorization (AAA) server. received radius notification reboots. goes down An indication Logon SSG.
PATH=/ciscoview/Routershare/config/ssg_tal_info.htm TITLE=SSG TAL Information TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select SSG from Category list. following appears: Max. authorization Requests (cssgTalMaxAuthRate) (cssgTalMaxAuthRateTimestamp) Auth. (cssgTalMinAuthRate) Min. (cssgTalMinAuthRateTimestamp) (cssgTalCurrentAuthRate) Last Recorded (cssgTalCurrentAuthRateTimestamp) (cssgTalResetAuthRates) Athorization (cssgTalMaxPendingAuthReqs) (cssgTalMaxAuthReqsRate) (cssgTalDropPakDuringAuthorization) Packets During (cssgTalUnidentifiedUserAllowTraff) (cssgTalUnidentifiedUserTimeout) (cssgTalMaxSuspectUsers) Traffic (cssgTalSuspectUserTimeout) Timeout Maximum rates of per second. given time, will overwrite previous value. This local when second, indicated by cssgTalMaxAuthRate, was recorded. Minimum cssgTalMinAuthRate, SSG. cssgTalCurrentAuthRate, Setting variable from/to 'reset' indicates that would number 'unknown'. not result any changes. An snmp-get always return outstanding allowed. If goes beyond value, does SYS log message received sending new radius request dropped. CEF path itself. set, applicable point onwards. existing exceeds values, these discarded. throttles sent 'true' are users 'false' unidentified suspect minutes. packet user, dropped/tcp-redirected, until reached. After timeout, trigger again. expiry, done user.
PATH=/ciscoview/Routershare/config/ssg_tal_user_info_table.htm TITLE=SSG TAL User Info Table TEXT=Procedure Right-click the device and then select Configure , or double-click the device. Select SSG from Category list. following information appears: (cssgTalUserIPAddress) Address (cssgTalUserState) This type of particular transparent used as index (together with identify unique entry table. state user.
PATH=/ciscoview/Routershare/config/SSG_TCP_Redirect_Group.htm TITLE=SSG TCP Redirect Group TEXT=The SSG TCP Redirect Group category of the Configure dialog box displays details on the service selection gateway (SSG) group. Procedure Right-click device, then double-click device. Select from list. following information appears: Redirect-Group (cssgTcpRedirectGrpName) (cssgTcpRedirectGrpServerAddrType) Type (cssgTcpRedirectGrpServerAddr) Redirection port (cssgTcpRedirectGrpServerPort) (cssgTcpRedirectGrpRowStatus) Status Value that represents address stored cssgTcpRedirectGrpServerAddr. IP server which traffic be redirected. table. entry. can used createAndGo delete conceptual rows To row, set objects There are no mandatory request. destroy
PATH=/ciscoview/Routershare/config/Traffic_DS_PHB_Group.htm TITLE=Traffic & DS PHB Group TEXT=GGSN Traffic & DS PHB Group Use this dialog to view Universal Mobile Telephone System (UMTS) traffic class mapping within Per Hop Behaviour (PHB) group. Procedure In another Chassis view, right-click device bandwidth, select Configure from popup menu. following information appears: (cggsnQosUmtsTrafficClass) Mapped (cggsnQosUmtsDiffServPhbgroup) PDP (cggsnQosUmtsPdps) QoS class. values. are: signalling(1) conversational(2), streaming(3), interactive(4), background(5) uses parameter make assumptions about source, determines maximum bit rate, guaranteed whenever performing admission control. only applies messages. which given by cggsnQosUmtsTrafficClass. architecture based number offer functional elements, PHB. PHBs specify queuing, queue management scheduling characteristics that provides means allocating resources(buffer resources each node among competing streams. various include: signallingClass(1) used does not apply any IP data packets. expedited forwarding efClass(2) There loss, latency, jitter, assured end-to-end service. through domains. Such endpoints like point-to-point connection, virtual leased line. afClass(3-6) provider different levels delivery assurances received customer domain. four classes, follows: afClass1, afClass2, afClass3 afClass4 defined, where AF allocated certain amount space bandwidth). assigned into more these according subscribed Within marked subscriber, domain, three possible drop precedence case congestion, relative importance Packets forwarded independently bestEffort(7) effort default aggregate output link required satisfy contexts associated identified
PATH=/ciscoview/Routershare/config/Virtual_Client_Info.htm TITLE=Virtual Client Info TEXT=This dialog box provides information about the client IP address, client mask, and the range of IP addresses clients. Procedure Right-click device, then selected, Configure > (SLB) Statistics With server. load balancing instance Servers entry VirClient IPAddress (slbVirtualClientIpAddress) (slbVirtualClientMask) (slbVirtualClientExclude) (slbVirtualClientRowStatus) status client. It used to represent subsets traffic being handled by general purpose particular truth value that determines whether should included excluded management station uses row create delete slbVirtualClientTable following textual convention.
PATH=/ciscoview/Routershare/config/Virtual_Server_Info.htm TITLE=Virtual Server Info TEXT=This dialog box provides information on the virtual server configured on the server load balancing (SLB) manager. IP address, port, outstanding associated farm name. Procdure Right-click device, then selected, Configure > Statistics With instance Servers following displayed. (slbVirtualServerName) (slbVirtualServerState) (slbVirtualIndex) (slbVirtualIpAddress) (slbVirtualPort) (slbVirtualProtocol) (slbVirtualService) (slbVirtualAdvertise) (slbVirtualFarmName) (slbVirtualDelayTimer) time (slbVirtualIdleTimer) (slbVirtualStickyTimer) (slbVirtualStickyGroup) ID Unanswered SYNs. count (slbVirtualSynguardCount) (slbVirtualSynguardPeriod) of Syngaurd (slbVirtualRowStatus) status Subnet mask (slbVirtualMask) server. state index assigned used correlate connections servers. protocol service setting values other than none result association being formed between clients using Subsequent packets from needing will forwarded nominated real advertising. It true if has added static route routing table attracting traffic destined slbVirtualIpAddress. bound amount entity maintains TCP context after been terminated. absence activity. remembered group sticky placed in. zero shows that number allowed reached, are dropped depending slbVirtualSynguardPeriod. interval which can have limit management station uses row create delete entry slbVirtualServerTable. applied filtering.
PATH=/ciscoview/Routershare/config/VPDN_Failure_Hist.htm TITLE=VPDN Failure History TEXT=Use this option to view failure records that are referenced with a user name. Procedure To access VPDN History: Right-click otherwise device and select Configure from popup menu. dialog box appears. Category displays: (cvpdnUnameToFailHistLocalName) (cvpdnUnameToFailHistUname) (cvpdnUnameToFailHistTunnelId) (cvpdnUnameToFailHistUserId) (cvpdnUnameToFailHistLocalInitConn) Initiated Connection (cvpdnUnameToFailHistRemoteName) (cvpdnUnameToFailHistSourceIp) IP Address Destination (cvpdnUnameToFailHistDestIp) (cvpdnUnameToFailHistCount) (cvpdnUnameToFailHistFailTime) (cvpdnUnameToFailHistFailType) (cvpdnUnameToFailHistFailReason) Note You can system information, tunnels session only Specifies active available. Related Topics Information Sessions user-name entry. ID; instigator, HGW/LNS NAS/LAC ID. The of Indicates whether which occurred. was generated locally. It router. served home gateway. configured host-name object empty before successful projection; thus, no source will remote serves interface end tunnel. receiver incremented when multiple failures have delta > 1 current latest series been recorded. time type record. An ASCII string describes reason
PATH=/ciscoview/Routershare/config/VPDN_Overview.htm TITLE=VPDN Overview TEXT=Virtual Private Dialup Network (VPDN) allows the private networks to span from the client directly to Home Gateway. of choice. Forwarding example, mobile users HP (such base. sales personnel) want numbers, able always connectivity anywhere, anytime. would contract Internet Service Providers (ISPs) that support VPDN. These configured if jsmith@hp.com dials into ISP-provided (NAS) automatically forward administering freed IP addresses, routing, Understanding other functions tied administration reduced issues terminology, Point (PPP) link between (jsmith) propagation Access Server brought about maintained by Link-Level Layer (L2F). More Information Introduction Technologies Resouce Pool Management Tunnels Protocol Group, Reorganization L2TP Switching Per-User Configuration Limiting Tracking Sessions User, Dialout Related Topics System Failure History
PATH=/ciscoview/Routershare/config/VPDN_Sessions.htm TITLE=VPDN Sessions TEXT=Use this option to view VPDN session information. Procedure To access VPDN session information: Right-click the devices and select Configure from popup menu. dialog box appears. Category displays: (cvpdnSystemTunnelType) (cvpdnSessionAttrDeviceType) (cvpdnTunnelAttrTunnelId) (cvpdnSessionAttrSessionId) (cvpdnSessionAttrUserName) Name (cvpdnSessionAttrState) (cvpdnSessionAttrCallDuration) Duration (cvpdnSessionAttrDeviceCallerId) Physical (cvpdnSessionAttrDevicePhyId) (cvpdnSessionAttrMultilink) (cvpdnSessionAttrModemSlotIndex) (cvpdnSessionAttrDS1SlotIndex) (cvpdnSessionAttrModemPortIndex) (cvpdnSessionAttrDS1PortIndex) (cvpdnSessionAttrDS1ChannelIndex) Channel (cvpdnSessionAttrModemCallStartTime) Time (cvpdnSessionAttrModemCallStartIndex) (cvpdnSessionAttrPacketsOut) (cvpdnSessionAttrBytesOut) (cvpdnSessionAttrBytesIn) (cvpdnSessionAttrPacketsIn) Note You can system information, tunnels only Specifies active. are available. Related Topics Information Failure History ID of session. user Current states L2F have with prefix. L2TP code each explained below: unknown. indicates l2fOpening has just been initiated through waiting remote end reply complete process. l2fCloseWait closed l2fWaitingForTunnel still state. It waits OPEN before allowed fully established. l2tpIdle that yet. l2tpWaitingTunnel l2tpWaitReply l2tpWaitConnect acknowledged connection request connect. l2tpEstablished l2tpShuttingDown shutting down. call. Number output packets sent bytes input received types attached local tunnel. meaning otherwise, any not defined. 'asyncInternalModem' modem. pool server. regular asynchronous serial interface. bchan ISDN xdsl cable Identification incoming caller. empty because provide index points ifTable. virtual interfaces ifTable, value zero. Link whether part multilink PPP, bundle, even there one bundle. If true. database slot associated will valid object; instantiated. port over start Arbitrary small integer distinguishes calls occurred same tick.
PATH=/ciscoview/Routershare/config/VPDN_System_Info.htm TITLE=VPDN System Information TEXT=Use this option to view VPDN system information. Procedure To access VPDN system information: Right-click the device and select Configure from popup menu. dialog box appears. Category displays: (cvpdnSystemTunnelType) Type (cvpdnSystemTunnelTotal) Sessions (cvpdnSystemSessionTotal) (cvpdnSystemDeniedUsersTotal) Users Note You can information, tunnels. session only if active are available. Related Topics Failure History protocol. Number of all denied user attempts since last time re-initialized.
PATH=/ciscoview/Routershare/config/VPDN_Tunnel_Attri.htm TITLE=VPDN Tunnel Attributes TEXT=VPDN Tunnels Use this option to view VPDN tunnel information. Procedure To access VPDN tunnels information: Right-click Otherwise device and select Configure from popup menu. dialog box appears. Category displays: (cvpdnSystemTunnelType) (cvpdnTunnelAttrTunnelId) (cvpdnTunnelAttrRemoteTunnelId) (cvpdnTunnelAttrLocalName) (cvpdnTunnelAttrRemoteName) (cvpdnTunnelAttrRemoteEndpointName) Initiated (cvpdnTunnelAttrLocalInitConnection) Originated (cvpdnTunnelAttrOrigCause) (cvpdnTunnelAttrState) (cvpdnTunnelAttrActiveSessions) Sessions (cvpdnTunnelAttrDeniedUsers) Users (cvpdnTunnelAttrSoftshut) l2tpShuttingDown (cvpdnTunnelAttrNetworkServiceType) Service IP (cvpdnTunnelAttrLocalIpAddress) (cvpdnTunnelAttrSourceIpAddress) (cvpdnTunnelAttrRemoteIpAddress) Note You can system information, session only different active. are available. Related Topics Information Failure History ID. tunnel. end-point instigator, HGW/LNS NAS/LAC, Two distinct with same may exist, types. The remote If tunnel, ID, locally. name, It router. serves was home gateway. Typically, configured host either domain DNIS, Indicates whether value true, cause that projected via stack group. current states 'l2f' have prefix. 'l2tp' codes explained below: unknown. l2fOpening has just been waiting reply complete process. l2fOpenWait received tunnel-open request. established. l2fClosing tunnel-close l2fCloseWait down. l2tpIdle yet. l2tpWaitCtlReply l2tpEstablished shutting l2tpNoSessionLeft there left number denied Prevents any new being added object specifies soft shut. network used address. interface source user configurable binding protocol.
