# Service Aware Configuration

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.
2. Select Service Aware Configuration from the Category list.

The following information appears:

> CSG Notification (cGgsnSACsgNotifEnabled)

> DCCA Notification (cGgsnSADccaNotifEnabled)

> GGSN Service Aware Feature (cGgsnSAServiceAware)

> Vodafone Specific (cGgsnSADccaClci)

### CSG Notification (cGgsnSACsgNotifEnabled)

Indicates whether cGgsnSACsgStateUpNotif and cGgsnSACsgStateDownNotif notifications are sent when the path state between the content service gateway and the quota server changes between UP/DOWN. When set to true, enables the device to send a notification. When set to false, prevents the device from sending a notification.

### DCCA Notification (cGgsnSADccaNotifEnabled)

Indicates whether any of these notifications are sent when a notification is generated by the device:

- cGgsnSADccaEndUsrServDeniedNotif
- cGgsnSADccaCreditLimReachedNotif
- cGgsnSADccaUserUnknownNotif
- cGgsnSADccaRatingFailed
- cGgsnSADccaAuthRejectedNotif

When set to true, enables the device to send a notification. When set to false, prevents the device from sending a notification.

### GGSN Service Aware Feature (cGgsnSAServiceAware)

Specifies the service-aware feature on GGSN. When set to true, enables service-aware features (for example, quota server, content service gateway, diameter credit control application). When set to false, disables the GGSN service from the GPRS service.

### Vodafone Specific (cGgsnSADccaClci)

Indicates whether GGSN's diameter credit control application (DCCA) implementation is vodafone-specific; enables the GPRS client to add vodafone-specific attributes to the request message:

- clci: DCCA implementation is vodafone-specific.
- a3Gpp: DCCA implementation is non-vodafone-specific.