# Transmit Side High Priority Traffic Statistics

Use this option to monitor statistics of high priority traffic reception to higher layer for current interval for a particular side of a particular SRP interface.

## Procedure

To access high priority traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Current Interval Statistics of Higher Layer dialog box appears.

2. Select Tx Higher Layer Statistics from the Category menu to display Transmit Side Higher Layer Statistics dialog box.

3. Select High Priority Traffic from the Category menu to display high priority traffic information.

High Priority Traffic dialog box displays:

Unicast High Priority Packets (srpHostCurUcastHighPriPktsOut)

Unicast High Priority Octets (srpHostCurUcastHighPriOctetsOut)

Multicast High Priority Packets (srpHostCurMcastHighPriPktsOut)

Multicast High Priority Octets (srpHostCurMcastHighPriOctetsOut)

### Unicast High Priority Packets (srpHostCurUcastHighPriPktsOut)

Number of high priority unicast packets going to the higher layer during a 15-minute interval.

### Unicast High Priority Octets (srpHostCurUcastHighPriOctetsOut)

Number of high priority unicast octets going to the higher layer during a 15-minute interval.

### Multicast High Priority Packets (srpHostCurMcastHighPriPktsOut)

Number of high priority multicast packets going to the higher layer during a 15-minute interval.

### Multicast High Priority Octets (srpHostCurMcastHighPriOctetsOut)

Number of high priority multicast octets going to the higher layer during a 15-minute interval.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components