# CDMA PDSN PCF and Service Option based RP Session Update Statistics

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Configure button.
4. Select category CDMA PDSN PCF and Service Option based RP Session Update.
5. Select a row.

> Note: Clicking the Monitor1 button displays information for CDMA PDSN PCF and Service Option based RP Session Update Statistics. Clicking the Monitor 2 button displays information for CDMA PDSN PCF and Service Option based RP Session Update Statistics Contd.

1. Click the Monitor1 button.

The following information appears:

> A11 Sessions Transmitted (cCdmaPcfSoRpSessUpdTxdReqs)

> A11 Sessions Acknowledged (cCdmaPcfSoRpSessUpdAcptdReqs)

> A11 Sessions Denied (cCdmaPcfSoRpSessUpdDeniedReqs)

> A11 Registration Acknowledgements (cCdmaPcfSoRpSessUpdNotAckedReqs)

> Initial A11 Session Updates (cCdmaPcfSoRpSessUpdInitTxdReqs)

> Re-transmitted A11 Session Updates (cCdmaPcfSoRpSessUpdReTxdReqs)

> Session Ack Since Restart (cCdmaPcfSoRpSessUpdRcvdAcks)

> Session Updates Discarded (cCdmaPcfSoRpSessUpdDiscardedAcks)

### A11 Sessions Transmitted (cCdmaPcfSoRpSessUpdTxdReqs)

Total number of A11 session updates transmitted since the system was last restarted.

### A11 Sessions Acknowledged (cCdmaPcfSoRpSessUpdAcptdReqs)

Total number of A11 session update acknowledgements received with the Status field set to zero (indicating that the corresponding registration update was accepted) since the system was last restarted.

### A11 Sessions Denied (cCdmaPcfSoRpSessUpdDeniedReqs)

Total number of A11 session update acknowledgements received with the Status field set to non-zero indicating that the corresponding registration update was denied since the system was last restarted.

### A11 Registration Acknowledgements (cCdmaPcfSoRpSessUpdNotAckedReqs)

Total number of A11 session updates sent, for which no corresponding A11 registration acknowledgements were received since the system was last restarted.

### Initial A11 Session Updates (cCdmaPcfSoRpSessUpdInitTxdReqs)

Total number of initial A11 session updates sent, excluding the re-transmitted A11 registration updates, since the system was last restarted.

### Re-transmitted A11 Session Updates (cCdmaPcfSoRpSessUpdReTxdReqs)

Total number of re-transmitted A11 session updates since the system was last restarted.

### Session Ack Since Restart (cCdmaPcfSoRpSessUpdRcvdAcks)

Total number of A11 session acknowledgements received since the system was last restarted.

### Session Updates Discarded (cCdmaPcfSoRpSessUpdDiscardedAcks)

Total number of A11 session update acknowledgements discarded since the system was last restarted.